Functions | Variables

# usb_device_task.h File Reference

This file contains the function declarations for USB device task. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Functions
void | usb_device_task_init (void)
| This function initializes the USB device controller.
void | usb_start_device (void)
| This function initializes the USB device controller.
void | usb_device_task (void)
| Entry point of the USB device mamagement.
## Variables
bit | usb_suspended
| Public : (bit) usb_suspended usb_suspended is set to TRUE when USB is in suspend mode usb_suspended is set to FALSE otherwise /.
bit | usb_connected
| Public : (bit) usb_connected usb_connected is set to TRUE when VBUS has been detected usb_connected is set to FALSE otherwise /.

## Detailed Description

This file contains the function declarations for USB device task.

- Compiler: IAR EWAVR and GNU GCC for AVR
- Supported devices: ATmega32U4

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file usb_device_task.h.