Defines

# ADC High Speed Mode Configuration
[ADC Macros]

Set the high spped mode in case ADC frequency is higher than 200KHz. More...

## Defines
#define | Enable_adc_high_speed_mode() (ADCSRB |= (1<<ADHSM))
#define | Disable_adc_high_speed_mode() (ADCSRB &= ~(1<<ADHSM))

## Detailed Description

Set the high spped mode in case ADC frequency is higher than 200KHz.

## Define Documentation

#define Enable_adc_high_speed_mode | ( | ) | (ADCSRB |= (1<<ADHSM))

Definition at line 85 of file adc_drv.h.

Referenced by ADC_Init(), and init_adc().

#define Disable_adc_high_speed_mode | ( | ) | (ADCSRB &= ~(1<<ADHSM))

Definition at line 86 of file adc_drv.h.

Referenced by init_adc().