Functions | Variables

# usb_device_task.c File Reference

This file manages the USB device controller. More...

`#include "config.h"`
`#include "conf_usb.h"`
`#include "usb_device_task.h"`
`#include "modules/usb/usb_task.h"`
`#include "lib_mcu/usb/usb_drv.h"`
`#include "usb_descriptors.h"`
`#include "modules/usb/device_chap9/usb_standard_request.h"`
`#include "lib_mcu/pll/pll_drv.h"`
Include dependency graph for usb_device_task.c:

Go to the source code of this file.

## Functions
void | usb_device_task_init (void)
| This function initializes the USB device controller and system interrupt.
void | usb_start_device (void)
| This function initializes the USB device controller.
void | usb_device_task (void)
| Entry point of the USB device mamagement.
## Variables
bit | usb_connected = (0==1)
| Public : (bit) usb_connected usb_connected is set to TRUE when VBUS has been detected usb_connected is set to FALSE otherwise /.
bit | usb_suspended = (0==1)
| Public : (bit) usb_suspended usb_suspended is set to TRUE when USB is in suspend mode usb_suspended is set to FALSE otherwise /.
U8 | usb_configuration_nb
| Public : (U8) usb_configuration_nb Store the number of the USB configuration used by the USB device when its value is different from zero, it means the device mode is enumerated Used with USB_DEVICE_FEATURE == ENABLED only /.

## Detailed Description

This file manages the USB device controller.

The USB task checks the income of new requests from the USB Host. When a Setup request occurs, this task will launch the processing of this setup contained in the usb_standard_request.c file. Other class specific requests are also processed in this file.

- Compiler: IAR EWAVR and GNU GCC for AVR
- Supported devices: ATmega32U4

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file usb_device_task.c.

## Variable Documentation

U8 usb_configuration_nb

Public : (U8) usb_configuration_nb Store the number of the USB configuration used by the USB device when its value is different from zero, it means the device mode is enumerated Used with USB_DEVICE_FEATURE == ENABLED only /.

Definition at line 100 of file usb_standard_request.c.

Referenced by usb_device_task(), usb_get_configuration(), and usb_set_configuration().