# board/atevk1104/include/board/led.h File Reference

Board-specific LED control. More...

`#include <chip/portmux.h>`

Include dependency graph for led.h:

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Enumerations
enum | board_led_id
| Connection of on-board LEDs. More...
## Functions
static void | led_activate (enum board_led_id id)
| Turn LED id on.
static void | led_deactivate (enum board_led_id id)
| Turn LED id off.

## Detailed Description

Board-specific LED control.

Please don't include this file directly. Use <led.h> instead.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: All devices
- AppNote:

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file led.h.

## Enumeration Type Documentation

enum board_led_id

Connection of on-board LEDs.

Definition at line 49 of file led.h.

## Function Documentation

static void led_activate | ( | enum board_led_id | id | ) | `[inline, static]`

Turn LED id on.

Definition at line 59 of file led.h.

References gpio_set_value().

Here is the call graph for this function:

static void led_deactivate | ( | enum board_led_id | id | ) | `[inline, static]`

Turn LED id off.

Definition at line 67 of file led.h.

References gpio_set_value().

Referenced by led_blink_start().

Here is the call graph for this function: