<area shape="rect" href="$delayed__work_8h.html#43bcb2f7c67b9d14a94df6c210ab3c20" title="Initialize delayed work structure." alt="" coords="397,149,520,176">
<area shape="rect" href="$include_2dmac_2dma__controller_8h.html#1bd3070a2745772cdd91cf426a94951d" title="Initialize a DMA request." alt="" coords="211,48,312,75">
<area shape="rect" href="$slist_8h.html#430c94443e9ea2bc2dbaf3c3ab0e29db" title="Initialize a singly linked list." alt="" coords="424,23,493,49">
<area shape="rect" href="$chip_2at32uc3a3_2include_2chip_2clk_8h.html#5da96d9699e5d1a2fae145a7c0f86070" title="Get the rate of the bus clock connected to a MMC controller." alt="" coords="197,99,325,125">
<area shape="rect" href="$string_8h.html#ce6ee45c30e71865e6eb635200379db9" title="Initialize memory area." alt="" coords="228,200,295,227">
<area shape="rect" href="$card__detect_8c.html#dccecbe259464bb15aee5f44938ed6e7" title="Initialize card detection handler." alt="" coords="207,251,316,277">
<area shape="rect" href="$include_2workqueue_8h.html#8baf4fd3963ae6e8186ed90d01de7be1" title="Initialize a work item." alt="" coords="389,301,528,328">
<area shape="rect" href="$slot_8c.html#644e0e32acfb311a741be0cd0fc0dc94" title="Init slot structure." alt="" coords="204,352,319,379">
<area shape="rect" href="$arch_2avr32_2include_2arch_2softirq_8h.html#d4f26a0a7523954cd23a33959ea22833" title="Install a soft interrupt handler." alt="" coords="196,403,327,429">
<area shape="rect" href="$timer__tc_8h.html#704f557f9f6a389b492c63c2714e7637" title="Initialize a new task." alt="" coords="620,149,727,176">
<area shape="rect" href="$timer__tc_8h.html#aa2176a86f8b5b8115ca42c75416e018" title="Reset a used task." alt="" coords="807,149,924,176">
<area shape="rect" href="$chip_2at32uc3a3_2include_2chip_2clk_8h.html#d04168beba1e3c3acec8528f5ed291f9" title="Get the PBA clock rate in Hz." alt="" coords="392,99,525,125">
<area shape="rect" href="$gpio__irq__handler_8h.html#ebbb8a9c8861e4680e57a0cbeb38dcce" title="Init GPIO irq handler." alt="" coords="389,200,528,227">
<area shape="rect" href="$gpio__irq__handler_8c.html#08098b250a73090b40e5f39098426314" title="Register GPIO irq handler." alt="" coords="376,251,541,277">
<area shape="rect" href="$arch_2avr32_2include_2arch_2interrupt_8h.html#14f8e74622b9b8015f683609244cc345" title="Restore saved interrupt state." alt="" coords="619,251,728,277">
<area shape="rect" href="$arch_2avr32_2include_2arch_2interrupt_8h.html#bf4cfce4899dfd1c9aed203894731ae7" title="Save the current interrupt state and disable interrupts." alt="" coords="624,301,723,328">
<area shape="rect" href="$gpio__irq__group_8h.html#039f8b5faa5560ddab5994efa01d53bf" title="Convert pin type to group index." alt="" coords="589,352,757,379">
<area shape="rect" href="$slist_8h.html#cd0f70535b445ece86170eb70bd54365" title="Insert node as the last node in list." alt="" coords="620,200,727,227">
