# include/usb/msc_function.h File Reference

USB Mass Storage Class function driver. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Defines
#define | MSC_MAX_SERIAL_LEN 20
| Maximum number of characters in the device serial number.

## Detailed Description

USB Mass Storage Class function driver.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: All devices with a USB device controller
- AppNote:

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file msc_function.h.

## Define Documentation

#define MSC_MAX_SERIAL_LEN 20

Maximum number of characters in the device serial number.

Note that there's usually no point in having more than 12 characters.

Definition at line 49 of file msc_function.h.