# board/atevk1104/include/board/dataflash.h File Reference

ATEVK1104 dataflash connection. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Defines
#define | BOARD_DATAFLASH_SPI_PORT 0
| Which SPI instance is the dataflash connected to.
#define | BOARD_DATAFLASH_CS_PIN 14
| Which GPIO pin is used as chip select for the dataflash.
#define | BOARD_DATAFLASH_SPI_FREQUENCY 10000000
| SPI frequency used for dataflash communication.
#define | BOARD_DATAFLASH_SPI_MODE SPI_MODE_0
| SPI mode used for dataflash communication.

## Detailed Description

ATEVK1104 dataflash connection.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: ATEVK1104
- AppNote:

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file dataflash.h.

## Define Documentation

#define BOARD_DATAFLASH_CS_PIN 14

Which GPIO pin is used as chip select for the dataflash.

Definition at line 47 of file dataflash.h.

#define BOARD_DATAFLASH_SPI_FREQUENCY 10000000

SPI frequency used for dataflash communication.

Definition at line 49 of file dataflash.h.

#define BOARD_DATAFLASH_SPI_MODE SPI_MODE_0

SPI mode used for dataflash communication.

Definition at line 51 of file dataflash.h.

#define BOARD_DATAFLASH_SPI_PORT 0

Which SPI instance is the dataflash connected to.

Definition at line 45 of file dataflash.h.