<area shape="rect" href="$buffer_8h.html#08e06f378926444e51a796c70ab9037b" title="Initialize a buffer for transmitting data." alt="" coords="233,5,329,32">
<area shape="rect" href="$request_8h.html#26a25fb6b9fc952dd70b838d8586c0ae" title="Add a buffer to a USB request." alt="" coords="215,56,348,83">
<area shape="rect" href="$usb__lib_8c.html#d54b52dea624d4d17cec46ada6ed51ea" title="Allocate and initialize a USB request structure." alt="" coords="231,107,332,133">
<area shape="rect" href="$cpu_2uc3_2include_2cpu_2dma_8h.html#b504eec8bf78487fe59d6302592f7f10" title="Map a single contiguous buffer for DMA transfer." alt="" coords="397,5,517,32">
<area shape="rect" href="$slist_8h.html#cd0f70535b445ece86170eb70bd54365" title="Insert node as the last node in list." alt="" coords="404,56,511,83">
<area shape="rect" href="$mempool_8h.html#97c97a278ea319fb52aed350cae1bd27" title="Allocate an object from a memory pool." alt="" coords="400,107,515,133">
<area shape="rect" href="$usb__lib_8c.html#94fdae85da696787911c520913048a78" title="Initialize a USB request." alt="" coords="412,157,503,184">
<area shape="rect" href="$arch_2avr32_2include_2arch_2interrupt_8h.html#14f8e74622b9b8015f683609244cc345" title="Restore saved interrupt state." alt="" coords="567,56,676,83">
<area shape="rect" href="$arch_2avr32_2include_2arch_2interrupt_8h.html#bf4cfce4899dfd1c9aed203894731ae7" title="Save the current interrupt state and disable interrupts." alt="" coords="572,107,671,133">
<area shape="rect" href="$slist_8h.html#430c94443e9ea2bc2dbaf3c3ab0e29db" title="Initialize a singly linked list." alt="" coords="587,157,656,184">
