Functions

# C:/AVR32/ASF2.0.0/avr32/applications/uc3l-ek-SleepWalking-demo/SleepWalking_demo.c File Reference

SleepWalking demo application using the ADCIFB and AST interface on AVR32 devices. More...

`#include "compiler.h"`
`#include "preprocessor.h"`
`#include "board.h"`
`#include "power_clocks_lib.h"`
`#include "gpio.h"`
`#include "ast.h"`
`#include "adcifb.h"`

## Defines
Preset value used by ADCIFB analog comparator to compare with sampled value from Accelerometer X channel, this value will change according to the ADC resolution used (8/10/12 bit)
#define | SENSOR_PRESET_VALUE 0xF9
Target frequency
#define | EXAMPLE_USART_CLOCK_MASK AVR32_USART3_CLK_PBA
#define | EXAMPLE_TARGET_DFLL_FREQ_HZ 96000000
#define | EXAMPLE_TARGET_MCUCLK_FREQ_HZ 12000000
#define | EXAMPLE_TARGET_PBACLK_FREQ_HZ 12000000
#define | EXAMPLE_TARGET_CLK_ADC_FREQ_HZ 1500000
## Functions
void | init_ast (void)
void | ADCIFB_init (void)
int | main (void)
| This is an example showing how to use SleepWalking feature.
Delay routine

## Detailed Description

SleepWalking demo application using the ADCIFB and AST interface on AVR32 devices.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: All AVR32 devices with GPIO/AST/ADCIFB.
- AppNote:

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

## Function Documentation

void ADCIFB_init | ( | void |  | ) |

ADCIFB_init.

void init_ast | ( | void |  | ) |

AST Init.

All Files Functions