Functions

# C:/AVR32/ASF2.0.0/avr32/drivers/gpio/led_chaser_example/led_chaser_example.c File Reference

LED chaser application using the GPIO interface on AVR32 devices. More...

`#include "compiler.h"`
`#include "preprocessor.h"`
`#include "board.h"`
`#include "pm.h"`
`#include "gpio.h"`

## Defines
Number of LEDs to be illuminated
#define | MAX_LEDS 4
## Functions
int | main (void)
| This is an example showing how to create a LED chaser application.
void | delay_wait ()
| Delay routine.

## Detailed Description

LED chaser application using the GPIO interface on AVR32 devices.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: All AVR32 devices with GPIO.
- AppNote:

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

All Files Functions