| AVR Z-LINKŪ |

# serialInterface.SerialPortUtilities Class Reference

List of all members.

## Detailed Description

This file defines utility functions for establishing connection to a
serial port (RS232 or USB).

Application note:
  AVR414: User's Guide - ATAVRRZ502 - Accessory Kit

Author:
  Atmel Corporation: http://www.atmel.com
  Support email: avr@atmel.com

Name
  vkbakken

Revision
  1.5

RCSfile
  code_header_template_CVS_DOXYGEN.txt,v

Date
  2006/04/07 12:40:07

Definition at line 33 of file SerialPortUtilities.java.

## Static Public Member Functions
static boolean | addSerialEventListener (SerialPort portToAddListener, SerialPortEventListener listener)
| This function is used to add listeners to the chosen serial port.
static SerialPort | connectToSerialPort (String serialPortName)
| This function is used to open a serial port given its name.
static Vector< String > | getSerialPortNames ()
| This function returns a vector with the names of the accessible serial ports on the machine.
static boolean | setBaudRate (SerialPort portToConfigure, final int BAUD_RATE)
| This function is used to set the baud rate of the chosen serial port.

@DOC_TITLE@