| AVR Z-LINKŪ |

# AVR414 User's Guide - ATAVRRZ502 - Accessory Kit Class List

Here are the classes, structs, unions and interfaces with brief descriptions:

gui.ChatWindow | ChatWindow is a class that defines the graphical interface to display the live traffic. Incomming messages will be appended to the conversation ("Chat") and the end user can type in new messages
gui.ChatWindowEvent | Defines a ChatWindowEvent instance
gui.ChatWindowEventListener | Defines a ChatWindowEventListener interface
gui.ConfigurationDialog | The ConfigurationDialog is a extension of the JDialog
gui.Dialogs | Group of JDialogs used by the GUI
main.EventHandler | The EventHandler is the class that catches and handles all the events from the radio and user interactions through the GUI
main.Main | Class that contains the main loop
gui.MainFrame | The MainFrame is the background component (JFrame) and where tabing is enabled. This is what the user will see directly after start-up
gui.MainFrameEvent | MainFrameEvents are sent to MainFrameEventListeners to notify them that something new has happened
gui.MainFrameEventListener | MainFrameEventLIstener interface
radioInterface.NewAssociationIndication | Defines a NewAssociationIndication instance
radioInterface.NewAssociationIndicationListener | This interface defines the function that any NewAssociationIndicationListener must implement
radioInterface.NewDataIndication | Defines a NewDataIndication instance
radioInterface.NewDataIndicationListener | This interface defines the function that any NewDataIndicationListener must implement
radioInterface.NewDisassociationIndication | Class that defines the NewDisassociationIndication object. The NewDisassociationIndication notifies the NewDisassociation listener that one of the radios in the peer-to-peer link wishes to disconnect
radioInterface.NewDisassociationIndicationListener | This interface defines the function that any NewDisassociationIndicationListener must implement
radioInterface.RadioInterface | The radio interface is the next higher layer of the SerialStream. This layer defines the AT-Command interface to the radio
radioInterface.RadioInterfaceStartException | Class that defines the exception thrown by the RadioInterface in the case of an error during start-up of the radio
serialInterface.SerialPortUtilities | This file defines utility functions for establishing connection to a serial port (RS232 or USB)
serialInterface.SerialStream | This class defines serial streams that can be used for writing and reading to/from serial ports
serialInterface.SerialStreamEvent | This class is used for generation of new SerialStreamEvents
serialInterface.SerialStreamException | This class defiens the SerialStreamException
serialInterface.SerialStreamListener | This class defines an interface for SerialStreamListeners
radioInterface.TimeOut | This class defines a TimerTask that is used to ensure that the radio answers any request/command within a specified time

@DOC_TITLE@