| AVR Z-LINKŪ |

- All
- Functions
- Variables
- Enumerations
- Enumerator
- Defines

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- u
- x

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - a -

- ACTIVE_SCAN_FAILED : chat.h
- applicationInit() : main.c
- ASSOCIATION_FAILED : chat.h
- ASSOCIATION_NOTIFICATION : serialPortHAL.c
- ATC : atParser.c
- ATD : atParser.c
- ATR : atParser.c
- ATT : atParser.c

### - b -

- baudRate_t : usart.h
- BR_19200 : usart.h
- BR_38400 : usart.h
- BR_9600 : usart.h
- BUFFER_OVERFLOW : serialPortHAL.h

### - c -

- CHAT_ACTIVE_SCAN_PENDING : chat.h
- CHAT_ASSOCIATION_PENDING : chat.h
- CHAT_CONNECTED : chat.h
- CHAT_IDLE : chat.h
- CHAT_RESET_PENDING : chat.h
- CHAT_SET_ADDRESS_PENDING : chat.h
- CHAT_SET_PERMIT_ASSOCIATION_PENDING : chat.h
- CHAT_START_PENDING : chat.h
- CHAT_WAIT_FOR_ASSOCIATION : chat.h
- chatChannel : chat.h, atParser.c
- chatError_t : chat.h
- chatPANID : chat.h, atParser.c
- chatRole_t : chat.h
- chatState_t : chat.h
- COLLECT_PARAMETERS : serialPortHAL.h
- COORD_SHORT_ADDRESS : chat.h
- COORDINATOR : chat.h
- CRNL : serialPortHAL.c

### - d -

- DATA_CONVERSION_FAILED : chat.h
- DATA_TRANSMISSION_FAILED : chat.h
- dataAvailable() : serialPortHAL.h, serialPortHAL.c
- DEFAULT_CHANNEL : chat.h
- DEFAULT_PANID : chat.h
- DEVICE_TYPE_COORDINATOR : atParser.h
- DEVICE_TYPE_END_DEVICE : atParser.h
- DISABLE_RECEIVE_COMPLETE_INTERRUPT : usart.h
- DISABLE_RECEIVER : usart.h
- DISABLE_TRANSMITTER : usart.h
- DISASSOCIATION_NOTIFICATION : serialPortHAL.c

### - e -

- ENABLE_RECEIVE_COMPLETE_INTERRUPT : usart.h
- ENABLE_RECEIVER : usart.h
- ENABLE_TRANSMITTER : usart.h
- END_DEVICE : chat.h
- END_DEVICE_SHORT_ADDRESS : chat.h
- END_OF_STRING : utilities.h
- EOC : serialPortHAL.h
- EOC_DELIMITER : serialPortHAL.h
- ERROR : serialPortHAL.c
- errToHex() : serialPortHAL.c
- EVENT_BUFFER_FULL : chat.h

### - f -

- FTDI_CONFIGURE_PIN_CHANGE_INTERRUPT : ftdi.h
- FTDI_DDR : ftdi.h
- FTDI_DISABLE_RECEIVER : ftdi.h
- FTDI_ENABLE_RECEIVER : ftdi.h
- FTDI_ENABLE_TX : ftdi.h
- FTDI_Fifo : ftdi.h
- FTDI_FIFO_ADDRESS : ftdi.h
- FTDI_PIN : ftdi.h
- FTDI_PORT : ftdi.h
- FTDI_RX_PIN : ftdi.h
- FTDI_TX_MASK : ftdi.h
- FTDI_TX_PIN : ftdi.h
- ftdiInitialization() : ftdi.h, ftdi.c
- ftdiSendSymbol() : ftdi.h, ftdi.c

### - g -

- getATCommand() : serialPortHAL.h, serialPortHAL.c
- getError() : serialPortHAL.h, serialPortHAL.c
- getParameterNumber() : serialPortHAL.h, serialPortHAL.c

### - h -

- handleNewCommand() : atParser.h, atParser.c
- hexTable : serialPortHAL.c
- htoi16() : utilities.h, utilities.c
- htoi8() : utilities.h, utilities.c

### - i -

- INCONSISTENT_STATE : chat.h
- INVALID_REQUEST : chat.h
- ISR() : serialPortHAL.h, serialPortHAL.c

### - l -

- LENGTH_OF_COMMAND : serialPortHAL.h
- LENGTH_OF_PARAMETER_BUFFER : serialPortHAL.h
- LOW : ftdi.h

### - m -

- main() : main.c
- MAX_MSG_LENGTH : chat.h

### - n -

- NEW_DATA_NOTIFICATION : serialPortHAL.c
- NO_ERROR : serialPortHAL.h
- NULL_PARAMETER : serialPortHAL.h
- NUMBER_OF_PARAMETERS : serialPortHAL.h

### - o -

- OK : serialPortHAL.c

### - p -

- PARAM_PREAMBLE : serialPortHAL.h
- PARAMETER_1 : serialPortHAL.h
- PARAMETER_2 : serialPortHAL.h
- PARAMETER_3 : serialPortHAL.h
- PARAMETER_DELIMITER : serialPortHAL.h
- PARAMETER_PREAMBLE_A : serialPortHAL.h
- PARAMETER_PREAMBLE_B : serialPortHAL.h
- paramter_t : serialPortHAL.h
- permit : callbacks.c

### - r -

- RECEIVE_BUFFER_SIZE : serialPortHAL.h
- RECEIVER_OFF : serialPortHAL.h
- RECEIVER_ON : serialPortHAL.h
- RESET_FAILED : chat.h
- role : chat.h, atParser.c
- rxData : serialPortHAL.c
- rxError_t : serialPortHAL.h
- rxReset() : serialPortHAL.h, serialPortHAL.c
- rxState : serialPortHAL.c
- rxState_t : serialPortHAL.h

### - s -

- SCANDURATION : chat.h
- sendAssociationNotification() : serialPortHAL.h, serialPortHAL.c
- sendDataNotification() : serialPortHAL.h, serialPortHAL.c
- sendDisAssociationNotification() : serialPortHAL.h, serialPortHAL.c
- sendERROR() : serialPortHAL.h, serialPortHAL.c
- sendFlashString() : serialPortHAL.h, serialPortHAL.c
- sendMsg() : atParser.c
- sendOK() : serialPortHAL.h, serialPortHAL.c
- sendString() : serialPortHAL.h, serialPortHAL.c
- sendStringWithLength() : serialPortHAL.c
- sendSymbol() : serialPortHAL.c
- serialInterfaceInitialization() : serialPortHAL.h, serialPortHAL.c
- SET_MAC_ADDRESS_FAILED : chat.h
- shortAddress : callbacks.c
- SOC : serialPortHAL.h
- START_NETWORK_FAILED : chat.h
- startNetworkOperation() : atParser.c
- state : chat.h, atParser.c
- stopNetworkOperation() : atParser.c
- stringCompare() : utilities.h, utilities.c

### - u -

- UART : serialPortHAL.h
- uartInitialization() : usart.h, usart.c
- uartSendSymbol() : usart.h, usart.c
- UNDEFINED : chat.h
- UNKNOWN_AT_COMMAND : chat.h
- UNKNOWN_DEVICE_TYPE : chat.h
- UNKNOWN_EOC_SEQUENCE : serialPortHAL.h
- UNKNOWN_RX_STATE : serialPortHAL.h
- UNKNOWN_SEQUENCE : serialPortHAL.h
- usr_mcps_data_conf() : callbacks.c
- usr_mcps_data_ind() : callbacks.c
- usr_mlme_associate_conf() : callbacks.c
- usr_mlme_associate_ind() : callbacks.c
- usr_mlme_comm_status_ind() : callbacks.c
- usr_mlme_reset_conf() : callbacks.c
- usr_mlme_scan_conf() : callbacks.c
- usr_mlme_set_conf() : callbacks.c
- usr_mlme_start_conf() : callbacks.c

### - x -

- XRAM_DISABLE : ftdi.h
- XRAM_ENABLE : ftdi.h

@DOC_TITLE@