| AVR Z-LINKŪ |

# Package radioInterface

## Classes
class | NewAssociationIndication
| Defines a NewAssociationIndication instance. More...
interface | NewAssociationIndicationListener
| This interface defines the function that any NewAssociationIndicationListener must implement. More...
class | NewDataIndication
| Defines a NewDataIndication instance. More...
interface | NewDataIndicationListener
| This interface defines the function that any NewDataIndicationListener must implement. More...
class | NewDisassociationIndication
| Class that defines the NewDisassociationIndication object. The NewDisassociationIndication notifies the NewDisassociation listener that one of the radios in the peer-to-peer link wishes to disconnect. More...
interface | NewDisassociationIndicationListener
| This interface defines the function that any NewDisassociationIndicationListener must implement. More...
class | RadioInterface
| The radio interface is the next higher layer of the SerialStream. This layer defines the AT-Command interface to the radio. More...
class | RadioInterfaceStartException
| Class that defines the exception thrown by the RadioInterface in the case of an error during start-up of the radio. More...
class | TimeOut
| This class defines a TimerTask that is used to ensure that the radio answers any request/command within a specified time. More...

@DOC_TITLE@