- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# USB pipe drivers
[USB low level drivers]

These macros manage the common features of the pipes. More...

## Defines
#define | Host_select_pipe(p) (UPNUM = (U8)p)
| selects pipe for CPU interface
#define | Host_get_selected_pipe() (UPNUM )
| get the currently selected pipe number
#define | Host_enable_pipe() (UPCONX |= (1<<PEN))
| enables pipe
#define | Host_disable_pipe() (UPCONX &= ~(1<<PEN))
| disables pipe
#define | Host_set_token_setup() (UPCFG0X = UPCFG0X & ~MSK_TOKEN_SETUP)
| sets SETUP token
#define | Host_set_token_in() (UPCFG0X = (UPCFG0X & ~MSK_TOKEN_SETUP) | MSK_TOKEN_IN)
| sets IN token
#define | Host_set_token_out() (UPCFG0X = (UPCFG0X & ~MSK_TOKEN_SETUP) | MSK_TOKEN_OUT)
| sets OUT token
#define | Host_get_endpoint_number() (UPCFG0X & (MSK_PEPNUM))
| returns the number of the endpoint associated to the current pipe
#define | Host_get_pipe_interrupt() (UPINT)
| returns pipe interrupt register
#define | Host_set_interrupt_frequency(frq) (UPCFG2X = (U8)frq)
| sets the interrupt frequency
#define | Is_pipe_configured() (UPSTAX & (1<<CFGOK))
| tests if current pipe is configured
#define | Is_host_one_bank_busy() ((UPSTAX & MSK_NBUSYBK) != 0)
| tests if at least one bank is busy
#define | Host_number_of_busy_bank() (UPSTAX & MSK_NBUSYBK)
| returns the number of busy banks
#define | Host_reset_pipe(p) (UPRST = 1<<p , UPRST = 0)
| resets the pipe
#define | Host_write_byte(dat) (UPDATX = dat)
| writes a byte into the pipe FIFO
#define | Host_read_byte() (UPDATX)
| reads a byte from the pipe FIFO
#define | Host_freeze_pipe() (UPCONX |= (1<<PFREEZE))
| freezes the pipe
#define | Host_unfreeze_pipe() (UPCONX &= ~(1<<PFREEZE))
| un-freezees the pipe
#define | Is_host_pipe_freeze() (UPCONX & (1<<PFREEZE))
| tests if the current pipe is frozen
#define | Host_reset_pipe_data_toggle() (UPCONX |= (1<<RSTDT) )
| resets data toggle
#define | Is_host_setup_sent() ((UPINTX & (1<<TXSTPI)) ? TRUE : FALSE)
| tests if SETUP has been sent
#define | Is_host_control_in_received() ((UPINTX & (1<<RXINI)) ? TRUE : FALSE)
| tests if control IN has been received
#define | Is_host_control_out_sent() ((UPINTX & (1<<TXOUTI)) ? TRUE : FALSE)
| tests if control OUT has been sent
#define | Is_host_stall() ((UPINTX & (1<<RXSTALLI)) ? TRUE : FALSE)
| tests if a STALL has been received
#define | Is_host_pipe_error() ((UPINTX & (1<<PERRI)) ? TRUE : FALSE)
| tests if an error occurs on current pipe
#define | Host_send_setup() (UPINTX &= ~(1<<FIFOCON))
| sends a setup
#define | Host_send_control_in() (UPINTX &= ~(1<<FIFOCON))
| sends a control IN
#define | Host_send_control_out() (UPINTX &= ~(1<<FIFOCON))
| sends a control OUT
#define | Host_ack_control_out() (UPINTX &= ~(1<<TXOUTI))
| acks control OUT
#define | Host_ack_control_in() (UPINTX &= ~(1<<RXINI))
| acks control IN
#define | Host_ack_setup() (UPINTX &= ~(1<<TXSTPI))
| acks setup
#define | Host_ack_stall() (UPINTX &= ~(1<<RXSTALLI))
| acks STALL reception
#define | Host_send_out() (UPINTX &= ~(1<<FIFOCON))
| sends a OUT
#define | Is_host_out_sent() ((UPINTX & (1<<TXOUTI)) ? TRUE : FALSE)
| tests if OUT has been sent
#define | Host_ack_out_sent() (UPINTX &= ~(1<<TXOUTI))
| acks OUT sent
#define | Is_host_in_received() ((UPINTX & (1<<RXINI)) ? TRUE : FALSE)
| tests if IN received
#define | Host_ack_in_received() (UPINTX &= ~(1<<RXINI))
| acks IN reception
#define | Host_send_in() (UPINTX &= ~(1<<FIFOCON))
| sends a IN
#define | Is_host_nak_received() ((UPINTX & (1<<NAKEDI)) ? TRUE : FALSE)
| tests if nak handshake has been received
#define | Host_ack_nak_received() (UPINTX &= ~(1<<NAKEDI))
| acks NAk received sent
#define | Is_host_read_enabled() (UPINTX&(1<<RWAL))
| tests if endpoint read allowed
#define | Is_host_write_enabled() (UPINTX&(1<<RWAL))
| tests if endpoint read allowed
#define | Host_standard_in_mode() (UPCONX &= ~(1<<INMODE))
| sets IN in standard mode
#define | Host_continuous_in_mode() (UPCONX |= (1<<INMODE))
| sets IN in continuous mode
#define | Host_in_request_number(in_num) (UPINRQX = (U8)in_num)
| sets number of IN requests to perform before freeze
#define | Host_get_in_request_number() (UPINRQX)
| returns number of remaining IN requests
#define | Host_data_length_U8() (UPBCLX)
| returns number of bytes (8 bits)
#define | Host_data_length_U16() ((((U16)UPBCHX)<<8) | UPBCLX)
| returns number of bytes (16 bits)
#define | Host_byte_counter() Host_data_length_U16()
| for device compatibility
#define | Host_byte_counter_8() Host_data_length_U8()
| for device compatibility
#define | Host_get_pipe_length() ((U16)0x08 << ((UPCFG1X & MSK_PSIZE)>>4))
| returns the size of the current pipe
#define | Host_get_pipe_type() (UPCFG0X>>6)
| returns the type of the current pipe
#define | Host_error_status() (UPERRX & MSK_ERROR)
| tests if error occurs on pipe
#define | Host_ack_all_errors() (UPERRX = 0x00)
| acks all pipe error
#define | Host_enable_transmit_interrupt() (UPIENX |= (1<<TXOUTE))
| Enable pipe end transmission interrupt.
#define | Host_disable_transmit_interrupt() (UPIENX &= ~(1<<TXOUTE))
| Disable pipe end transmission interrupt.
#define | Host_enable_receive_interrupt() (UPIENX |= (1<<RXINE))
| Enable pipe reception interrupt.
#define | Host_disable_receive_interrupt() (UPIENX &= ~(1<<RXINE))
| Disable pipe recption interrupt.
#define | Host_enable_stall_interrupt() (UPIENX |= (1<<RXSTALLE))
| Enable pipe stall interrupt.
#define | Host_disable_stall_interrupt() (UPIENX &= ~(1<<RXSTALLE))
| Disable pipe stall interrupt.
#define | Host_enable_error_interrupt() (UPIENX |= (1<<PERRE))
| Enable pipe error interrupt.
#define | Host_disable_error_interrupt() (UPIENX &= ~(1<<PERRE))
| Disable pipe error interrupt.
#define | Host_enable_nak_interrupt() (UPIENX |= (1<<NAKEDE))
| Enable pipe NAK interrupt.
#define | Host_disable_nak_interrupt() (UPIENX &= ~(1<<NAKEDE))
| Disable pipe NAK interrupt.
#define | Get_pipe_token(x) ((x & (0x80)) ? TOKEN_IN : TOKEN_OUT)

## Detailed Description

These macros manage the common features of the pipes.

## Define Documentation

#define Host_select_pipe | ( | p |  | ) | (UPNUM = (U8)p)

selects pipe for CPU interface

Definition at line 766 of file usb_drv.h.

Referenced by freeze_user_periodic_pipe(), host_auto_configure_endpoint(), host_disable_all_pipe(), host_get_data(), host_get_data_interrupt(), host_mem_stall_management(), host_send_control(), host_send_data(), host_send_data_interrupt(), remove_device_entry(), unfreeze_user_periodic_pipe(), usb_general_interrupt(), usb_host_task(), and usb_pipe_interrupt().

#define Host_get_selected_pipe | ( |  | ) | (UPNUM )

get the currently selected pipe number

Definition at line 769 of file usb_drv.h.

Referenced by host_auto_configure_endpoint(), remove_device_entry(), usb_general_interrupt(), and usb_pipe_interrupt().

#define Host_enable_pipe | ( |  | ) | (UPCONX |= (1<<PEN))

enables pipe

Definition at line 772 of file usb_drv.h.

Referenced by host_auto_configure_endpoint(), and host_config_pipe().

#define Host_disable_pipe | ( |  | ) | (UPCONX &= ~(1<<PEN))

disables pipe

Definition at line 774 of file usb_drv.h.

Referenced by host_auto_configure_endpoint(), and host_disable_all_pipe().

#define Host_set_token_setup | ( |  | ) | (UPCFG0X = UPCFG0X & ~MSK_TOKEN_SETUP)

sets SETUP token

Definition at line 777 of file usb_drv.h.

Referenced by host_send_control().

#define Host_set_token_in | ( |  | ) | (UPCFG0X = (UPCFG0X & ~MSK_TOKEN_SETUP) | MSK_TOKEN_IN)

sets IN token

Definition at line 779 of file usb_drv.h.

Referenced by host_get_data(), host_get_data_interrupt(), and host_send_control().

#define Host_set_token_out | ( |  | ) | (UPCFG0X = (UPCFG0X & ~MSK_TOKEN_SETUP) | MSK_TOKEN_OUT)

sets OUT token

Definition at line 781 of file usb_drv.h.

Referenced by host_send_control(), and host_send_data().

#define Host_get_endpoint_number | ( |  | ) | (UPCFG0X & (MSK_PEPNUM))

returns the number of the endpoint associated to the current pipe

Definition at line 784 of file usb_drv.h.

Referenced by host_mem_stall_management().

#define Host_get_pipe_interrupt | ( |  | ) | (UPINT)

returns pipe interrupt register

Definition at line 787 of file usb_drv.h.

Referenced by usb_get_nb_pipe_interrupt().

#define Host_set_interrupt_frequency | ( | frq |  | ) | (UPCFG2X = (U8)frq)

sets the interrupt frequency

Definition at line 790 of file usb_drv.h.

#define Is_pipe_configured | ( |  | ) | (UPSTAX & (1<<CFGOK))

tests if current pipe is configured

Definition at line 793 of file usb_drv.h.

Referenced by host_config_pipe().

#define Is_host_one_bank_busy | ( |  | ) | ((UPSTAX & MSK_NBUSYBK) != 0)

tests if at least one bank is busy

Definition at line 795 of file usb_drv.h.

#define Host_number_of_busy_bank | ( |  | ) | (UPSTAX & MSK_NBUSYBK)

returns the number of busy banks

Definition at line 797 of file usb_drv.h.

Referenced by host_send_data().

#define Host_reset_pipe | ( | p |  | ) | (UPRST = 1<<p , UPRST = 0)

resets the pipe

Definition at line 800 of file usb_drv.h.

Referenced by host_disable_all_pipe(), host_get_data(), host_get_data_interrupt(), host_send_control(), host_send_data(), and host_send_data_interrupt().

#define Host_write_byte | ( | dat |  | ) | (UPDATX = dat)

writes a byte into the pipe FIFO

Definition at line 803 of file usb_drv.h.

Referenced by host_send_control(), host_send_data(), host_send_data_interrupt(), and usb_pipe_interrupt().

#define Host_read_byte | ( |  | ) | (UPDATX)

reads a byte from the pipe FIFO

Definition at line 805 of file usb_drv.h.

Referenced by host_get_data(), host_send_control(), usb_host_task(), and usb_pipe_interrupt().

#define Host_freeze_pipe | ( |  | ) | (UPCONX |= (1<<PFREEZE))

freezes the pipe

Definition at line 808 of file usb_drv.h.

Referenced by freeze_user_periodic_pipe(), host_get_data(), host_send_control(), host_send_data(), usb_host_task(), and usb_pipe_interrupt().

#define Host_unfreeze_pipe | ( |  | ) | (UPCONX &= ~(1<<PFREEZE))

un-freezees the pipe

Definition at line 810 of file usb_drv.h.

Referenced by df_host_read_sector(), df_host_write_sector(), host_get_data(), host_get_data_interrupt(), host_send_control(), host_send_data(), host_send_data_interrupt(), unfreeze_user_periodic_pipe(), usb_host_task(), and usb_pipe_interrupt().

#define Is_host_pipe_freeze | ( |  | ) | (UPCONX & (1<<PFREEZE))

tests if the current pipe is frozen

Definition at line 812 of file usb_drv.h.

Referenced by freeze_user_periodic_pipe().

#define Host_reset_pipe_data_toggle | ( |  | ) | (UPCONX |= (1<<RSTDT) )

resets data toggle

Definition at line 815 of file usb_drv.h.

Referenced by host_mem_stall_management().

#define Is_host_setup_sent | ( |  | ) | ((UPINTX & (1<<TXSTPI)) ? TRUE : FALSE)

tests if SETUP has been sent

Definition at line 818 of file usb_drv.h.

Referenced by host_send_control().

#define Is_host_control_in_received | ( |  | ) | ((UPINTX & (1<<RXINI)) ? TRUE : FALSE)

tests if control IN has been received

Definition at line 820 of file usb_drv.h.

Referenced by host_send_control().

#define Is_host_control_out_sent | ( |  | ) | ((UPINTX & (1<<TXOUTI)) ? TRUE : FALSE)

tests if control OUT has been sent

Definition at line 822 of file usb_drv.h.

Referenced by host_send_control().

#define Is_host_stall | ( |  | ) | ((UPINTX & (1<<RXSTALLI)) ? TRUE : FALSE)

tests if a STALL has been received

Definition at line 824 of file usb_drv.h.

Referenced by host_get_data(), host_send_control(), host_send_data(), usb_host_task(), and usb_pipe_interrupt().

#define Is_host_pipe_error | ( |  | ) | ((UPINTX & (1<<PERRI)) ? TRUE : FALSE)

tests if an error occurs on current pipe

Definition at line 826 of file usb_drv.h.

Referenced by host_get_data(), host_send_control(), host_send_data(), and usb_pipe_interrupt().

#define Host_send_setup | ( |  | ) | (UPINTX &= ~(1<<FIFOCON))

sends a setup

Definition at line 828 of file usb_drv.h.

Referenced by host_send_control().

#define Host_send_control_in | ( |  | ) | (UPINTX &= ~(1<<FIFOCON))

sends a control IN

Definition at line 830 of file usb_drv.h.

Referenced by host_send_control().

#define Host_send_control_out | ( |  | ) | (UPINTX &= ~(1<<FIFOCON))

sends a control OUT

Definition at line 832 of file usb_drv.h.

Referenced by host_send_control().

#define Host_ack_control_out | ( |  | ) | (UPINTX &= ~(1<<TXOUTI))

acks control OUT

Definition at line 834 of file usb_drv.h.

Referenced by host_send_control().

#define Host_ack_control_in | ( |  | ) | (UPINTX &= ~(1<<RXINI))

acks control IN

Definition at line 836 of file usb_drv.h.

Referenced by host_send_control().

#define Host_ack_setup | ( |  | ) | (UPINTX &= ~(1<<TXSTPI))

acks setup

Definition at line 838 of file usb_drv.h.

Referenced by host_send_control().

#define Host_ack_stall | ( |  | ) | (UPINTX &= ~(1<<RXSTALLI))

acks STALL reception

Definition at line 840 of file usb_drv.h.

Referenced by host_get_data(), host_get_data_interrupt(), host_mem_stall_management(), host_send_control(), host_send_data(), and host_send_data_interrupt().

#define Host_send_out | ( |  | ) | (UPINTX &= ~(1<<FIFOCON))

sends a OUT

Definition at line 843 of file usb_drv.h.

Referenced by df_host_read_sector(), host_send_data(), host_send_data_interrupt(), and usb_pipe_interrupt().

#define Is_host_out_sent | ( |  | ) | ((UPINTX & (1<<TXOUTI)) ? TRUE : FALSE)

tests if OUT has been sent

Definition at line 845 of file usb_drv.h.

Referenced by df_host_read_sector(), host_send_data(), and usb_pipe_interrupt().

#define Host_ack_out_sent | ( |  | ) | (UPINTX &= ~(1<<TXOUTI))

acks OUT sent

Definition at line 847 of file usb_drv.h.

Referenced by df_host_read_sector(), host_send_data(), host_send_data_interrupt(), and usb_pipe_interrupt().

#define Is_host_in_received | ( |  | ) | ((UPINTX & (1<<RXINI)) ? TRUE : FALSE)

tests if IN received

Definition at line 849 of file usb_drv.h.

Referenced by host_get_data(), usb_host_task(), and usb_pipe_interrupt().

#define Host_ack_in_received | ( |  | ) | (UPINTX &= ~(1<<RXINI))

acks IN reception

Definition at line 851 of file usb_drv.h.

Referenced by df_host_write_sector(), host_get_data(), host_get_data_interrupt(), host_send_control(), usb_host_task(), and usb_pipe_interrupt().

#define Host_send_in | ( |  | ) | (UPINTX &= ~(1<<FIFOCON))

sends a IN

Definition at line 853 of file usb_drv.h.

Referenced by host_get_data(), usb_host_task(), and usb_pipe_interrupt().

#define Is_host_nak_received | ( |  | ) | ((UPINTX & (1<<NAKEDI)) ? TRUE : FALSE)

tests if nak handshake has been received

Definition at line 855 of file usb_drv.h.

Referenced by host_get_data(), host_send_data(), usb_host_task(), and usb_pipe_interrupt().

#define Host_ack_nak_received | ( |  | ) | (UPINTX &= ~(1<<NAKEDI))

acks NAk received sent

Definition at line 857 of file usb_drv.h.

Referenced by host_get_data(), host_get_data_interrupt(), host_send_data(), host_send_data_interrupt(), usb_host_task(), and usb_pipe_interrupt().

#define Is_host_read_enabled | ( |  | ) | (UPINTX&(1<<RWAL))

tests if endpoint read allowed

Definition at line 862 of file usb_drv.h.

Referenced by df_host_write_sector().

#define Is_host_write_enabled | ( |  | ) | (UPINTX&(1<<RWAL))

tests if endpoint read allowed

Definition at line 864 of file usb_drv.h.

#define Host_standard_in_mode | ( |  | ) | (UPCONX &= ~(1<<INMODE))

sets IN in standard mode

Definition at line 867 of file usb_drv.h.

Referenced by host_send_control().

#define Host_continuous_in_mode | ( |  | ) | (UPCONX |= (1<<INMODE))

sets IN in continuous mode

Definition at line 869 of file usb_drv.h.

Referenced by host_get_data(), and host_get_data_interrupt().

#define Host_in_request_number | ( | in_num |  | ) | (UPINRQX = (U8)in_num)

sets number of IN requests to perform before freeze

Definition at line 872 of file usb_drv.h.

#define Host_get_in_request_number | ( |  | ) | (UPINRQX)

returns number of remaining IN requests

Definition at line 874 of file usb_drv.h.

#define Host_data_length_U8 | ( |  | ) | (UPBCLX)

returns number of bytes (8 bits)

Definition at line 877 of file usb_drv.h.

Referenced by host_send_control().

#define Host_data_length_U16 | ( |  | ) | ((((U16)UPBCHX)<<8) | UPBCLX)

returns number of bytes (16 bits)

Definition at line 879 of file usb_drv.h.

#define Host_byte_counter | ( |  | ) | Host_data_length_U16()

for device compatibility

Definition at line 881 of file usb_drv.h.

Referenced by host_get_data(), and usb_pipe_interrupt().

#define Host_byte_counter_8 | ( |  | ) | Host_data_length_U8()

for device compatibility

Definition at line 883 of file usb_drv.h.

#define Host_get_pipe_length | ( |  | ) | ((U16)0x08 << ((UPCFG1X & MSK_PSIZE)>>4))

returns the size of the current pipe

Definition at line 886 of file usb_drv.h.

Referenced by host_get_data(), host_send_data(), host_send_data_interrupt(), and usb_pipe_interrupt().

#define Host_get_pipe_type | ( |  | ) | (UPCFG0X>>6)

returns the type of the current pipe

Definition at line 889 of file usb_drv.h.

Referenced by usb_general_interrupt(), and usb_pipe_interrupt().

#define Host_error_status | ( |  | ) | (UPERRX & MSK_ERROR)

tests if error occurs on pipe

Definition at line 892 of file usb_drv.h.

Referenced by host_get_data(), host_send_control(), host_send_data(), and usb_pipe_interrupt().

#define Host_ack_all_errors | ( |  | ) | (UPERRX = 0x00)

acks all pipe error

Definition at line 894 of file usb_drv.h.

Referenced by host_get_data(), host_send_control(), host_send_data(), and usb_pipe_interrupt().

#define Host_enable_transmit_interrupt | ( |  | ) | (UPIENX |= (1<<TXOUTE))

Enable pipe end transmission interrupt.

Definition at line 897 of file usb_drv.h.

Referenced by host_send_data_interrupt().

#define Host_disable_transmit_interrupt | ( |  | ) | (UPIENX &= ~(1<<TXOUTE))

Disable pipe end transmission interrupt.

Definition at line 899 of file usb_drv.h.

#define Host_enable_receive_interrupt | ( |  | ) | (UPIENX |= (1<<RXINE))

Enable pipe reception interrupt.

Definition at line 902 of file usb_drv.h.

Referenced by host_get_data_interrupt().

#define Host_disable_receive_interrupt | ( |  | ) | (UPIENX &= ~(1<<RXINE))

Disable pipe recption interrupt.

Definition at line 904 of file usb_drv.h.

#define Host_enable_stall_interrupt | ( |  | ) | (UPIENX |= (1<<RXSTALLE))

Enable pipe stall interrupt.

Definition at line 907 of file usb_drv.h.

Referenced by host_get_data_interrupt(), and host_send_data_interrupt().

#define Host_disable_stall_interrupt | ( |  | ) | (UPIENX &= ~(1<<RXSTALLE))

Disable pipe stall interrupt.

Definition at line 909 of file usb_drv.h.

#define Host_enable_error_interrupt | ( |  | ) | (UPIENX |= (1<<PERRE))

Enable pipe error interrupt.

Definition at line 912 of file usb_drv.h.

Referenced by host_get_data_interrupt(), and host_send_data_interrupt().

#define Host_disable_error_interrupt | ( |  | ) | (UPIENX &= ~(1<<PERRE))

Disable pipe error interrupt.

Definition at line 914 of file usb_drv.h.

#define Host_enable_nak_interrupt | ( |  | ) | (UPIENX |= (1<<NAKEDE))

Enable pipe NAK interrupt.

Definition at line 917 of file usb_drv.h.

Referenced by host_get_data_interrupt(), and host_send_data_interrupt().

#define Host_disable_nak_interrupt | ( |  | ) | (UPIENX &= ~(1<<NAKEDE))

Disable pipe NAK interrupt.

Definition at line 919 of file usb_drv.h.

#define Get_pipe_token | ( | x |  | ) | ((x & (0x80)) ? TOKEN_IN : TOKEN_OUT)

Definition at line 921 of file usb_drv.h.

Referenced by host_auto_configure_endpoint().