- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# USB regulator configuration
[USB application configuration]

## Defines
#define | USE_USB_PADS_REGULATOR ENABLE

## Define Documentation

#define USE_USB_PADS_REGULATOR ENABLE

Enable the internal regulator for USB pads When the application voltage is lower than 3.5V, to optimize power consumption the internal USB pads regulatr can be disabled.

Definition at line 81 of file conf_usb.h.