- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# storage_task.h File Reference

`#include "config.h"`

Include dependency graph for storage_task.h:

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Defines
#define | Usb_set_ms_data_direction_in() (ms_data_direction = 1)
#define | Usb_set_ms_data_direction_out() (ms_data_direction = 0)
#define | Is_usb_ms_data_direction_in() (ms_data_direction == 1)
#define | Is_usb_ms_data_direction_out() (ms_data_direction == 0)
## Functions
void | sof_action (void)

## Detailed Description

This file contains the function declarations - Compiler: IAR EWAVR and GNU GCC for AVR

- Supported devices: AT90USB1287, AT90USB1286, AT90USB647, AT90USB646
  Author:
    Atmel Corporation: http://www.atmel.com
    Support and FAQ: http://support.atmel.no/

Definition in file storage_task.h.

## Define Documentation

#define Usb_set_ms_data_direction_in | ( |  | ) | (ms_data_direction = 1)

Definition at line 51 of file storage_task.h.

Referenced by usb_mass_storage_cbw().

#define Usb_set_ms_data_direction_out | ( |  | ) | (ms_data_direction = 0)

Definition at line 52 of file storage_task.h.

Referenced by usb_mass_storage_cbw().

#define Is_usb_ms_data_direction_in | ( |  | ) | (ms_data_direction == 1)

Definition at line 53 of file storage_task.h.

Referenced by sbc_write_10(), and usb_mass_storage_cbw().

#define Is_usb_ms_data_direction_out | ( |  | ) | (ms_data_direction == 0)

Definition at line 54 of file storage_task.h.

Referenced by sbc_read_10().

## Function Documentation

void sof_action | ( | void |  | ) |