- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# timer16_drv.h

Go to the documentation of this file.

    00001 /*This file has been prepared for Doxygen automatic documentation generation.*/
    00013
    00014 /* Copyright (c) 2007, Atmel Corporation All rights reserved.
    00015  *
    00016  * Redistribution and use in source and binary forms, with or without
    00017  * modification, are permitted provided that the following conditions are met:
    00018  *
    00019  * 1. Redistributions of source code must retain the above copyright notice,
    00020  * this list of conditions and the following disclaimer.
    00021  *
    00022  * 2. Redistributions in binary form must reproduce the above copyright notice,
    00023  * this list of conditions and the following disclaimer in the documentation
    00024  * and/or other materials provided with the distribution.
    00025  *
    00026  * 3. The name of ATMEL may not be used to endorse or promote products derived
    00027  * from this software without specific prior written permission.
    00028  *
    00029  * THIS SOFTWARE IS PROVIDED BY ATMEL ``AS IS'' AND ANY EXPRESS OR IMPLIED
    00030  * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
    00031  * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NON-INFRINGEMENT ARE EXPRESSLY AND
    00032  * SPECIFICALLY DISCLAIMED. IN NO EVENT SHALL ATMEL BE LIABLE FOR ANY DIRECT,
    00033  * INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
    00034  * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
    00035  * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
    00036  * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
    00037  * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
    00038  * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
    00039  */
    00040
    00041 #ifndef _TIMER16_DRV_H_
    00042 #define _TIMER16_DRV_H_
    00043
    00044 //_____ I N C L U D E S ________________________________________________________
    00045
    00046 #include "config.h"
    00047
    00048 //_____ G E N E R A L    D E F I N I T I O N S _________________________________
    00049
    00050 #ifndef FOSC
    00051 #  error  You must define FOSC in "config.h" file
    00052 #endif
    00053     // ----------
    00054 #ifndef TIMER16_1            // 16-bit TIMER 1 Defintion
    00055 #define TIMER16_1       0x01
    00056 #endif
    00057 #ifndef TIMER16_3            // 16-bit TIMER 3 Defintion
    00058 #define TIMER16_3       0x03
    00059 #endif
    00060 #ifndef BOTH_TIMER16         // Both the 16-bit TIMERs Defintion
    00061 #define BOTH_TIMER16    0xFF
    00062 #endif
    00063
    00064 //_____ M A C R O S ____________________________________________________________
    00065
    00066     // ---------- To order the loading (reading) of 16-bit registers
    00067 #define Timer16_get_counter()       ( timer16_get_counter() )        // c.f. "timer16_drv.c" file
    00068 #define Timer16_get_capture()       ( timer16_get_capture() )        // c.f. "timer16_drv.c" file
    00069     // ---------- Two ways to have a look on the things
    00070 #define Timer16_set_pwm_a(value)    ( Timer16_set_compare_a(value) ) // c.f. above !
    00071 #define Timer16_set_pwm_b(value)    ( Timer16_set_compare_b(value) ) // c.f. above !
    00072 #define Timer16_set_pwm_c(value)    ( Timer16_set_compare_c(value) ) // c.f. above !
    00073 #define Timer16_get_pwm_a()         ( Timer16_get_compare_a() )      // c.f. above !
    00074 #define Timer16_get_pwm_b()         ( Timer16_get_compare_b() )      // c.f. above !
    00075 #define Timer16_get_pwm_c()         ( Timer16_get_compare_c() )      // c.f. above !
    00076     // ---------- If no clock, the timer is off !
    00077 #define Timer16_off()                 Timer16_set_clock(TIMER16_NO_CLOCK)
    00078
    00079 //_____ D E F .  &   M A C R O S   for   H W   C O N F . _______________________
    00080
    00081     //----- CARE WITH THE ORDER WHEN 16-BIT REGISTERS ARE READ
    00082     //      ==================================================
    00083     //----- For sensitive 16-bit registers (c.f. temporary reg), the macros are:
    00084     //-----     *  Timer16_get_nnn_low()
    00085     //-----     *  Timer16_get_nnn_high()
    00086     //----- For instance, in your main, do not write:
    00087     //-----     short_temp = ((Timer16_get_nnn_high())<<8) | (Timer16_get_nnn_low());
    00088     //-----   or
    00089     //-----     short_temp = (Timer16_get_nnn_low()) | ((Timer16_get_nnn_high())<<8);
    00090     //-----   because IAR and ImageCraft doesn't evaluate the operandes in the same order!
    00091     //-----
    00092     //----- The good way to write a READ (load) sequence is in 2 times:
    00093     //-----     short_temp  =  Timer16_get_nnn_low();
    00094     //-----     short_temp |= (Timer16_get_nnn_high() << 8 );
    00095     //-----
    00096     //----- Otherwise a macro "Timer16_get_nnn()" exits and call "timer16_get_counter()" function
    00097
    00098 #ifndef USE_TIMER16
    00099 #       error You must define USE_TIMER16 to TIMER16_1 or TIMER16_3 or BOTH_TIMER16 in "config.h" file
    00100 #   elif (USE_TIMER16 == TIMER16_1)
    00101
    00102
    00103
    00104 #       define Timer16_select(timer16_num)     // Empty !
    00105     // ---------- Macros
    00106 #       define Timer16_clear()  ( TCCR1B=0, TCCR1A=0, TCCR1C=0, TCNT1H=0, TCNT1L= 0, OCR1AH=0, OCR1AL=0, \
    00107                                   OCR1BH=0, OCR1BL=0, OCR1CH=0, OCR1CL=0, ICR1H=0, ICR1L=0              )
    00108         // ----------
    00109 #       define Timer16_set_counter(value)       ( TCNT1H = ((U8)(value>>8)), TCNT1L = ((U8)(value)))
    00110 #       define Timer16_get_counter_low()        ((U16)(TCNT1L))
    00111 #       define Timer16_get_counter_high()       ((U16)(TCNT1H))
    00112         // ----------
    00113 #       define Timer16_set_compare_a(value)     ( OCR1AH = ((U8)(value>>8)), OCR1AL = ((U8)(value)))
    00114 #       define Timer16_set_compare_b(value)     ( OCR1BH = ((U8)(value>>8)), OCR1BL = ((U8)(value)))
    00115 #       define Timer16_set_compare_c(value)     ( OCR1CH = ((U8)(value>>8)), OCR1CL = ((U8)(value)))
    00116 #       define Timer16_get_compare_a()          ( OCR1A )      // The temporary register is not used
    00117 #       define Timer16_get_compare_b()          ( OCR1B )      // The temporary register is not used
    00118 #       define Timer16_get_compare_c()          ( OCR1C )      // The temporary register is not used
    00119         // ----------
    00120 #       define Timer16_set_capture(value)       { ICR1H = ((U8)(value>>8)); ICR1L = ((U8)(value)); }
    00121 #       define Timer16_get_capture_low()        ((U16)(ICR1L))
    00122 #       define Timer16_get_capture_high()       ((U16)(ICR1H))
    00123         // ----------
    00124 #       define Timer16_set_mode_output_a(conf)  ( TCCR1A = (TCCR1A & (~TIMER16_COMP_MODE_MASK_A)) | (conf << COM1A0) )
    00125 #       define Timer16_set_mode_output_b(conf)  ( TCCR1A = (TCCR1A & (~TIMER16_COMP_MODE_MASK_B)) | (conf << COM1B0) )
    00126 #       define Timer16_set_mode_output_c(conf)  ( TCCR1A = (TCCR1A & (~TIMER16_COMP_MODE_MASK_C)) | (conf << COM1C0) )
    00127 #       define Timer16_get_mode_output_a()      ((TCCR1A & TIMER16_COMP_MODE_MASK_A) >> COM1A0 )
    00128 #       define Timer16_get_mode_output_b()      ((TCCR1A & TIMER16_COMP_MODE_MASK_B) >> COM1B0 )
    00129 #       define Timer16_get_mode_output_c()      ((TCCR1A & TIMER16_COMP_MODE_MASK_C) >> COM1C0 )
    00130         // ----------
    00131 #       define Timer16_set_waveform_mode(conf)  ( TCCR1A = (TCCR1A & (~TIMER16_WGM_RA_MASK)) | ((conf &  0x3) << WGM10), \
    00132                                                   TCCR1B = (TCCR1B & (~TIMER16_WGM_RB_MASK)) | ((conf >> 0x2) << WGM12)  )
    00133 #       define Timer16_get_waveform_mode()     (((TCCR1A & TIMER16_WGM_RA_MASK) >> WGM10) |         \
    00134                                                (((TCCR1B & TIMER16_WGM_RB_MASK) >> WGM12) << 0x2)   )
    00135         // ----------
    00136 #       define Timer16_set_clock(value)        ( TCCR1B = (TCCR1B & (~TIMER16_CLK_MASK)) | (value << CS10) )
    00137 #       define Timer16_get_clock()            (((TCCR1B & TIMER16_CLK_MASK) >> CS10) )
    00138         // ----------
    00139 #       define Timer16_set_input_filter()      ( TCCR1B |=  (1<<ICNC1) )
    00140 #       define Timer16_clear_input_filter()    ( TCCR1B &= ~(1<<ICNC1) )
    00141 #       define Timer16_get_input_filter()      ((TCCR1B  &  (1<<ICNC1)) >> ICNC1 )
    00142     // ----------
    00143 #       define Timer16_set_input_rising_edge() ( TCCR1B |=  (1<<ICES1) )
    00144 #       define Timer16_set_input_falling_edge()( TCCR1B &= ~(1<<ICES1) )
    00145 #       define Timer16_get_input_capture_edge()((TCCR1B &   (1<<ICES1)) >> ICES1 )
    00146     // ----------
    00147 #       define Timer16_set_compare_force_a()   ( TCCR1C |=  (1<<FOC1A) )
    00148 #       define Timer16_set_compare_force_b()   ( TCCR1C |=  (1<<FOC1B) )
    00149 #       define Timer16_set_compare_force_c()   ( TCCR1C |=  (1<<FOC1C) )
    00150 #       define Timer16_clear_compare_force_a() ( TCCR1C &= ~(1<<FOC1A) )
    00151 #       define Timer16_clear_compare_force_b() ( TCCR1C &= ~(1<<FOC1B) )
    00152 #       define Timer16_clear_compare_force_c() ( TCCR1C &= ~(1<<FOC1C) )
    00153 #       define Timer16_get_compare_force_a()   ((TCCR1C  &  (1<<FOC1A)) >> FOC1A )
    00154 #       define Timer16_get_compare_force_b()   ((TCCR1C  &  (1<<FOC1B)) >> FOC1B )
    00155 #       define Timer16_get_compare_force_c()   ((TCCR1C  &  (1<<FOC1C)) >> FOC1C )
    00156     // ----------
    00157 #       define Timer16_overflow_it_enable()    ( TIMSK1 |=  (1<<TOIE1)  )
    00158 #       define Timer16_overflow_it_disable()   ( TIMSK1 &= ~(1<<TOIE1)  )
    00159 #       define Timer16_compare_a_it_enable()   ( TIMSK1 |=  (1<<OCIE1A) )
    00160 #       define Timer16_compare_a_it_disable()  ( TIMSK1 &= ~(1<<OCIE1A) )
    00161 #       define Timer16_compare_b_it_enable()   ( TIMSK1 |=  (1<<OCIE1B) )
    00162 #       define Timer16_compare_b_it_disable()  ( TIMSK1 &= ~(1<<OCIE1B) )
    00163 #       define Timer16_compare_c_it_enable()   ( TIMSK1 |=  (1<<OCIE1C) )
    00164 #       define Timer16_compare_c_it_disable()  ( TIMSK1 &= ~(1<<OCIE1C) )
    00165 #       define Timer16_capture_it_enable()     ( TIMSK1 |=  (1<<ICIE1)  )
    00166 #       define Timer16_capture_it_disable()    ( TIMSK1 &= ~(1<<ICIE1)  )
    00167 #       define Timer16_get_overflow_it_mask()  ((TIMSK1  &  (1<<TOIE1) ) >> TOIE1  )
    00168 #       define Timer16_get_compare_a_it_mask() ((TIMSK1  &  (1<<OCIE1A)) >> OCIE1A )
    00169 #       define Timer16_get_compare_b_it_mask() ((TIMSK1  &  (1<<OCIE1B)) >> OCIE1B )
    00170 #       define Timer16_get_compare_c_it_mask() ((TIMSK1  &  (1<<OCIE1C)) >> OCIE1C )
    00171 #       define Timer16_get_capture_it_mask()   ((TIMSK1  &  (1<<ICIE1) ) >> ICIE1  )
    00172     // ----------
    00173 #       define Timer16_clear_overflow_it()     ( TIFR1 |=  (1<<TOV1)  )
    00174 #       define Timer16_clear_compare_a_it()    ( TIFR1 |=  (1<<OCF1A) )
    00175 #       define Timer16_clear_compare_b_it()    ( TIFR1 |=  (1<<OCF1B) )
    00176 #       define Timer16_clear_compare_c_it()    ( TIFR1 |=  (1<<OCF1C) )
    00177 #       define Timer16_clear_capture_it()      ( TIFR1 |=  (1<<ICF1)  )
    00178 #       define Timer16_get_overflow_it()       ((TIFR1  &  (1<<TOV1) ) >> TOV1  )
    00179 #       define Timer16_get_compare_a_it()      ((TIFR1  &  (1<<OCF1A)) >> OCF1A )
    00180 #       define Timer16_get_compare_b_it()      ((TIFR1  &  (1<<OCF1B)) >> OCF1B )
    00181 #       define Timer16_get_compare_c_it()      ((TIFR1  &  (1<<OCF1C)) >> OCF1C )
    00182 #       define Timer16_get_capture_it()        ((TIFR1  &  (1<<ICF1) ) >> ICF1  )
    00183
    00184 #   elif USE_TIMER16 == TIMER16_3
    00185
    00186
    00187
    00188 #       define Timer16_select(timer16_num)     // Empty !
    00189     // ---------- Macros
    00190 #       define Timer16_clear()  { TCCR3B=0; TCCR3A=0; TCCR3C=0; TCNT3H=0; TCNT3L= 0; OCR3AH=0; OCR3AL=0; \
    00191                                   OCR3BH=0; OCR3BL=0; OCR3CH=0; OCR3CL=0; ICR3H=0, ICR3L=0;              }
    00192         // ----------
    00193 #       define Timer16_set_counter(value)       ( TCNT3H = ((U8)(value>>8)), TCNT3L = ((U8)(value)))
    00194 #       define Timer16_get_counter_low()        ((U16)(TCNT3L))
    00195 #       define Timer16_get_counter_high()       ((U16)(TCNT3H))
    00196         // ----------
    00197 #       define Timer16_set_compare_a(value)     { OCR3AH = ((U8)(value>>8)); OCR3AL = ((U8)(value)); }
    00198 #       define Timer16_set_compare_b(value)     { OCR3BH = ((U8)(value>>8)); OCR3BL = ((U8)(value)); }
    00199 #       define Timer16_set_compare_c(value)     { OCR3CH = ((U8)(value>>8)); OCR3CL = ((U8)(value)); }
    00200 #       define Timer16_get_compare_a()          ( OCR3A )      // The temporary register is not used
    00201 #       define Timer16_get_compare_b()          ( OCR3B )      // The temporary register is not used
    00202 #       define Timer16_get_compare_c()          ( OCR3C )      // The temporary register is not used
    00203         // ----------
    00204 #       define Timer16_set_capture(value)       { ICR3H = ((U8)(value>>8)); ICR3L = ((U8)(value)); }
    00205 #       define Timer16_get_capture_low()        ((U16)(ICR3L))
    00206 #       define Timer16_get_capture_high()       ((U16)(ICR3H))
    00207         // ----------
    00208 #       define Timer16_set_mode_output_a(conf)  ( TCCR3A = (TCCR3A & (~TIMER16_COMP_MODE_MASK_A)) | (conf << COM3A0) )
    00209 #       define Timer16_set_mode_output_b(conf)  ( TCCR3A = (TCCR3A & (~TIMER16_COMP_MODE_MASK_B)) | (conf << COM3B0) )
    00210 #       define Timer16_set_mode_output_c(conf)  ( TCCR3A = (TCCR3A & (~TIMER16_COMP_MODE_MASK_C)) | (conf << COM3C0) )
    00211 #       define Timer16_get_mode_output_a()      ((TCCR3A & TIMER16_COMP_MODE_MASK_A) >> COM3A0 )
    00212 #       define Timer16_get_mode_output_b()      ((TCCR3A & TIMER16_COMP_MODE_MASK_B) >> COM3B0 )
    00213 #       define Timer16_get_mode_output_c()      ((TCCR3A & TIMER16_COMP_MODE_MASK_C) >> COM3C0 )
    00214         // ----------
    00215 #       define Timer16_set_waveform_mode(conf)  ( TCCR3A = (TCCR3A & (~TIMER16_WGM_RA_MASK)) | ((conf &  0x3) << WGM30), \
    00216                                                   TCCR3B = (TCCR3B & (~TIMER16_WGM_RB_MASK)) | ((conf >> 0x2) << WGM32)  )
    00217 #       define Timer16_get_waveform_mode()     (((TCCR3A & TIMER16_WGM_RA_MASK) >> WGM30) |         \
    00218                                                (((TCCR3B & TIMER16_WGM_RB_MASK) >> WGM32) << 0x2)   )
    00219         // ----------
    00220 #       define Timer16_set_clock(value)        ( TCCR3B = (TCCR3B & (~TIMER16_CLK_MASK)) | (value << CS30) )
    00221 #       define Timer16_get_clock()            (((TCCR3B & TIMER16_CLK_MASK) >> CS30) )
    00222         // ----------
    00223 #       define Timer16_set_input_filter()      ( TCCR3B |=  (1<<ICNC3) )
    00224 #       define Timer16_clear_input_filter()    ( TCCR3B &= ~(1<<ICNC3) )
    00225 #       define Timer16_get_input_filter()      ((TCCR3B  &  (1<<ICNC3)) >> ICNC3 )
    00226     // ----------
    00227 #       define Timer16_set_input_rising_edge() ( TCCR3B |=  (1<<ICES3) )
    00228 #       define Timer16_set_input_falling_edge()( TCCR3B &= ~(1<<ICES3) )
    00229 #       define Timer16_get_input_capture_edge()((TCCR3B &   (1<<ICES3)) >> ICES3 )
    00230     // ----------
    00231 #       define Timer16_set_compare_force_a()   ( TCCR3C |=  (1<<FOC3A) )
    00232 #       define Timer16_set_compare_force_b()   ( TCCR3C |=  (1<<FOC3B) )
    00233 #       define Timer16_set_compare_force_c()   ( TCCR3C |=  (1<<FOC3C) )
    00234 #       define Timer16_clear_compare_force_a() ( TCCR3C &= ~(1<<FOC3A) )
    00235 #       define Timer16_clear_compare_force_b() ( TCCR3C &= ~(1<<FOC3B) )
    00236 #       define Timer16_clear_compare_force_c() ( TCCR3C &= ~(1<<FOC3C) )
    00237 #       define Timer16_get_compare_force_a()   ((TCCR3C  &  (1<<FOC3A)) >> FOC3A )
    00238 #       define Timer16_get_compare_force_b()   ((TCCR3C  &  (1<<FOC3B)) >> FOC3B )
    00239 #       define Timer16_get_compare_force_c()   ((TCCR3C  &  (1<<FOC3C)) >> FOC3C )
    00240     // ----------
    00241 #       define Timer16_overflow_it_enable()    ( TIMSK3 |=  (1<<TOIE3)  )
    00242 #       define Timer16_overflow_it_disable()   ( TIMSK3 &= ~(1<<TOIE3)  )
    00243 #       define Timer16_compare_a_it_enable()   ( TIMSK3 |=  (1<<OCIE3A) )
    00244 #       define Timer16_compare_a_it_disable()  ( TIMSK3 &= ~(1<<OCIE3A) )
    00245 #       define Timer16_compare_b_it_enable()   ( TIMSK3 |=  (1<<OCIE3B) )
    00246 #       define Timer16_compare_b_it_disable()  ( TIMSK3 &= ~(1<<OCIE3B) )
    00247 #       define Timer16_compare_c_it_enable()   ( TIMSK3 |=  (1<<OCIE3C) )
    00248 #       define Timer16_compare_c_it_disable()  ( TIMSK3 &= ~(1<<OCIE3C) )
    00249 #       define Timer16_capture_it_enable()     ( TIMSK3 |=  (1<<ICIE3)  )
    00250 #       define Timer16_capture_it_disable()    ( TIMSK3 &= ~(1<<ICIE3)  )
    00251 #       define Timer16_get_overflow_it_mask()  ((TIMSK3  &  (1<<TOIE3) ) >> TOIE3  )
    00252 #       define Timer16_get_compare_a_it_mask() ((TIMSK3  &  (1<<OCIE3A)) >> OCIE3A )
    00253 #       define Timer16_get_compare_b_it_mask() ((TIMSK3  &  (1<<OCIE3B)) >> OCIE3B )
    00254 #       define Timer16_get_compare_c_it_mask() ((TIMSK3  &  (1<<OCIE3C)) >> OCIE3C )
    00255 #       define Timer16_get_capture_it_mask()   ((TIMSK3  &  (1<<ICIE3) ) >> ICIE3  )
    00256     // ----------
    00257 #       define Timer16_clear_overflow_it()     ( TIFR3 |=  (1<<TOV3)  )
    00258 #       define Timer16_clear_compare_a_it()    ( TIFR3 |=  (1<<OCF3A) )
    00259 #       define Timer16_clear_compare_b_it()    ( TIFR3 |=  (1<<OCF3B) )
    00260 #       define Timer16_clear_compare_c_it()    ( TIFR3 |=  (1<<OCF3C) )
    00261 #       define Timer16_clear_capture_it()      ( TIFR3 |=  (1<<ICF3)  )
    00262 #       define Timer16_get_overflow_it()       ((TIFR3  &  (1<<TOV3) ) >> TOV3  )
    00263 #       define Timer16_get_compare_a_it()      ((TIFR3  &  (1<<OCF3A)) >> OCF3A )
    00264 #       define Timer16_get_compare_b_it()      ((TIFR3  &  (1<<OCF3B)) >> OCF3B )
    00265 #       define Timer16_get_compare_c_it()      ((TIFR3  &  (1<<OCF3C)) >> OCF3C )
    00266 #       define Timer16_get_capture_it()        ((TIFR3  &  (1<<ICF3) ) >> ICF3  )
    00267
    00268 #   elif USE_TIMER16 == BOTH_TIMER16
    00269
    00270
    00271
    00272         extern U8 timer16_selected;         // $$$-- EXTERNAL DECLARATION --$$$
    00273 #       define Timer16_select(timer16_num)     (timer16_selected=timer16_num)
    00274     // ---------- Macros
    00275 #       define Timer16_clear()              ((timer16_selected==TIMER16_1)? \
    00276                                                 (TCCR1B=0, TCCR1A=0, TCCR1C=0, TCNT1H=0, TCNT1L= 0, OCR1AH=0, OCR1AL=0, \
    00277                                                  OCR1BH=0, OCR1BL=0, OCR1CH=0, OCR1CL=0, ICR1H=0, ICR1L=0 )             \
    00278                                                 : \
    00279                                                 (TCCR3B=0, TCCR3A=0, TCCR3C=0, TCNT3H=0, TCNT3L= 0, OCR3AH=0, OCR3AL=0, \
    00280                                                  OCR3BH=0, OCR3BL=0, OCR3CH=0, OCR3CL=0, ICR3H=0, ICR3L=0 )             )
    00281         // ----------
    00282 #       define Timer16_set_counter(value)   ((timer16_selected==TIMER16_1)? \
    00283                                                 (TCNT1H = ((U8)(value>>8)), TCNT1L = ((U8)(value)) ) \
    00284                                                 : \
    00285                                                 (TCNT3H = ((U8)(value>>8)), TCNT3L = ((U8)(value)) ) )
    00286 #       define Timer16_get_counter_low()    ((timer16_selected==TIMER16_1)? ((U16)(TCNT1L)) : ((U16)(TCNT3L)) )
    00287 #       define Timer16_get_counter_high()   ((timer16_selected==TIMER16_1)? ((U16)(TCNT1H)) : ((U16)(TCNT3H)) )
    00288         // ----------
    00289 #       define Timer16_set_compare_a(value) ((timer16_selected==TIMER16_1)? \
    00290                                                 (OCR1AH = ((U8)(value>>8)), OCR1AL = ((U8)(value)) ) \
    00291                                                 : \
    00292                                                 (OCR3AH = ((U8)(value>>8)), OCR3AL = ((U8)(value)) ) )
    00293 #       define Timer16_set_compare_b(value) ((timer16_selected==TIMER16_1)? \
    00294                                                 (OCR1BH = ((U8)(value>>8)), OCR1BL = ((U8)(value)) ) \
    00295                                                 : \
    00296                                                 (OCR3BH = ((U8)(value>>8)), OCR3BL = ((U8)(value)) ) )
    00297 #       define Timer16_set_compare_c(value) ((timer16_selected==TIMER16_1)? \
    00298                                                 (OCR3CH = ((U8)(value>>8)), OCR3CL = ((U8)(value)) ) \
    00299                                                 : \
    00300                                                 (OCR1CH = ((U8)(value>>8)), OCR1CL = ((U8)(value)) ) )
    00301 #       define Timer16_get_compare_a()      ((timer16_selected==TIMER16_1)? (OCR1A) : (OCR3A) )   // The temporary register is not used
    00302 #       define Timer16_get_compare_b()      ((timer16_selected==TIMER16_1)? (OCR1B) : (OCR3B) )   // The temporary register is not used
    00303 #       define Timer16_get_compare_c()      ((timer16_selected==TIMER16_1)? (OCR1C) : (OCR3C) )   // The temporary register is not used
    00304         // ----------
    00305 #       define Timer16_set_capture(value)   ((timer16_selected==TIMER16_1)? \
    00306                                                 (ICR1H = ((U8)(value>>8)), ICR1L = ((U8)(value))) \
    00307                                                 : \
    00308                                                 (ICR3H = ((U8)(value>>8)), ICR3L = ((U8)(value))) )
    00309 #       define Timer16_get_capture_low()    ((timer16_selected==TIMER16_1)? ((U16)(ICR1L)) : ((U16)(ICR3L)) )
    00310 #       define Timer16_get_capture_high()   ((timer16_selected==TIMER16_1)? ((U16)(ICR1H)) : ((U16)(ICR3H)) )
    00311         // ----------
    00312 #       define Timer16_set_mode_output_a(conf)  ((timer16_selected==TIMER16_1)? \
    00313                                                     (TCCR1A = (TCCR1A & (~TIMER16_COMP_MODE_MASK_A)) | (conf << COM1A0)) \
    00314                                                     : \
    00315                                                     (TCCR3A = (TCCR3A & (~TIMER16_COMP_MODE_MASK_A)) | (conf << COM3A0)) )
    00316 #       define Timer16_set_mode_output_b(conf)  ((timer16_selected==TIMER16_1)? \
    00317                                                     (TCCR1A = (TCCR1A & (~TIMER16_COMP_MODE_MASK_B)) | (conf << COM1B0)) \
    00318                                                     : \
    00319                                                     (TCCR3A = (TCCR3A & (~TIMER16_COMP_MODE_MASK_B)) | (conf << COM3B0)) )
    00320 #       define Timer16_set_mode_output_c(conf)  ((timer16_selected==TIMER16_1)? \
    00321                                                     (TCCR1A = (TCCR1A & (~TIMER16_COMP_MODE_MASK_C)) | (conf << COM1C0)) \
    00322                                                     : \
    00323                                                     (TCCR3A = (TCCR3A & (~TIMER16_COMP_MODE_MASK_C)) | (conf << COM3C0)) )
    00324 #       define Timer16_get_mode_output_a()   ((timer16_selected==TIMER16_1)? \
    00325                                                 ((TCCR1A & TIMER16_COMP_MODE_MASK_A) >> COM1A0) : ((TCCR3A & TIMER16_COMP_MODE_MASK_A) >> COM3A0 ) )
    00326 #       define Timer16_get_mode_output_b()   ((timer16_selected==TIMER16_1)? \
    00327                                                 ((TCCR1A & TIMER16_COMP_MODE_MASK_B) >> COM1B0) : ((TCCR3A & TIMER16_COMP_MODE_MASK_B) >> COM3B0) )
    00328 #       define Timer16_get_mode_output_c()   ((timer16_selected==TIMER16_1)? \
    00329                                                 ((TCCR1A & TIMER16_COMP_MODE_MASK_C) >> COM1C0) : ((TCCR3A & TIMER16_COMP_MODE_MASK_C) >> COM3C0) )
    00330         // ----------
    00331 #       define Timer16_set_waveform_mode(conf)  ((timer16_selected==TIMER16_1)? \
    00332                                                     (TCCR1A = (TCCR1A & (~TIMER16_WGM_RA_MASK)) | ((conf &  0x3) << WGM10) , \
    00333                                                      TCCR1B = (TCCR1B & (~TIMER16_WGM_RB_MASK)) | ((conf >> 0x2) << WGM12) ) \
    00334                                                      : \
    00335                                                     (TCCR3A = (TCCR3A & (~TIMER16_WGM_RA_MASK)) | ((conf &  0x3) << WGM30) , \
    00336                                                      TCCR3B = (TCCR3B & (~TIMER16_WGM_RB_MASK)) | ((conf >> 0x2) << WGM32) ) )
    00337 #       define Timer16_get_waveform_mode()   ((timer16_selected==TIMER16_1)? \
    00338                                                 (((TCCR1A & TIMER16_WGM_RA_MASK) >> WGM10) | (((TCCR1B & TIMER16_WGM_RB_MASK) >> WGM12) << 0x2)) \
    00339                                                 : \
    00340                                                 (((TCCR3A & TIMER16_WGM_RA_MASK) >> WGM30) | (((TCCR3B & TIMER16_WGM_RB_MASK) >> WGM32) << 0x2)) )
    00341         // ----------
    00342 #       define Timer16_set_clock(value)      ((timer16_selected==TIMER16_1)? \
    00343                                                 (TCCR1B = (TCCR1B & (~TIMER16_CLK_MASK)) | (value << CS10)) \
    00344                                                 : \
    00345                                                 (TCCR3B = (TCCR3B & (~TIMER16_CLK_MASK)) | (value << CS30)) )
    00346
    00347 #       define Timer16_get_clock()           ((timer16_selected==TIMER16_1)? \
    00348                                                 (((TCCR1B & TIMER16_CLK_MASK) >> CS10)) : (((TCCR3B & TIMER16_CLK_MASK) >> CS30)) )
    00349         // ----------
    00350 #       define Timer16_set_input_filter()    ((timer16_selected==TIMER16_1)? \
    00351                                                 (TCCR1B |= (1<<ICNC1)) : ( TCCR3B |= (1<<ICNC3)) )
    00352 #       define Timer16_clear_input_filter()  ((timer16_selected==TIMER16_1)? \
    00353                                                 (TCCR1B &= ~(1<<ICNC1)) :  ( TCCR3B &= ~(1<<ICNC3)) )
    00354 #       define Timer16_get_input_filter()    ((timer16_selected==TIMER16_1)? \
    00355                                                 ((TCCR1B & (1<<ICNC1)) >> ICNC1) : ((TCCR3B & (1<<ICNC3)) >> ICNC3) )
    00356     // ----------
    00357 #       define Timer16_set_input_rising_edge()  ((timer16_selected==TIMER16_1)? \
    00358                                                     (TCCR1B |= (1<<ICES1)) : (TCCR3B |= (1<<ICES3)) )
    00359 #       define Timer16_set_input_falling_edge() ((timer16_selected==TIMER16_1)? \
    00360                                                     (TCCR1B &= ~(1<<ICES1)) : ( TCCR3B &= ~(1<<ICES3)) )
    00361 #       define Timer16_get_input_capture_edge() ((timer16_selected==TIMER16_1)? \
    00362                                                     ((TCCR1B & (1<<ICES1)) >> ICES1) : ((TCCR3B & (1<<ICES3)) >> ICES3) )
    00363     // ----------
    00364 #       define Timer16_set_compare_force_a()    ((timer16_selected==TIMER16_1)? \
    00365                                                     (TCCR1C |= (1<<FOC1A)) : (TCCR3C |= (1<<FOC3A)) )
    00366 #       define Timer16_set_compare_force_b()    ((timer16_selected==TIMER16_1)? \
    00367                                                     (TCCR1C |= (1<<FOC1B)) : (TCCR3C |= (1<<FOC3B)) )
    00368 #       define Timer16_set_compare_force_c()    ((timer16_selected==TIMER16_1)? \
    00369                                                     (TCCR1C |= (1<<FOC1C)) : (TCCR3C |= (1<<FOC3C)) )
    00370 #       define Timer16_clear_compare_force_a()  ((timer16_selected==TIMER16_1)? \
    00371                                                     (TCCR1C &= ~(1<<FOC1A ) : (TCCR3C &= ~(1<<FOC3A)) )
    00372 #       define Timer16_clear_compare_force_b()  ((timer16_selected==TIMER16_1)? \
    00373                                                     (TCCR1C &= ~(1<<FOC1B)) : (TCCR3C &= ~(1<<FOC3B)) )
    00374 #       define Timer16_clear_compare_force_c()  ((timer16_selected==TIMER16_1)? \
    00375                                                     (TCCR1C &= ~(1<<FOC1C)) : (TCCR3C &= ~(1<<FOC3C)) )
    00376 #       define Timer16_get_compare_force_a()    ((timer16_selected==TIMER16_1)? \
    00377                                                     ((TCCR1C & (1<<FOC1A)) >> FOC1A) : ((TCCR3C & (1<<FOC3A)) >> FOC3A) )
    00378 #       define Timer16_get_compare_force_b()    ((timer16_selected==TIMER16_1)? \
    00379                                                     ((TCCR1C & (1<<FOC1B)) >> FOC1B) : ((TCCR3C & (1<<FOC3B)) >> FOC3B) )
    00380 #       define Timer16_get_compare_force_c()    ((timer16_selected==TIMER16_1)? \
    00381                                                     ((TCCR1C & (1<<FOC1C)) >> FOC1C) : ((TCCR3C & (1<<FOC3C)) >> FOC3C) )
    00382     // ----------
    00383 #       define Timer16_overflow_it_enable()     ((timer16_selected==TIMER16_1)? \
    00384                                                     (TIMSK1 |= (1<<TOIE1)) : (TIMSK3 |= (1<<TOIE3)) )
    00385 #       define Timer16_overflow_it_disable()    ((timer16_selected==TIMER16_1)? \
    00386                                                     (TIMSK1 &= ~(1<<TOIE1)) : (TIMSK3 &= ~(1<<TOIE3)) )
    00387 #       define Timer16_compare_a_it_enable()    ((timer16_selected==TIMER16_1)? \
    00388                                                     (TIMSK1 |= (1<<OCIE1A)) : (TIMSK3 |= (1<<OCIE3A)) )
    00389 #       define Timer16_compare_a_it_disable()   ((timer16_selected==TIMER16_1)? \
    00390                                                     (TIMSK1 &= ~(1<<OCIE1A)) : (TIMSK3 &= ~(1<<OCIE3A)) )
    00391 #       define Timer16_compare_b_it_enable()    ((timer16_selected==TIMER16_1)? \
    00392                                                     (TIMSK1 |= (1<<OCIE1B)) : (TIMSK3 |= (1<<OCIE3B)) )
    00393 #       define Timer16_compare_b_it_disable()   ((timer16_selected==TIMER16_1)? \
    00394                                                     (TIMSK1 &= ~(1<<OCIE1B)) : (TIMSK3 &= ~(1<<OCIE3B)) )
    00395 #       define Timer16_compare_c_it_enable()    ((timer16_selected==TIMER16_1)? \
    00396                                                     (TIMSK1 |= (1<<OCIE1C)) : (TIMSK3 |= (1<<OCIE3C)) )
    00397 #       define Timer16_compare_c_it_disable()   ((timer16_selected==TIMER16_1)? \
    00398                                                     (TIMSK1 &= ~(1<<OCIE1C)) : (TIMSK3 &= ~(1<<OCIE3C)) )
    00399 #       define Timer16_capture_it_enable()      ((timer16_selected==TIMER16_1)? \
    00400                                                     (TIMSK1 |= (1<<ICIE1)) : (TIMSK3 |= (1<<ICIE3)) )
    00401 #       define Timer16_capture_it_disable()     ((timer16_selected==TIMER16_1)? \
    00402                                                     (TIMSK1 &= ~(1<<ICIE1)) : (TIMSK3 &= ~(1<<ICIE3)) )
    00403 #       define Timer16_get_overflow_it_mask()   ((timer16_selected==TIMER16_1)? \
    00404                                                     ((TIMSK1 & (1<<TOIE1)) >> TOIE1) : ((TIMSK3 & (1<<TOIE3)) >> TOIE3) )
    00405 #       define Timer16_get_compare_a_it_mask()  ((timer16_selected==TIMER16_1)? \
    00406                                                     ((TIMSK1 & (1<<OCIE1A)) >> OCIE1A) : ((TIMSK3 & (1<<OCIE3A)) >> OCIE3A) )
    00407 #       define Timer16_get_compare_b_it_mask()  ((timer16_selected==TIMER16_1)? \
    00408                                                     ((TIMSK1 & (1<<OCIE1B)) >> OCIE1B) : ((TIMSK3 & (1<<OCIE3B)) >> OCIE3B) )
    00409 #       define Timer16_get_compare_c_it_mask()  ((timer16_selected==TIMER16_1)? \
    00410                                                     ((TIMSK1 & (1<<OCIE1C)) >> OCIE1C) : ((TIMSK3 & (1<<OCIE3C)) >> OCIE3C) )
    00411 #       define Timer16_get_capture_it_mask()    ((timer16_selected==TIMER16_1)? \
    00412                                                     ((TIMSK1 & (1<<ICIE1)) >> ICIE1) : ((TIMSK3 & (1<<ICIE3)) >> ICIE3) )
    00413     // ----------
    00414 #       define Timer16_clear_overflow_it()      ((timer16_selected==TIMER16_1)? \
    00415                                                     (TIFR1 |= (1<<TOV1)) : (TIFR3 |= (1<<TOV3)) )
    00416 #       define Timer16_clear_compare_a_it()     ((timer16_selected==TIMER16_1)? \
    00417                                                     (TIFR1 |= (1<<OCF1A)) : (TIFR3 |= (1<<OCF3A)) )
    00418 #       define Timer16_clear_compare_b_it()     ((timer16_selected==TIMER16_1)? \
    00419                                                     (TIFR1 |= (1<<OCF1B)) : (TIFR3 |= (1<<OCF3B)) )
    00420 #       define Timer16_clear_compare_c_it()     ((timer16_selected==TIMER16_1)? \
    00421                                                     (TIFR1 |= (1<<OCF1C)) : (TIFR3 |= (1<<OCF3C)) )
    00422 #       define Timer16_clear_capture_it()       ((timer16_selected==TIMER16_1)? \
    00423                                                     (TIFR1 |= (1<<ICF1)) : (TIFR3 |= (1<<ICF3)) )
    00424 #       define Timer16_get_overflow_it()        ((timer16_selected==TIMER16_1)? \
    00425                                                     ((TIFR1 & (1<<TOV1)) >> TOV1) : ((TIFR3 & (1<<TOV3)) >> TOV3) )
    00426 #       define Timer16_get_compare_a_it()       ((timer16_selected==TIMER16_1)? \
    00427                                                     ((TIFR1 & (1<<OCF1A)) >> OCF1A) : ((TIFR3 & (1<<OCF3A)) >> OCF3A) )
    00428 #       define Timer16_get_compare_b_it()       ((timer16_selected==TIMER16_1)? \
    00429                                                     ((TIFR1 & (1<<OCF1B)) >> OCF1B) : ((TIFR3 & (1<<OCF3B)) >> OCF3B) )
    00430 #       define Timer16_get_compare_c_it()       ((timer16_selected==TIMER16_1)? \
    00431                                                     ((TIFR1 & (1<<OCF1C)) >> OCF1C) : ((TIFR3 & (1<<OCF3C)) >> OCF3C) )
    00432 #       define Timer16_get_capture_it()         ((timer16_selected==TIMER16_1)? \
    00433                                                     ((TIFR1 & (1<<ICF1)) >> ICF1) : ((TIFR3 & (1<<ICF3)) >> ICF3) )
    00434
    00435     #else
    00436         #error USE_TIMER16 definition is not referenced in "timer16_drv.h" file
    00437 #endif
    00438
    00439 //_____ T I M E R   D E F I N I T I O N S ______________________________________
    00440
    00441     // ---------- Pre-definitions for "conf" field for Timer16_set(get)_mode_output_x(conf) macros
    00442 #define TIMER16_COMP_MODE_NORMAL    (0)
    00443 #define TIMER16_COMP_MODE_TOGGLE    (1)
    00444 #define TIMER16_COMP_MODE_CLEAR_OC  (2)
    00445 #define TIMER16_COMP_MODE_SET_OC    (3)
    00446 #define TIMER16_COMP_MODE_MASK_A    (3<<COM1A0)
    00447 #define TIMER16_COMP_MODE_MASK_B    (3<<COM1B0)
    00448 #define TIMER16_COMP_MODE_MASK_C    (3<<COM1C0)
    00449     // ---------- Pre-definitions for "conf" field for Timer16_set_waveform_mode(conf) macro
    00450 #define TIMER16_WGM_NORMAL          (0)
    00451 #define TIMER16_WGM_CTC_OCR         (4)
    00452 #define TIMER16_WGM_CTC_ICR         (12)
    00453 #define TIMER16_WGM_PWM_PC8         (1)
    00454 #define TIMER16_WGM_PWM_PC9         (2)
    00455 #define TIMER16_WGM_PWM_PC10        (3)
    00456 #define TIMER16_WGM_PWM_PC_ICR      (10)
    00457 #define TIMER16_WGM_PWM_PC_OCR      (11)
    00458 #define TIMER16_WGM_PWM_PFC_ICR     (8)
    00459 #define TIMER16_WGM_PWM_PFC_OCR     (9)
    00460 #define TIMER16_WGM_FAST_PWM8       (5)
    00461 #define TIMER16_WGM_FAST_PWM9       (6)
    00462 #define TIMER16_WGM_FAST_PWM10      (7)
    00463 #define TIMER16_WGM_FAST_PWM_ICR    (14)
    00464 #define TIMER16_WGM_FAST_PWM_OCR    (15)
    00465 #define TIMER16_WGM_RA_MASK         (3<<WGM10)
    00466 #define TIMER16_WGM_RB_MASK         (3<<WGM12)
    00467     // ---------- Pre-definitions for "value" field for Timer16_set_clock(value) macro
    00468 #define TIMER16_NO_CLOCK                 (0)
    00469 #define TIMER16_CLKIO_BY_1               (1)
    00470 #define TIMER16_CLKIO_BY_8               (2)
    00471 #define TIMER16_CLKIO_BY_64              (3)
    00472 #define TIMER16_CLKIO_BY_256             (4)
    00473 #define TIMER16_CLKIO_BY_1024            (5)
    00474 #define TIMER16_EXT_CLOCK_FALLING_EDGE   (6)
    00475 #define TIMER16_EXT_CLOCK_RISING_EDGE    (7)
    00476 #define TIMER16_CLK_MASK                 (7<<CS10)
    00477
    00478
    00479 //_____ D E C L A R A T I O N S ________________________________________________
    00480
    00481 //------------------------------------------------------------------------------
    00482 //  @fn timer16_get_counter
    00492 extern  U16 timer16_get_counter(void);
    00493
    00494 //------------------------------------------------------------------------------
    00495 //  @fn timer16_get_capture
    00505 extern  U16 timer16_get_capture(void);
    00506
    00507 //______________________________________________________________________________
    00508
    00509 #endif  // _TIMER16_DRV_H_
    00510
    00511
    00512
    00513
    00514
    00515
    00516
    00517
    00518
    00519
    00520
    00521
    00522
    00523
    00524
    00525
    00526
    00527
    00528
    00529
    00530
    00531
    00532
    00533
    00534
    00535
    00536
    00537
    00538
    00539