- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# ctrl_status.h File Reference

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Enumerations
enum | Ctrl_status { CTRL_GOOD = (PASS ), CTRL_FAIL = (FAIL ), CTRL_NO_PRESENT = (FAIL+1), CTRL_BUSY = (FAIL+2) }
| Define control status. More...

## Detailed Description

This file contains the interface : - between USB <-> MEMORY OR

- between USB <- Access Memory Ctrl -> Memory This interface may be controled by a "Access Memory Control" for :
- include a management of write protect global or specific
- include a management of access password
- ...

- Compiler: IAR EWAVR and GNU GCC for AVR
- Supported devices: AT90USB1287, AT90USB1286, AT90USB647, AT90USB646

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file ctrl_status.h.

## Enumeration Type Documentation

enum Ctrl_status

Define control status.

Enumerator:

  CTRL_GOOD |
  CTRL_FAIL |
  CTRL_NO_PRESENT |
  CTRL_BUSY |

Definition at line 56 of file ctrl_status.h.

    00057 {
    00058    CTRL_GOOD         =(PASS  )  // It is ready
    00059 ,  CTRL_FAIL         =(FAIL  )  // Memory fail
    00060 ,  CTRL_NO_PRESENT   =(FAIL+1)  // Memory unplug
    00061 ,  CTRL_BUSY         =(FAIL+2)  // Not initialize
    00062 } Ctrl_status;