- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# usb_commun.h File Reference

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Defines
Vendor Identifiant according by USB org to ATMEL
#define | VID_ATMEL 0x03EB
Product Identifiant according by ATMEL
#define | PID_MegaHIDGeneric 0x2013
#define | PID_MegaHIDKeyboard 0x2017
#define | PID_MegaCDC 0x2018
#define | PID_MegaAUDIO_IN 0x2019
#define | PID_MegaMS 0x201A
#define | PID_MegaAUDIO_IN_OUT 0x201B
#define | PID_MegaHIDMouse 0x201C
#define | PID_MegaHIDMouse_certif_U4 0x201D
#define | PID_MegaCDC_multi 0x201E
#define | PID_AT90USB128_64_MS_HIDMS_HID_USBKEY 0x2022
#define | PID_AT90USB128_64_MS_HIDMS_HID_STK525 0x2023
#define | PID_AT90USB128_64_MS 0x2029
#define | PID_Mega_MS_HIDMS 0x202A
#define | PID_MegaMS_2 0x2032
#define | PID_MegaLibUsb 0x2050
#define | PID_ATMega8U2_DFU 0x2FEE
#define | PID_ATMega16U2_DFU 0x2FEF
#define | PID_ATMega32U2_DFU 0x2FF0
#define | PID_ATMega32U6_DFU 0x2FF2
#define | PID_ATMega16U4_DFU 0x2FF3
#define | PID_ATMega32U4_DFU 0x2FF4
#define | PID_AT90USB82_DFU 0x2FF7
#define | PID_AT90USB64_DFU 0x2FF9
#define | PID_AT90USB162_DFU 0x2FFA
#define | PID_AT90USB128_DFU 0x2FFB
Global Class, SubClass & Protocol constants
#define | CLASS_APPLICATION 0xFE
| Use to declare a specific interface link at VID-PID.
#define | CLASS_VENDOR 0xFF
| Use to declare a specific interface link at VID-PID.
#define | NO_CLASS 0x00
#define | NO_SUBCLASS 0x00
#define | NO_PROTOCOL 0x00
IAD Interface Association Descriptor constants
#define | CLASS_IAD 0xEF
#define | SUB_CLASS_IAD 0x02
#define | PROTOCOL_IAD 0x01
Status constant of device
Bit 0 Self Powered Bit 1 Remote Wakeup Bit 2 Battery Powered
#define | USB_DEVICE_STATUS_BUS_POWERED 0x00
#define | USB_DEVICE_STATUS_SELF_POWERED 0x01
#define | USB_DEVICE_STATUS_REMOTEWAKEUP 0x02
#define | USB_DEVICE_STATUS_BATTERYPOWERED 0x04
Attribut constant of status device
#define | USB_CONFIG_ATTRIBUTES_RESERVED 0x80
#define | USB_CONFIG_ATTRIBUTES_REMOTEWAKEUP 0x20
#define | USB_CONFIG_ATTRIBUTES_SELFPOWERED 0x40
#define | USB_CONFIG_BUSPOWERED (USB_CONFIG_ATTRIBUTES_RESERVED)
#define | USB_CONFIG_REMOTEWAKEUP (USB_CONFIG_ATTRIBUTES_RESERVED | USB_CONFIG_ATTRIBUTES_REMOTEWAKEUP)
#define | USB_CONFIG_SELFPOWERED (USB_CONFIG_ATTRIBUTES_RESERVED | USB_CONFIG_ATTRIBUTES_SELFPOWERED)
Constants used in Endpoint Descriptor
#define | USB_ENDPOINT_BULK 0x02
#define | USB_ENDPOINT_INTERRUPT 0x03
#define | USB_ENDPOINT_OUT 0x00
#define | USB_ENDPOINT_IN 0x80
#define | USB_ENDPOINT_DIR_MASK 0x80
#define | USB_ENDPOINT_NUM_MASK (~USB_ENDPOINT_DIR_MASK)
Data transfer direction
bit 7, 0 = Host to device 1 = Device to host
#define | USB_SETUP_DIR_HOST_TO_DEVICE (0<<7)
#define | USB_SETUP_DIR_DEVICE_TO_HOST (1<<7)
Type
bit 6 to 5, 0 = Standard 1 = Class 2 = Vendor 3 = Reserved
#define | USB_SETUP_TYPE_STANDARD (0<<5)
#define | USB_SETUP_TYPE_CLASS (1<<5)
#define | USB_SETUP_TYPE_VENDOR (2<<5)
Recipient
bit 4 to 0, 0 = device 1 = Interface 2 = Endpoint 3 = Other 4. ..31 = Reserved
#define | USB_SETUP_RECIPIENT_DEVICE (0)
#define | USB_SETUP_RECIPIENT_INTERFACE (1)
#define | USB_SETUP_RECIPIENT_ENDPOINT (2)
#define | USB_SETUP_RECIPIENT_OTHER (3)
Request type used by standard setup request
#define | USB_SETUP_SET_STAND_DEVICE (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_DEVICE)
#define | USB_SETUP_GET_STAND_DEVICE (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_DEVICE)
#define | USB_SETUP_SET_STAND_INTERFACE (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_INTERFACE)
#define | USB_SETUP_GET_STAND_INTERFACE (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_INTERFACE)
#define | USB_SETUP_SET_STAND_ENDPOINT (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_ENDPOINT)
#define | USB_SETUP_GET_STAND_ENDPOINT (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_ENDPOINT)
Request type used by specific setup request from class driver
#define | USB_SETUP_SET_CLASS_DEVICE (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_DEVICE)
#define | USB_SETUP_GET_CLASS_DEVICE (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_DEVICE)
#define | USB_SETUP_SET_CLASS_INTER (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_INTERFACE)
#define | USB_SETUP_GET_CLASS_INTER (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_INTERFACE)
#define | USB_SETUP_SET_CLASS_ENDPOINT (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_ENDPOINT)
#define | USB_SETUP_GET_CLASS_ENDPOINT (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_ENDPOINT)
#define | USB_SETUP_SET_CLASS_OTHER (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_OTHER)
#define | USB_SETUP_GET_CLASS_OTHER (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_OTHER)
#define | USB_SETUP_SET_VENDOR_DEVICE (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_VENDOR |USB_SETUP_RECIPIENT_DEVICE)
#define | USB_SETUP_GET_VENDOR_DEVICE (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_VENDOR |USB_SETUP_RECIPIENT_DEVICE)
Standard Requests (bRequest)
#define | SETUP_GET_STATUS 0x00
#define | SETUP_GET_DEVICE 0x01
#define | SETUP_CLEAR_FEATURE 0x01
#define | SETUP_GET_STRING 0x03
#define | SETUP_SET_FEATURE 0x03
#define | SETUP_SET_ADDRESS 0x05
#define | SETUP_GET_DESCRIPTOR 0x06
#define | SETUP_SET_DESCRIPTOR 0x07
#define | SETUP_GET_CONFIGURATION 0x08
#define | SETUP_SET_CONFIGURATION 0x09
#define | SETUP_GET_INTERFACE 0x0A
#define | SETUP_SET_INTERFACE 0x0B
#define | SETUP_SYNCH_FRAME 0x0C
Descriptor types used in several setup requests
#define | DESCRIPTOR_DEVICE 0x01
#define | DESCRIPTOR_CONFIGURATION 0x02
#define | DESCRIPTOR_STRING 0x03
#define | DESCRIPTOR_INTERFACE 0x04
#define | DESCRIPTOR_ENDPOINT 0x05
#define | DESCRIPTOR_DEVICE_QUALIFIER 0x06
#define | DESCRIPTOR_CONF_OTHER_SPEED 0x07
#define | DESCRIPTOR_OTG 0x09
#define | DESCRIPTOR_IAD 0x0B
Feature types for SETUP_X_FEATURE standard request
#define | FEATURE_DEVICE_REMOTE_WAKEUP 0x01
#define | FEATURE_DEVICE_TEST 0x02
#define | FEATURE_DEVICE_OTG_B_HNP_ENABLE 0x03
#define | FEATURE_DEVICE_OTG_A_HNP_SUPPORT 0x04
#define | FEATURE_DEVICE_OTG_A_ALT_HNP_SUPPORT 0x05
#define | FEATURE_ENDPOINT_HALT 0x00
Feature types for SETUP_X_FEATURE standard test request
#define | FEATURE_DEVICE_TEST_J 0x01
#define | FEATURE_DEVICE_TEST_K 0x02
#define | FEATURE_DEVICE_TEST_SEO_NAK 0x03
#define | FEATURE_DEVICE_TEST_PACKET 0x04
#define | FEATURE_DEVICE_TEST_FORCE_ENABLE 0x05
OTG descriptor (see OTG_BMATTRIBUTES)
#define | DESCRIPTOR_OTG_bLength 0x03
#define | HNP_SUPPORT 0x02
#define | SRP_SUPPORT 0x01

## Detailed Description

This file contains the usb definition constant parameters from USB V2.0 - Compiler: IAR EWAVR and GNU GCC for AVR

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file usb_commun.h.

## Define Documentation

#define VID_ATMEL 0x03EB

Definition at line 44 of file usb_commun.h.

#define PID_MegaHIDGeneric 0x2013

Definition at line 49 of file usb_commun.h.

#define PID_MegaHIDKeyboard 0x2017

Definition at line 50 of file usb_commun.h.

#define PID_MegaCDC 0x2018

Definition at line 51 of file usb_commun.h.

#define PID_MegaAUDIO_IN 0x2019

Definition at line 52 of file usb_commun.h.

#define PID_MegaMS 0x201A

Definition at line 53 of file usb_commun.h.

#define PID_MegaAUDIO_IN_OUT 0x201B

Definition at line 54 of file usb_commun.h.

#define PID_MegaHIDMouse 0x201C

Definition at line 55 of file usb_commun.h.

#define PID_MegaHIDMouse_certif_U4 0x201D

Definition at line 56 of file usb_commun.h.

#define PID_MegaCDC_multi 0x201E

Definition at line 57 of file usb_commun.h.

#define PID_AT90USB128_64_MS_HIDMS_HID_USBKEY 0x2022

Definition at line 58 of file usb_commun.h.

#define PID_AT90USB128_64_MS_HIDMS_HID_STK525 0x2023

Definition at line 59 of file usb_commun.h.

#define PID_AT90USB128_64_MS 0x2029

Definition at line 60 of file usb_commun.h.

#define PID_Mega_MS_HIDMS 0x202A

Definition at line 61 of file usb_commun.h.

#define PID_MegaMS_2 0x2032

Definition at line 62 of file usb_commun.h.

#define PID_MegaLibUsb 0x2050

Definition at line 63 of file usb_commun.h.

#define PID_ATMega8U2_DFU 0x2FEE

Definition at line 64 of file usb_commun.h.

#define PID_ATMega16U2_DFU 0x2FEF

Definition at line 65 of file usb_commun.h.

#define PID_ATMega32U2_DFU 0x2FF0

Definition at line 66 of file usb_commun.h.

#define PID_ATMega32U6_DFU 0x2FF2

Definition at line 67 of file usb_commun.h.

#define PID_ATMega16U4_DFU 0x2FF3

Definition at line 68 of file usb_commun.h.

#define PID_ATMega32U4_DFU 0x2FF4

Definition at line 69 of file usb_commun.h.

#define PID_AT90USB82_DFU 0x2FF7

Definition at line 70 of file usb_commun.h.

#define PID_AT90USB64_DFU 0x2FF9

Definition at line 71 of file usb_commun.h.

#define PID_AT90USB162_DFU 0x2FFA

Definition at line 72 of file usb_commun.h.

#define PID_AT90USB128_DFU 0x2FFB

Definition at line 73 of file usb_commun.h.

#define CLASS_APPLICATION 0xFE

Use to declare a specific interface link at VID-PID.

Definition at line 79 of file usb_commun.h.

#define CLASS_VENDOR 0xFF

Use to declare a specific interface link at VID-PID.

Definition at line 80 of file usb_commun.h.

#define NO_CLASS 0x00

Definition at line 81 of file usb_commun.h.

#define NO_SUBCLASS 0x00

Definition at line 82 of file usb_commun.h.

#define NO_PROTOCOL 0x00

Definition at line 83 of file usb_commun.h.

#define CLASS_IAD 0xEF

Definition at line 88 of file usb_commun.h.

#define SUB_CLASS_IAD 0x02

Definition at line 89 of file usb_commun.h.

#define PROTOCOL_IAD 0x01

Definition at line 90 of file usb_commun.h.

#define USB_DEVICE_STATUS_BUS_POWERED 0x00

Definition at line 99 of file usb_commun.h.

#define USB_DEVICE_STATUS_SELF_POWERED 0x01

Definition at line 100 of file usb_commun.h.

#define USB_DEVICE_STATUS_REMOTEWAKEUP 0x02

Definition at line 101 of file usb_commun.h.

Referenced by usb_clear_feature(), and usb_set_feature().

#define USB_DEVICE_STATUS_BATTERYPOWERED 0x04

Definition at line 102 of file usb_commun.h.

#define USB_CONFIG_ATTRIBUTES_RESERVED 0x80

Definition at line 108 of file usb_commun.h.

#define USB_CONFIG_ATTRIBUTES_REMOTEWAKEUP 0x20

Definition at line 109 of file usb_commun.h.

#define USB_CONFIG_ATTRIBUTES_SELFPOWERED 0x40

Definition at line 110 of file usb_commun.h.

#define USB_CONFIG_BUSPOWERED (USB_CONFIG_ATTRIBUTES_RESERVED)

Definition at line 111 of file usb_commun.h.

#define USB_CONFIG_REMOTEWAKEUP (USB_CONFIG_ATTRIBUTES_RESERVED | USB_CONFIG_ATTRIBUTES_REMOTEWAKEUP)

Definition at line 112 of file usb_commun.h.

#define USB_CONFIG_SELFPOWERED (USB_CONFIG_ATTRIBUTES_RESERVED | USB_CONFIG_ATTRIBUTES_SELFPOWERED)

Definition at line 113 of file usb_commun.h.

#define USB_ENDPOINT_BULK 0x02

Definition at line 119 of file usb_commun.h.

#define USB_ENDPOINT_INTERRUPT 0x03

Definition at line 120 of file usb_commun.h.

#define USB_ENDPOINT_OUT 0x00

Definition at line 121 of file usb_commun.h.

#define USB_ENDPOINT_IN 0x80

Definition at line 122 of file usb_commun.h.

#define USB_ENDPOINT_DIR_MASK 0x80

Definition at line 123 of file usb_commun.h.

#define USB_ENDPOINT_NUM_MASK (~USB_ENDPOINT_DIR_MASK)

Definition at line 124 of file usb_commun.h.

#define USB_SETUP_DIR_HOST_TO_DEVICE (0<<7)

Definition at line 139 of file usb_commun.h.

#define USB_SETUP_DIR_DEVICE_TO_HOST (1<<7)

Definition at line 140 of file usb_commun.h.

Referenced by host_send_control().

#define USB_SETUP_TYPE_STANDARD (0<<5)

Definition at line 150 of file usb_commun.h.

#define USB_SETUP_TYPE_CLASS (1<<5)

Definition at line 151 of file usb_commun.h.

#define USB_SETUP_TYPE_VENDOR (2<<5)

Definition at line 152 of file usb_commun.h.

#define USB_SETUP_RECIPIENT_DEVICE (0)

Definition at line 163 of file usb_commun.h.

#define USB_SETUP_RECIPIENT_INTERFACE (1)

Definition at line 164 of file usb_commun.h.

#define USB_SETUP_RECIPIENT_ENDPOINT (2)

Definition at line 165 of file usb_commun.h.

#define USB_SETUP_RECIPIENT_OTHER (3)

Definition at line 166 of file usb_commun.h.

#define USB_SETUP_SET_STAND_DEVICE (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_DEVICE)

Definition at line 171 of file usb_commun.h.

Referenced by usb_clear_feature(), usb_process_request(), and usb_set_feature().

#define USB_SETUP_GET_STAND_DEVICE (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_DEVICE)

Definition at line 172 of file usb_commun.h.

Referenced by usb_get_status(), and usb_process_request().

#define USB_SETUP_SET_STAND_INTERFACE (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_INTERFACE)

Definition at line 173 of file usb_commun.h.

Referenced by usb_clear_feature(), usb_process_request(), and usb_set_feature().

#define USB_SETUP_GET_STAND_INTERFACE (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_INTERFACE)

Definition at line 174 of file usb_commun.h.

Referenced by usb_get_status(), and usb_process_request().

#define USB_SETUP_SET_STAND_ENDPOINT (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_ENDPOINT)

Definition at line 175 of file usb_commun.h.

Referenced by usb_clear_feature(), and usb_set_feature().

#define USB_SETUP_GET_STAND_ENDPOINT (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_STANDARD |USB_SETUP_RECIPIENT_ENDPOINT)

Definition at line 176 of file usb_commun.h.

Referenced by usb_get_status().

#define USB_SETUP_SET_CLASS_DEVICE (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_DEVICE)

Definition at line 181 of file usb_commun.h.

#define USB_SETUP_GET_CLASS_DEVICE (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_DEVICE)

Definition at line 182 of file usb_commun.h.

#define USB_SETUP_SET_CLASS_INTER (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_INTERFACE)

Definition at line 183 of file usb_commun.h.

Referenced by usb_user_read_request().

#define USB_SETUP_GET_CLASS_INTER (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_INTERFACE)

Definition at line 184 of file usb_commun.h.

Referenced by usb_user_read_request().

#define USB_SETUP_SET_CLASS_ENDPOINT (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_ENDPOINT)

Definition at line 185 of file usb_commun.h.

#define USB_SETUP_GET_CLASS_ENDPOINT (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_ENDPOINT)

Definition at line 186 of file usb_commun.h.

#define USB_SETUP_SET_CLASS_OTHER (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_OTHER)

Definition at line 187 of file usb_commun.h.

#define USB_SETUP_GET_CLASS_OTHER (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_CLASS |USB_SETUP_RECIPIENT_OTHER)

Definition at line 188 of file usb_commun.h.

#define USB_SETUP_SET_VENDOR_DEVICE (USB_SETUP_DIR_HOST_TO_DEVICE |USB_SETUP_TYPE_VENDOR |USB_SETUP_RECIPIENT_DEVICE)

Definition at line 189 of file usb_commun.h.

#define USB_SETUP_GET_VENDOR_DEVICE (USB_SETUP_DIR_DEVICE_TO_HOST |USB_SETUP_TYPE_VENDOR |USB_SETUP_RECIPIENT_DEVICE)

Definition at line 190 of file usb_commun.h.

#define SETUP_GET_STATUS 0x00

Definition at line 196 of file usb_commun.h.

Referenced by usb_process_request().

#define SETUP_GET_DEVICE 0x01

Definition at line 197 of file usb_commun.h.

#define SETUP_CLEAR_FEATURE 0x01

Definition at line 198 of file usb_commun.h.

Referenced by usb_process_request().

#define SETUP_GET_STRING 0x03

Definition at line 199 of file usb_commun.h.

#define SETUP_SET_FEATURE 0x03

Definition at line 200 of file usb_commun.h.

Referenced by usb_process_request().

#define SETUP_SET_ADDRESS 0x05

Definition at line 201 of file usb_commun.h.

Referenced by usb_process_request().

#define SETUP_GET_DESCRIPTOR 0x06

Definition at line 202 of file usb_commun.h.

Referenced by usb_process_request().

#define SETUP_SET_DESCRIPTOR 0x07

Definition at line 203 of file usb_commun.h.

#define SETUP_GET_CONFIGURATION 0x08

Definition at line 204 of file usb_commun.h.

Referenced by usb_process_request().

#define SETUP_SET_CONFIGURATION 0x09

Definition at line 205 of file usb_commun.h.

Referenced by usb_process_request().

#define SETUP_GET_INTERFACE 0x0A

Definition at line 206 of file usb_commun.h.

Referenced by usb_process_request().

#define SETUP_SET_INTERFACE 0x0B

Definition at line 207 of file usb_commun.h.

Referenced by usb_process_request().

#define SETUP_SYNCH_FRAME 0x0C

Definition at line 208 of file usb_commun.h.

#define DESCRIPTOR_DEVICE 0x01

Definition at line 213 of file usb_commun.h.

Referenced by usb_get_descriptor().

#define DESCRIPTOR_CONFIGURATION 0x02

Definition at line 214 of file usb_commun.h.

Referenced by host_check_class(), and usb_get_descriptor().

#define DESCRIPTOR_STRING 0x03

Definition at line 215 of file usb_commun.h.

Referenced by usb_user_get_descriptor().

#define DESCRIPTOR_INTERFACE 0x04

Definition at line 216 of file usb_commun.h.

Referenced by get_interface_descriptor_offset(), and host_check_class().

#define DESCRIPTOR_ENDPOINT 0x05

Definition at line 217 of file usb_commun.h.

Referenced by host_auto_configure_endpoint().

#define DESCRIPTOR_DEVICE_QUALIFIER 0x06

Definition at line 218 of file usb_commun.h.

#define DESCRIPTOR_CONF_OTHER_SPEED 0x07

Definition at line 219 of file usb_commun.h.

#define DESCRIPTOR_OTG 0x09

Definition at line 220 of file usb_commun.h.

#define DESCRIPTOR_IAD 0x0B

Definition at line 221 of file usb_commun.h.

#define FEATURE_DEVICE_REMOTE_WAKEUP 0x01

Definition at line 226 of file usb_commun.h.

Referenced by usb_clear_feature(), and usb_set_feature().

#define FEATURE_DEVICE_TEST 0x02

Definition at line 227 of file usb_commun.h.

#define FEATURE_DEVICE_OTG_B_HNP_ENABLE 0x03

Definition at line 228 of file usb_commun.h.

#define FEATURE_DEVICE_OTG_A_HNP_SUPPORT 0x04

Definition at line 229 of file usb_commun.h.

#define FEATURE_DEVICE_OTG_A_ALT_HNP_SUPPORT 0x05

Definition at line 230 of file usb_commun.h.

#define FEATURE_ENDPOINT_HALT 0x00

Definition at line 231 of file usb_commun.h.

Referenced by usb_clear_feature(), and usb_set_feature().

#define FEATURE_DEVICE_TEST_J 0x01

Definition at line 236 of file usb_commun.h.

#define FEATURE_DEVICE_TEST_K 0x02

Definition at line 237 of file usb_commun.h.

#define FEATURE_DEVICE_TEST_SEO_NAK 0x03

Definition at line 238 of file usb_commun.h.

#define FEATURE_DEVICE_TEST_PACKET 0x04

Definition at line 239 of file usb_commun.h.

#define FEATURE_DEVICE_TEST_FORCE_ENABLE 0x05

Definition at line 240 of file usb_commun.h.

#define DESCRIPTOR_OTG_bLength 0x03

Definition at line 246 of file usb_commun.h.

#define HNP_SUPPORT 0x02

Definition at line 247 of file usb_commun.h.

Referenced by usb_set_feature().

#define SRP_SUPPORT 0x01

Definition at line 248 of file usb_commun.h.