- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# usb_drv.h File Reference

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Defines
#define | MAX_EP_NB 7
#define | EP_CONTROL 0
#define | EP_1 1
#define | EP_2 2
#define | EP_3 3
#define | EP_4 4
#define | EP_5 5
#define | EP_6 6
#define | EP_7 7
#define | PIPE_CONTROL 0
#define | PIPE_0 0
#define | PIPE_1 1
#define | PIPE_2 2
#define | PIPE_3 3
#define | PIPE_4 4
#define | PIPE_5 5
#define | PIPE_6 6
#define | PIPE_7 7
#define | MSK_EP_DIR 0x7F
#define | MSK_UADD 0x7F
#define | MSK_EPTYPE 0xC0
#define | MSK_EPSIZE 0x70
#define | MSK_EPBK 0x0C
#define | MSK_DTSEQ 0x0C
#define | MSK_NBUSYBK 0x03
#define | MSK_CURRBK 0x03
#define | MSK_DAT 0xFF
#define | MSK_BYCTH 0x07
#define | MSK_BYCTL 0xFF
#define | MSK_EPINT 0x7F
#define | MSK_HADDR 0xFF
#define | MSK_PNUM 0x07
#define | MSK_PRST 0x7F
#define | MSK_PTYPE 0xC0
#define | MSK_PTOKEN 0x30
#define | MSK_PEPNUM 0x0F
#define | MSK_PSIZE 0x70
#define | MSK_PBK 0x0C
#define | MSK_NBUSYBK 0x03
#define | MSK_ERROR 0x1F
#define | MSK_PTYPE 0xC0
#define | MSK_PTOKEN 0x30
#define | MSK_TOKEN_SETUP 0x30
#define | MSK_TOKEN_IN 0x10
#define | MSK_TOKEN_OUT 0x20
#define | MSK_PEPNUM 0x0F
#define | MSK_PSIZE 0x70
#define | MSK_PBK 0x0C
#define | TYPE_CONTROL 0
#define | TYPE_ISOCHRONOUS 1
#define | TYPE_BULK 2
#define | TYPE_INTERRUPT 3
#define | DIRECTION_OUT 0
#define | DIRECTION_IN 1
#define | SIZE_8 0
#define | SIZE_16 1
#define | SIZE_32 2
#define | SIZE_64 3
#define | SIZE_128 4
#define | SIZE_256 5
#define | SIZE_512 6
#define | SIZE_1024 7
#define | ONE_BANK 0
#define | TWO_BANKS 1
#define | NYET_ENABLED 0
#define | NYET_DISABLED 1
#define | TOKEN_SETUP 0
#define | TOKEN_IN 1
#define | TOKEN_OUT 2
#define | Is_ep_addr_in(x) ( (x&USB_ENDPOINT_DIR_MASK)? TRUE : FALSE)
#define | VBUSRISE_20MS 0x00
| OTG Timers customizing.
#define | VBUSRISE_50MS 0x01
#define | VBUSRISE_70MS 0x02
#define | VBUSRISE_100MS 0x03
#define | VBUSPULSE_15MS 0x20
#define | VBUSPULSE_23MS 0x21
#define | VBUSPULSE_31MS 0x22
#define | VBUSPULSE_40MS 0x23
#define | VFALLTMOUT_93MS 0x40
#define | VFALLTMOUT_105MS 0x41
#define | VFALLTMOUT_118MS 0x42
#define | VFALLTMOUT_131MS 0x43
#define | SRPMINDET_10US 0x60
#define | SRPMINDET_100US 0x61
#define | SRPMINDET_1MS 0x62
#define | SRPMINDET_11MS 0x63
#define | Usb_build_ep_config0(type, dir, nyet) ((type<<6) | (nyet<<1) | (dir))
#define | Usb_build_ep_config1(size, bank) ((size<<4) | (bank<<2) )
#define | usb_configure_endpoint(num, type, dir, size, bank, nyet)
#define | Host_build_pipe_config0(type, token, ep_num) ((type<<6) | (token<<4) | (ep_num))
#define | Host_build_pipe_config1(size, bank) ((size<<4) | (bank<<2) )
#define | host_configure_pipe(num, type, token, ep_num, size, bank, freq)
#define | Usb_enable_regulator() (UHWCON |= (1<<UVREGE))
| Enable internal USB pads regulator.
#define | Usb_disable_regulator() (UHWCON &= ~(1<<UVREGE))
| Disable internal USB pads regulator.
#define | Is_usb_regulator_enabled() ((UHWCON & (1<<UVREGE)) ? TRUE : FALSE)
| Check regulator enable bit.
#define | Usb_enable_uid_pin() (UHWCON |= (1<<UIDE))
| Enable external UID pin.
#define | Usb_disable_uid_pin() (UHWCON &= ~(1<<UIDE))
| Disable external UID pin.
#define | Usb_force_device_mode() (Usb_disable_uid_pin(), UHWCON |= (1<<UIMOD))
| Disable external UID pin and force device mode.
#define | Usb_force_host_mode() (Usb_disable_uid_pin(), UHWCON &= ~(1<<UIMOD))
| Disable external UID pin and force host mode.
#define | Usb_enable_uvcon_pin() (UHWCON |= (1<<UVCONE))
| Enable external UVCON pin.
#define | Usb_disable_uvcon_pin() (UHWCON &= ~(1<<UVCONE))
| Enable external UVCON pin.
#define | Usb_full_speed_mode() (UDCON &= ~(1<<LSM))
| Use device full speed mode (default mode).
#define | Usb_low_speed_mode() (UDCON |= (1<<LSM))
| For device mode, force low speed mode.
#define | Usb_enable() (USBCON |= ((1<<USBE) | (1<<OTGPADE)))
| Enable both USB interface and Vbus pad.
#define | Usb_disable() (USBCON &= ~((1<<USBE) | (1<<OTGPADE)))
| Disable both USB interface and Vbus pad.
#define | Is_usb_enabled() ((USBCON & (1<<USBE)) ? TRUE : FALSE)
#define | Usb_engine_enable() (USBCON |= (1<<USBE) )
| Enable USB engine only.
#define | Usb_engine_disable() (USBCON &= ~(1<<USBE))
| Disable both USB interface and Vbus pad.
#define | Usb_enable_vbus_pad() (USBCON |= (1<<OTGPADE))
| Enable VBUS pad.
#define | Usb_disable_vbus_pad() (USBCON &= ~(1<<OTGPADE))
| Disable VBUS pad.
#define | Usb_select_device() (USBCON &= ~(1<<HOST))
#define | Usb_select_host() (USBCON |= (1<<HOST))
#define | Is_usb_host_enabled() ((USBCON & (1<<HOST)) ? TRUE : FALSE)
#define | Is_usb_device_enabled() ((USBCON & (1<<HOST)) ? FALSE : TRUE)
#define | Usb_freeze_clock() (USBCON |= (1<<FRZCLK))
| Stop internal USB clock in interface (freeze the interface register).
#define | Usb_unfreeze_clock() (USBCON &= ~(1<<FRZCLK))
#define | Is_usb_clock_freezed() ((USBCON & (1<<FRZCLK)) ? TRUE : FALSE)
#define | Usb_enable_id_interrupt() (USBCON |= (1<<IDTE))
#define | Usb_disable_id_interrupt() (USBCON &= ~(1<<IDTE))
#define | Is_usb_id_interrupt_enabled() ((USBCON & (1<<IDTE)) ? TRUE : FALSE)
#define | Is_usb_id_device() ((USBSTA & (1<<ID)) ? TRUE : FALSE)
#define | Is_usb_id_host() ((USBSTA & (1<<ID)) ? FALSE : TRUE)
#define | Usb_ack_id_transition() (USBINT = ~(1<<IDTI))
#define | Is_usb_id_transition() ((USBINT & (1<<IDTI)) ? TRUE : FALSE)
#define | Usb_enable_vbus_interrupt() (USBCON |= (1<<VBUSTE))
#define | Usb_disable_vbus_interrupt() (USBCON &= ~(1<<VBUSTE))
#define | Is_usb_vbus_interrupt_enabled() ((USBCON & (1<<VBUSTE)) ? TRUE : FALSE)
#define | Is_usb_vbus_high() ((USBSTA & (1<<VBUS)) ? TRUE : FALSE)
#define | Is_usb_vbus_low() ((USBSTA & (1<<VBUS)) ? FALSE : TRUE)
#define | Usb_ack_vbus_transition() (USBINT = ~(1<<VBUSTI))
#define | Is_usb_vbus_transition() ((USBINT & (1<<VBUSTI)) ? TRUE : FALSE)
#define | MSK_IDTE_VBUSTE ((1<<IDTE)|(1<<VBUSTE))
#define | Usb_get_general_interrupt() (USBINT & (USBCON & MSK_IDTE_VBUSTE))
| returns the USB general interrupts (interrupt enabled)
#define | Usb_ack_all_general_interrupt() (USBINT = ~(USBCON & MSK_IDTE_VBUSTE))
| acks the general interrupts (interrupt enabled)
#define | Usb_ack_cache_id_transition(x) ((x) &= ~(1<<IDTI))
#define | Usb_ack_cache_vbus_transition(x) ((x) &= ~(1<<VBUSTI))
#define | Is_usb_cache_id_transition(x) (((x) & (1<<IDTI)) )
#define | Is_usb_cache_vbus_transition(x) (((x) & (1<<VBUSTI)))
#define | Usb_get_otg_interrupt() (OTGINT & OTGIEN)
| returns the USB Pad interrupts (interrupt enabled)
#define | Usb_ack_all_otg_interrupt() (OTGINT = ~OTGIEN)
| acks the USB Pad interrupts (interrupt enabled)
#define | Is_otg_cache_bconnection_error(x) (((x) & MSK_BCERRI))
#define | Usb_ack_cache_bconnection_error(x) ((x) &= ~MSK_BCERRI)
#define | Usb_enter_dpram_mode() (UDPADDH = (1<<DPACC))
#define | Usb_exit_dpram_mode() (UDPADDH = (U8)~(1<<DPACC))
#define | Usb_set_dpram_address(addr) (UDPADDH = (1<<DPACC) + ((Uint16)addr >> 8), UDPADDL = (Uchar)addr)
#define | Usb_write_dpram_byte(val) (UEDATX=val)
#define | Usb_read_dpram_byte() (UEDATX)
#define | Usb_enable_vbus() (OTGCON |= (1<<VBUSREQ))
| requests for VBus activation
#define | Usb_disable_vbus() (OTGCON |= (1<<VBUSRQC))
| requests for VBus desactivation
#define | Usb_enable_manual_vbus() (PORTE|=0x80,DDRE|=0x80,Usb_disable_uvcon_pin())
| Manually request VBUS ON without UVCON signal from USB interface.
#define | Usb_disable_manual_vbus() (PORTE&=~0x80,DDRE|=0x80,Usb_enable_uvcon_pin())
| Manually request VBUS OFF without UVCON signal from USB interface.
#define | Is_usb_vbus_manual_on() (((PINE&0x80) != 0) ? TRUE : FALSE)
| is vbus manually activated ?
#define | Usb_device_initiate_hnp() (OTGCON |= (1<<HNPREQ))
| initiates a Host Negociation Protocol
#define | Usb_device_stop_hnp() (OTGCON &= ~(1<<HNPREQ))
| stops a Host Negociation Protocol
#define | Usb_host_accept_hnp() (OTGCON |= (1<<HNPREQ))
| accepts a Host Negociation Protocol
#define | Usb_host_reject_hnp() (OTGCON &= ~(1<<HNPREQ))
| rejects a Host Negociation Protocol
#define | Usb_device_initiate_srp() (OTGCON |= (1<<SRPREQ))
| initiates a Session Request Protocol
#define | Usb_select_vbus_srp_method() (OTGCON |= (1<<SRPSEL))
| selects VBus as SRP method
#define | Usb_select_data_srp_method() (OTGCON &= ~(1<<SRPSEL))
| selects data line as SRP method
#define | Usb_enable_vbus_hw_control() (OTGCON &= ~(1<<VBUSHWC))
| enables hardware control on VBus
#define | Usb_disable_vbus_hw_control() (OTGCON |= (1<<VBUSHWC))
| disables hardware control on VBus
#define | Is_usb_vbus_enabled() ((OTGCON & (1<<VBUSREQ)) ? TRUE : FALSE)
| tests if VBus has been requested
#define | Is_usb_hnp() ((OTGCON & (1<<HNPREQ)) ? TRUE : FALSE)
| tests if a HNP occurs
#define | Is_usb_device_srp() ((OTGCON & (1<<SRPREQ)) ? TRUE : FALSE)
| tests if a SRP from device occurs
#define | Is_usb_device_initiating_srp() ((OTGCON & (1<<SRPREQ)) ? TRUE : FALSE)
| tests if device is initiating SRP
#define | Set_otg_custom_timer(sel) (OTGTCON = sel)
| selects one of the four OTG timers and sets up the specified delay
#define | Usb_enable_suspend_time_out_interrupt() (OTGIEN |= (1<<STOE))
| enables suspend time out interrupt
#define | Usb_disable_suspend_time_out_interrupt() (OTGIEN &= ~(1<<STOE))
| disables suspend time out interrupt
#define | Is_suspend_time_out_interrupt_enabled() ((OTGIEN & (1<<STOE)) ? TRUE : FALSE)
#define | Usb_ack_suspend_time_out_interrupt() (OTGINT &= ~(1<<STOI))
| acks suspend time out interrupt
#define | Is_usb_suspend_time_out_interrupt() ((OTGINT & (1<<STOI)) ? TRUE : FALSE)
| tests if a suspend time out occurs
#define | Usb_enable_hnp_error_interrupt() (OTGIEN |= (1<<HNPERRE))
| enables HNP error interrupt
#define | Usb_disable_hnp_error_interrupt() (OTGIEN &= ~(1<<HNPERRE))
| disables HNP error interrupt
#define | Is_hnp_error_interrupt_enabled() ((OTGIEN & (1<<HNPERRE)) ? TRUE : FALSE)
#define | Usb_ack_hnp_error_interrupt() (OTGINT &= ~(1<<HNPERRI))
| acks HNP error interrupt
#define | Is_usb_hnp_error_interrupt() ((OTGINT & (1<<HNPERRI)) ? TRUE : FALSE)
| tests if a HNP error occurs
#define | Usb_enable_role_exchange_interrupt() (OTGIEN |= (1<<ROLEEXE))
| enables role exchange interrupt
#define | Usb_disable_role_exchange_interrupt() (OTGIEN &= ~(1<<ROLEEXE))
| disables role exchange interrupt
#define | Is_role_exchange_interrupt_enabled() ((OTGIEN & (1<<ROLEEXE)) ? TRUE : FALSE)
#define | Usb_ack_role_exchange_interrupt() (OTGINT &= ~(1<<ROLEEXI))
| acks role exchange interrupt
#define | Is_usb_role_exchange_interrupt() ((OTGINT & (1<<ROLEEXI)) ? TRUE : FALSE)
| tests if a role exchange occurs
#define | Usb_enable_bconnection_error_interrupt() (OTGIEN |= (1<<BCERRE))
| enables B device connection error interrupt
#define | Usb_disable_bconnection_error_interrupt() (OTGIEN &= ~(1<<BCERRE))
| disables B device connection error interrupt
#define | Is_bconnection_error_interrupt_enabled() ((OTGIEN & (1<<BCERRE)) ? TRUE : FALSE)
#define | Usb_ack_bconnection_error_interrupt() (OTGINT &= ~(1<<BCERRI))
| acks B device connection error interrupt
#define | Is_usb_bconnection_error_interrupt() ((OTGINT & (1<<BCERRI)) ? TRUE : FALSE)
| tests if a B device connection error occurs
#define | Usb_enable_vbus_error_interrupt() (OTGIEN |= (1<<VBERRE))
| enables VBus error interrupt
#define | Usb_disable_vbus_error_interrupt() (OTGIEN &= ~(1<<VBERRE))
| disables VBus error interrupt
#define | Is_vbus_error_interrupt_enabled() ((OTGIEN & (1<<VBERRE)) ? TRUE : FALSE)
#define | Usb_ack_vbus_error_interrupt() (OTGINT &= ~(1<<VBERRI))
| acks VBus error interrupt
#define | Is_usb_vbus_error_interrupt() ((OTGINT & (1<<VBERRI)) ? TRUE : FALSE)
| tests if a VBus error occurs
#define | Usb_enable_srp_interrupt() (OTGIEN |= (1<<SRPE))
| enables SRP interrupt
#define | Usb_disable_srp_interrupt() (OTGIEN &= ~(1<<SRPE))
| disables SRP interrupt
#define | Is_srp_interrupt_enabled() ((OTGIEN & (1<<SRPE)) ? TRUE : FALSE)
#define | Usb_ack_srp_interrupt() (OTGINT &= ~(1<<SRPI))
| acks SRP interrupt
#define | Is_usb_srp_interrupt() ((OTGINT & (1<<SRPI)) ? TRUE : FALSE)
| tests if a SRP occurs
#define | Usb_initiate_remote_wake_up() (UDCON |= (1<<RMWKUP))
| initiates a remote wake-up
#define | Usb_detach() (UDCON |= (1<<DETACH))
| detaches from USB bus
#define | Usb_attach() (UDCON &= ~(1<<DETACH))
| attaches to USB bus
#define | Is_usb_pending_remote_wake_up() ((UDCON & (1<<RMWKUP)) ? TRUE : FALSE)
| test if remote wake-up still running
#define | Is_usb_detached() ((UDCON & (1<<DETACH)) ? TRUE : FALSE)
| test if the device is detached
#define | Usb_get_device_interrupt() (UDINT & (1<<UDIEN))
| returns the USB device interrupts (interrupt enabled)
#define | Usb_ack_all_device_interrupt() (UDINT = ~(1<<UDIEN))
| acks the USB device interrupts (interrupt enabled)
#define | Usb_enable_remote_wake_up_interrupt() (UDIEN |= (1<<UPRSME))
| enables remote wake-up interrupt
#define | Usb_disable_remote_wake_up_interrupt() (UDIEN &= ~(1<<UPRSME))
| disables remote wake-up interrupt
#define | Is_remote_wake_up_interrupt_enabled() ((UDIEN & (1<<UPRSME)) ? TRUE : FALSE)
#define | Usb_ack_remote_wake_up_start() (UDINT = ~(1<<UPRSMI))
| acks remote wake-up
#define | Is_usb_remote_wake_up_start() ((UDINT & (1<<UPRSMI)) ? TRUE : FALSE)
| tests if remote wake-up still running
#define | Usb_enable_resume_interrupt() (UDIEN |= (1<<EORSME))
| enables resume interrupt
#define | Usb_disable_resume_interrupt() (UDIEN &= ~(1<<EORSME))
| disables resume interrupt
#define | Is_resume_interrupt_enabled() ((UDIEN & (1<<EORSME)) ? TRUE : FALSE)
#define | Usb_ack_resume() (UDINT = ~(1<<EORSMI))
| acks resume
#define | Is_usb_resume() ((UDINT & (1<<EORSMI)) ? TRUE : FALSE)
| tests if resume occurs
#define | Usb_enable_wake_up_interrupt() (UDIEN |= (1<<WAKEUPE))
| enables wake-up interrupt
#define | Usb_disable_wake_up_interrupt() (UDIEN &= ~(1<<WAKEUPE))
| disables wake-up interrupt
#define | Is_wake_up_interrupt_enabled() ((UDIEN & (1<<WAKEUPE)) ? TRUE : FALSE)
#define | Usb_ack_wake_up() (UDINT = ~(1<<WAKEUPI))
| acks wake-up
#define | Is_usb_wake_up() ((UDINT & (1<<WAKEUPI)) ? TRUE : FALSE)
| tests if wake-up occurs
#define | Usb_enable_reset_interrupt() (UDIEN |= (1<<EORSTE))
| enables USB reset interrupt
#define | Usb_disable_reset_interrupt() (UDIEN &= ~(1<<EORSTE))
| disables USB reset interrupt
#define | Is_reset_interrupt_enabled() ((UDIEN & (1<<EORSTE)) ? TRUE : FALSE)
#define | Usb_ack_reset() (UDINT = ~(1<<EORSTI))
| acks USB reset
#define | Is_usb_reset() ((UDINT & (1<<EORSTI)) ? TRUE : FALSE)
| tests if USB reset occurs
#define | Usb_enable_sof_interrupt() (UDIEN |= (1<<SOFE))
| enables Start Of Frame Interrupt
#define | Usb_disable_sof_interrupt() (UDIEN &= ~(1<<SOFE))
| disables Start Of Frame Interrupt
#define | Is_sof_interrupt_enabled() ((UDIEN & (1<<SOFE)) ? TRUE : FALSE)
#define | Usb_ack_sof() (UDINT = ~(1<<SOFI))
| acks Start Of Frame
#define | Is_usb_sof() ((UDINT & (1<<SOFI)) ? TRUE : FALSE)
| tests if Start Of Frame occurs
#define | Usb_enable_suspend_interrupt() (UDIEN |= (1<<SUSPE))
| enables suspend state interrupt
#define | Usb_disable_suspend_interrupt() (UDIEN &= ~(1<<SUSPE))
| disables suspend state interrupt
#define | Is_suspend_interrupt_enabled() ((UDIEN & (1<<SUSPE)) ? TRUE : FALSE)
#define | Usb_ack_suspend() (UDINT = ~(1<<SUSPI))
| acks Suspend
#define | Is_usb_suspend() ((UDINT & (1<<SUSPI)) ? TRUE : FALSE)
| tests if Suspend state detected
#define | Usb_enable_address() (UDADDR |= (1<<ADDEN))
| enables USB device address
#define | Usb_disable_address() (UDADDR &= ~(1<<ADDEN))
| disables USB device address
#define | Usb_configure_address(addr) (UDADDR = (UDADDR & (1<<ADDEN)) | ((U8)addr & MSK_UADD))
| sets the USB device address
#define | Usb_frame_number() ((U16)((((U16)UDFNUMH) << 8) | ((U16)UDFNUML)))
| returns the last frame number
#define | Is_usb_frame_number_crc_error() ((UDMFN & (1<<FNCERR)) ? TRUE : FALSE)
| tests if a crc error occurs in frame number
#define | Usb_select_endpoint(ep) (UENUM = (U8)ep )
| selects the endpoint number to interface with the CPU
#define | Usb_get_selected_endpoint() (UENUM )
| get the currently selected endpoint number
#define | Usb_reset_endpoint(ep) (UERST = 1 << (U8)ep, UERST = 0)
| resets the selected endpoint
#define | Usb_enable_endpoint() (UECONX |= (1<<EPEN))
| enables the current endpoint
#define | Usb_enable_stall_handshake() (UECONX |= (1<<STALLRQ))
| enables the STALL handshake for the next transaction
#define | Usb_reset_data_toggle() (UECONX |= (1<<RSTDT))
| resets the data toggle sequence
#define | Usb_disable_endpoint() (UECONX &= ~(1<<EPEN))
| disables the current endpoint
#define | Usb_disable_stall_handshake() (UECONX |= (1<<STALLRQC))
| disables the STALL handshake
#define | Usb_select_epnum_for_cpu() (UECONX &= ~(1<<EPNUMS))
| selects endpoint interface on CPU
#define | Is_usb_endpoint_enabled() ((UECONX & (1<<EPEN)) ? TRUE : FALSE)
| tests if the current endpoint is enabled
#define | Is_usb_endpoint_stall_requested() ((UECONX & (1<<STALLRQ)) ? TRUE : FALSE)
| tests if STALL handshake request is running
#define | Usb_configure_endpoint_type(type) (UECFG0X = (UECFG0X & ~(MSK_EPTYPE)) | ((U8)type << 6))
| configures the current endpoint
#define | Usb_configure_endpoint_direction(dir) (UECFG0X = (UECFG0X & ~(1<<EPDIR)) | ((U8)dir))
| configures the current endpoint direction
#define | Usb_configure_endpoint_size(size) (UECFG1X = (UECFG1X & ~MSK_EPSIZE) | ((U8)size << 4))
| configures the current endpoint size
#define | Usb_configure_endpoint_bank(bank) (UECFG1X = (UECFG1X & ~MSK_EPBK) | ((U8)bank << 2))
| configures the current endpoint number of banks
#define | Usb_allocate_memory() (UECFG1X |= (1<<ALLOC))
| allocates the current configuration in DPRAM memory
#define | Usb_unallocate_memory() (UECFG1X &= ~(1<<ALLOC))
| un-allocates the current configuration in DPRAM memory
#define | Usb_ack_overflow_interrupt() (UESTA0X &= ~(1<<OVERFI))
| acks endpoint overflow interrupt
#define | Usb_ack_underflow_interrupt() (UESTA0X &= ~(1<<UNDERFI))
| acks endpoint underflow memory
#define | Usb_ack_zlp() (UESTA0X &= ~(1<<ZLPSEEN))
| acks Zero Length Packet received
#define | Usb_data_toggle() ((UESTA0X&MSK_DTSEQ) >> 2)
| returns data toggle
#define | Usb_nb_busy_bank() (UESTA0X & MSK_NBUSYBK)
| returns the number of busy banks
#define | Is_usb_one_bank_busy() ((UESTA0X & MSK_NBUSYBK) == 0 ? FALSE : TRUE)
| tests if at least one bank is busy
#define | Is_endpoint_configured() ((UESTA0X & (1<<CFGOK)) ? TRUE : FALSE)
| tests if current endpoint is configured
#define | Is_usb_overflow() ((UESTA0X & (1<<OVERFI)) ? TRUE : FALSE)
| tests if an overflows occurs
#define | Is_usb_underflow() ((UESTA0X & (1<<UNDERFI)) ? TRUE : FALSE)
| tests if an underflow occurs
#define | Is_usb_zlp() ((UESTA0X & (1<<ZLPSEEN)) ? TRUE : FALSE)
| tests if a ZLP has been detected
#define | Usb_control_direction() ((UESTA1X & (1<<CTRLDIR)) >> 2)
| returns the control direction
#define | Usb_current_bank() ( UESTA1X & MSK_CURRBK)
| returns the number of the current bank
#define | Usb_ack_fifocon() (UEINTX &= ~(1<<FIFOCON))
| clears FIFOCON bit
#define | Usb_ack_nak_in() (UEINTX &= ~(1<<NAKINI))
| acks NAK IN received
#define | Usb_ack_nak_out() (UEINTX &= ~(1<<NAKOUTI))
| acks NAK OUT received
#define | Usb_ack_receive_setup() (UEINTX &= ~(1<<RXSTPI))
| acks receive SETUP
#define | Usb_ack_receive_out() (UEINTX &= ~(1<<RXOUTI), Usb_ack_fifocon())
| acks reveive OUT
#define | Usb_ack_stalled() (MSK_STALLEDI= 0)
| acks STALL sent
#define | Usb_ack_in_ready() (UEINTX &= ~(1<<TXINI), Usb_ack_fifocon())
| acks IN ready
#define | Usb_kill_last_in_bank() (UENTTX |= (1<<RXOUTI))
| Kills last bank.
#define | Is_usb_read_enabled() (UEINTX&(1<<RWAL))
| tests if endpoint read allowed
#define | Is_usb_write_enabled() (UEINTX&(1<<RWAL))
| tests if endpoint write allowed
#define | Is_usb_read_control_enabled() (UEINTX&(1<<TXINI))
| tests if read allowed on control endpoint
#define | Is_usb_nak_in_sent() (UEINTX&(1<<NAKINI))
| tests if a NAK has been sent on IN endpoint
#define | Is_usb_nak_out_sent() (UEINTX&(1<<NAKOUTI))
| tests if a NAK has been sent on OUT endpoint
#define | Is_usb_receive_setup() (UEINTX&(1<<RXSTPI))
| tests if SETUP received
#define | Is_usb_receive_out() (UEINTX&(1<<RXOUTI))
| tests if OUT received
#define | Is_usb_in_ready() (UEINTX&(1<<TXINI))
| tests if IN ready
#define | Usb_send_in() (UEINTX &= ~(1<<FIFOCON))
| sends IN
#define | Usb_send_control_in() (UEINTX &= ~(1<<TXINI))
| sends IN on control endpoint
#define | Usb_free_out_bank() (UEINTX &= ~(1<<FIFOCON))
| frees OUT bank
#define | Usb_ack_control_out() (UEINTX &= ~(1<<RXOUTI))
| acks OUT on control endpoint
#define | Usb_enable_flow_error_interrupt() (UEIENX |= (1<<FLERRE))
| enables flow error interrupt
#define | Usb_enable_nak_in_interrupt() (UEIENX |= (1<<NAKINE))
| enables NAK IN interrupt
#define | Usb_enable_nak_out_interrupt() (UEIENX |= (1<<NAKOUTE))
| enables NAK OUT interrupt
#define | Usb_enable_receive_setup_interrupt() (UEIENX |= (1<<RXSTPE))
| enables receive SETUP interrupt
#define | Usb_enable_receive_out_interrupt() (UEIENX |= (1<<RXOUTE))
| enables receive OUT interrupt
#define | Usb_enable_stalled_interrupt() (UEIENX |= (1<<STALLEDE))
| enables STALL sent interrupt
#define | Usb_enable_in_ready_interrupt() (UEIENX |= (1<<TXIN))
| enables IN ready interrupt
#define | Usb_disable_flow_error_interrupt() (UEIENX &= ~(1<<FLERRE))
| disables flow error interrupt
#define | Usb_disable_nak_in_interrupt() (UEIENX &= ~(1<<NAKINE))
| disables NAK IN interrupt
#define | Usb_disable_nak_out_interrupt() (UEIENX &= ~(1<<NAKOUTE))
| disables NAK OUT interrupt
#define | Usb_disable_receive_setup_interrupt() (UEIENX &= ~(1<<RXSTPE))
| disables receive SETUP interrupt
#define | Usb_disable_receive_out_interrupt() (UEIENX &= ~(1<<RXOUTE))
| disables receive OUT interrupt
#define | Usb_disable_stalled_interrupt() (UEIENX &= ~(1<<STALLEDE))
| disables STALL sent interrupt
#define | Usb_disable_in_ready_interrupt() (UEIENX &= ~(1<<TXIN))
| disables IN ready interrupt
#define | Usb_read_byte() (UEDATX)
| returns FIFO byte for current endpoint
#define | Usb_write_byte(byte) (UEDATX = (U8)byte)
| writes byte in FIFO for current endpoint
#define | Usb_byte_counter() ((((U16)UEBCHX) << 8) | (UEBCLX))
| returns number of bytes in FIFO current endpoint (16 bits)
#define | Usb_byte_counter_8() ((U8)UEBCLX)
| returns number of bytes in FIFO current endpoint (8 bits)
#define | Usb_interrupt_flags() (UEINT)
| tests the general endpoint interrupt flags
#define | Is_usb_endpoint_event() (Usb_interrupt_flags() != 0x00)
| tests the general endpoint interrupt flags
#define | Host_allocate_memory() (UPCFG1X |= (1<<ALLOC))
| allocates the current configuration in DPRAM memory
#define | Host_unallocate_memory() (UPCFG1X &= ~(1<<ALLOC))
| un-allocates the current configuration in DPRAM memory
#define | Is_host_pipe_memory_allocated() (UPCFG1X & (1<<ALLOC) ? TRUE : FALSE)
| Check if pipe memory is allocated.
#define | Host_enable() (USBCON |= (1<<HOST))
| enables USB Host function
#define | SOFEN 0
#define | Host_enable_sof() (UHCON |= (1<<SOFEN))
| enables SOF generation
#define | Host_disable_sof() (UHCON &= ~(1<<SOFEN))
| disables SOF generation
#define | Host_send_reset() (UHCON |= (1<<RESET))
| sends a USB Reset to the device
#define | Host_is_reset() ((UHCON & (1<<RESET)) ? TRUE : FALSE)
| tests if USB Reset running
#define | Host_send_resume() (UHCON |= (1<<RESUME))
| sends a USB Resume to the device
#define | Host_is_resume() ((UHCON & (1<<RESUME)) ? TRUE : FALSE)
| tests if USB Resume running
#define | Host_enable_sof_interrupt() (UHIEN |= (1<<HSOFE))
| enables host start of frame interrupt
#define | Host_disable_sof_interrupt() (UHIEN &= ~(1<<HSOFE))
| enables host start of frame interrupt
#define | Is_host_sof_interrupt_enabled() ((UHIEN & (1<<HSOFE)) ? TRUE : FALSE)
#define | Host_is_sof() ((UHINT & (1<<HSOFI)) ? TRUE : FALSE)
| tests if SOF detected
#define | Is_host_sof() ((UHINT & (1<<HSOFI)) ? TRUE : FALSE)
#define | Host_ack_sof() (UHINT &= ~(1<<HSOFI))
#define | Host_enable_hwup_interrupt() (UHIEN |= (1<<HWUPE))
| enables host wake up interrupt detection
#define | Host_disable_hwup_interrupt() (UHIEN &= ~(1<<HWUPE))
| disables host wake up interrupt detection
#define | Is_host_hwup_interrupt_enabled() ((UHIEN & (1<<HWUPE)) ? TRUE : FALSE)
#define | Host_is_hwup() ((UHINT & (1<<HWUPI)) ? TRUE : FALSE)
| tests if host wake up detected
#define | Is_host_hwup() ((UHINT & (1<<HWUPI)) ? TRUE : FALSE)
| Ack host wake up detection.
#define | Host_ack_hwup() (UHINT &= ~(1<<HWUPI))
#define | Host_enable_down_stream_resume_interrupt() (UHIEN |= (1<<RSMEDE))
| enables host down stream rsm sent interrupt detection
#define | Host_disable_down_stream_resume_interrupt() (UHIEN &= ~(1<<RSMEDE))
| disables host down stream rsm sent interrupt detection
#define | Is_host_down_stream_resume_interrupt_enabled() ((UHIEN & (1<<RSMEDE)) ? TRUE : FALSE)
#define | Is_host_down_stream_resume() ((UHINT & (1<<RSMEDI)) ? TRUE : FALSE)
| Ack host down stream resume sent.
#define | Host_ack_down_stream_resume() (UHINT &= ~(1<<RSMEDI))
#define | Host_enable_remote_wakeup_interrupt() (UHIEN |= (1<<RXRSME))
| enables host remote wake up interrupt detection
#define | Host_disable_remote_wakeup_interrupt() (UHIEN &= ~(1<<RXRSME))
| disables host remote wake up interrupt detection
#define | Is_host_remote_wakeup_interrupt_enabled() ((UHIEN & (1<<RXRSME)) ? TRUE : FALSE)
#define | Host_is_remote_wakeup() ((UHINT & (1<<RXRSMI)) ? TRUE : FALSE)
| tests if host wake up detected
#define | Is_host_remote_wakeup() ((UHINT & (1<<RXRSMI)) ? TRUE : FALSE)
| Ack host wake up detection.
#define | Host_ack_remote_wakeup() (UHINT &= ~(1<<RXRSMI))
#define | Host_enable_device_connection_interrupt() (UHIEN |= (1<<DCONNE))
| enables host device connection interrupt
#define | Host_disable_device_connection_interrupt() (UHIEN &= ~(1<<DCONNE))
| disables USB device connection interrupt
#define | Is_host_device_connection_interrupt_enabled() ((UHIEN & (1<<DCONNE)) ? TRUE : FALSE)
#define | Is_device_connection() (UHINT & (1<<DCONNI))
| tests if a USB device has been detected
#define | Host_ack_device_connection() (UHINT = ~(1<<DCONNI))
| acks device connection
#define | Host_enable_device_disconnection_interrupt() (UHIEN |= (1<<DDISCE))
| enables host device disconnection interrupt
#define | Host_disable_device_disconnection_interrupt() (UHIEN &= ~(1<<DDISCE))
| disables USB device connection interrupt
#define | Is_host_device_disconnection_interrupt_enabled() ((UHIEN & (1<<DDISCE)) ? TRUE : FALSE)
#define | Is_device_disconnection() (UHINT & (1<<DDISCI) ? TRUE : FALSE)
| tests if a USB device has been removed
#define | Host_ack_device_disconnection() (UHINT = ~(1<<DDISCI))
| acks device disconnection
#define | Host_enable_reset_interrupt() (UHIEN |= (1<<RSTE))
| enables host USB reset interrupt
#define | Host_disable_reset_interrupt() (UHIEN &= ~(1<<RSTE))
| disables host USB reset interrupt
#define | Is_host_reset_interrupt_enabled() ((UHIEN & (1<<RSTE)) ? TRUE : FALSE)
#define | Host_ack_reset() (UHINT = ~(1<<RSTI))
| acks host USB reset sent
#define | Is_host_reset() Host_is_reset()
| tests if USB reset has been sent
#define | Host_vbus_request() (OTGCON |= (1<<VBUSREQ))
| switches on VBus
#define | Host_clear_vbus_request() (OTGCON |= (1<<VBUSRQC))
| switches off VBus
#define | Host_configure_address(addr) (UHADDR = addr & MSK_HADDR)
| configures the address to use for the device
#define | Is_host_full_speed() ((USBSTA & (1<<SPEED)) ? TRUE : FALSE)
| Get connected device speed, returns TRUE when in full speed mode.
#define | Host_select_pipe(p) (UPNUM = (U8)p)
| selects pipe for CPU interface
#define | Host_get_selected_pipe() (UPNUM )
| get the currently selected pipe number
#define | Host_enable_pipe() (UPCONX |= (1<<PEN))
| enables pipe
#define | Host_disable_pipe() (UPCONX &= ~(1<<PEN))
| disables pipe
#define | Host_set_token_setup() (UPCFG0X = UPCFG0X & ~MSK_TOKEN_SETUP)
| sets SETUP token
#define | Host_set_token_in() (UPCFG0X = (UPCFG0X & ~MSK_TOKEN_SETUP) | MSK_TOKEN_IN)
| sets IN token
#define | Host_set_token_out() (UPCFG0X = (UPCFG0X & ~MSK_TOKEN_SETUP) | MSK_TOKEN_OUT)
| sets OUT token
#define | Host_get_endpoint_number() (UPCFG0X & (MSK_PEPNUM))
| returns the number of the endpoint associated to the current pipe
#define | Host_get_pipe_interrupt() (UPINT)
| returns pipe interrupt register
#define | Host_set_interrupt_frequency(frq) (UPCFG2X = (U8)frq)
| sets the interrupt frequency
#define | Is_pipe_configured() (UPSTAX & (1<<CFGOK))
| tests if current pipe is configured
#define | Is_host_one_bank_busy() ((UPSTAX & MSK_NBUSYBK) != 0)
| tests if at least one bank is busy
#define | Host_number_of_busy_bank() (UPSTAX & MSK_NBUSYBK)
| returns the number of busy banks
#define | Host_reset_pipe(p) (UPRST = 1<<p , UPRST = 0)
| resets the pipe
#define | Host_write_byte(dat) (UPDATX = dat)
| writes a byte into the pipe FIFO
#define | Host_read_byte() (UPDATX)
| reads a byte from the pipe FIFO
#define | Host_freeze_pipe() (UPCONX |= (1<<PFREEZE))
| freezes the pipe
#define | Host_unfreeze_pipe() (UPCONX &= ~(1<<PFREEZE))
| un-freezees the pipe
#define | Is_host_pipe_freeze() (UPCONX & (1<<PFREEZE))
| tests if the current pipe is frozen
#define | Host_reset_pipe_data_toggle() (UPCONX |= (1<<RSTDT) )
| resets data toggle
#define | Is_host_setup_sent() ((UPINTX & (1<<TXSTPI)) ? TRUE : FALSE)
| tests if SETUP has been sent
#define | Is_host_control_in_received() ((UPINTX & (1<<RXINI)) ? TRUE : FALSE)
| tests if control IN has been received
#define | Is_host_control_out_sent() ((UPINTX & (1<<TXOUTI)) ? TRUE : FALSE)
| tests if control OUT has been sent
#define | Is_host_stall() ((UPINTX & (1<<RXSTALLI)) ? TRUE : FALSE)
| tests if a STALL has been received
#define | Is_host_pipe_error() ((UPINTX & (1<<PERRI)) ? TRUE : FALSE)
| tests if an error occurs on current pipe
#define | Host_send_setup() (UPINTX &= ~(1<<FIFOCON))
| sends a setup
#define | Host_send_control_in() (UPINTX &= ~(1<<FIFOCON))
| sends a control IN
#define | Host_send_control_out() (UPINTX &= ~(1<<FIFOCON))
| sends a control OUT
#define | Host_ack_control_out() (UPINTX &= ~(1<<TXOUTI))
| acks control OUT
#define | Host_ack_control_in() (UPINTX &= ~(1<<RXINI))
| acks control IN
#define | Host_ack_setup() (UPINTX &= ~(1<<TXSTPI))
| acks setup
#define | Host_ack_stall() (UPINTX &= ~(1<<RXSTALLI))
| acks STALL reception
#define | Host_send_out() (UPINTX &= ~(1<<FIFOCON))
| sends a OUT
#define | Is_host_out_sent() ((UPINTX & (1<<TXOUTI)) ? TRUE : FALSE)
| tests if OUT has been sent
#define | Host_ack_out_sent() (UPINTX &= ~(1<<TXOUTI))
| acks OUT sent
#define | Is_host_in_received() ((UPINTX & (1<<RXINI)) ? TRUE : FALSE)
| tests if IN received
#define | Host_ack_in_received() (UPINTX &= ~(1<<RXINI))
| acks IN reception
#define | Host_send_in() (UPINTX &= ~(1<<FIFOCON))
| sends a IN
#define | Is_host_nak_received() ((UPINTX & (1<<NAKEDI)) ? TRUE : FALSE)
| tests if nak handshake has been received
#define | Host_ack_nak_received() (UPINTX &= ~(1<<NAKEDI))
| acks NAk received sent
#define | Is_host_read_enabled() (UPINTX&(1<<RWAL))
| tests if endpoint read allowed
#define | Is_host_write_enabled() (UPINTX&(1<<RWAL))
| tests if endpoint read allowed
#define | Host_standard_in_mode() (UPCONX &= ~(1<<INMODE))
| sets IN in standard mode
#define | Host_continuous_in_mode() (UPCONX |= (1<<INMODE))
| sets IN in continuous mode
#define | Host_in_request_number(in_num) (UPINRQX = (U8)in_num)
| sets number of IN requests to perform before freeze
#define | Host_get_in_request_number() (UPINRQX)
| returns number of remaining IN requests
#define | Host_data_length_U8() (UPBCLX)
| returns number of bytes (8 bits)
#define | Host_data_length_U16() ((((U16)UPBCHX)<<8) | UPBCLX)
| returns number of bytes (16 bits)
#define | Host_byte_counter() Host_data_length_U16()
| for device compatibility
#define | Host_byte_counter_8() Host_data_length_U8()
| for device compatibility
#define | Host_get_pipe_length() ((U16)0x08 << ((UPCFG1X & MSK_PSIZE)>>4))
| returns the size of the current pipe
#define | Host_get_pipe_type() (UPCFG0X>>6)
| returns the type of the current pipe
#define | Host_error_status() (UPERRX & MSK_ERROR)
| tests if error occurs on pipe
#define | Host_ack_all_errors() (UPERRX = 0x00)
| acks all pipe error
#define | Host_enable_transmit_interrupt() (UPIENX |= (1<<TXOUTE))
| Enable pipe end transmission interrupt.
#define | Host_disable_transmit_interrupt() (UPIENX &= ~(1<<TXOUTE))
| Disable pipe end transmission interrupt.
#define | Host_enable_receive_interrupt() (UPIENX |= (1<<RXINE))
| Enable pipe reception interrupt.
#define | Host_disable_receive_interrupt() (UPIENX &= ~(1<<RXINE))
| Disable pipe recption interrupt.
#define | Host_enable_stall_interrupt() (UPIENX |= (1<<RXSTALLE))
| Enable pipe stall interrupt.
#define | Host_disable_stall_interrupt() (UPIENX &= ~(1<<RXSTALLE))
| Disable pipe stall interrupt.
#define | Host_enable_error_interrupt() (UPIENX |= (1<<PERRE))
| Enable pipe error interrupt.
#define | Host_disable_error_interrupt() (UPIENX &= ~(1<<PERRE))
| Disable pipe error interrupt.
#define | Host_enable_nak_interrupt() (UPIENX |= (1<<NAKEDE))
| Enable pipe NAK interrupt.
#define | Host_disable_nak_interrupt() (UPIENX &= ~(1<<NAKEDE))
| Disable pipe NAK interrupt.
#define | Get_pipe_token(x) ((x & (0x80)) ? TOKEN_IN : TOKEN_OUT)
#define | wSWAP(x)
| wSWAP This macro swaps the U8 order in words.
#define | Usb_write_word_enum_struc(x) (wSWAP(x))
| Usb_write_word_enum_struc This macro help to fill the U16 fill in USB enumeration struct.
## Typedefs
typedef enum endpoint_parameter | t_endpoint_parameter
## Enumerations
enum | endpoint_parameter { ep_num, ep_type, ep_direction, ep_size, ep_bank, nyet_status }
## Functions
U8 | usb_config_ep (U8, U8)
| usb_configure_endpoint.
U8 | usb_select_enpoint_interrupt (void)
| usb_select_endpoint_interrupt.
U16 | usb_get_nb_byte_epw (void)
U8 | usb_send_packet (U8, U8 *, U8)
| usb_send_packet.
U8 | usb_read_packet (U8, U8 *, U8)
| usb_read_packet.
void | usb_halt_endpoint (U8)
| usb_halt_endpoint.
void | usb_reset_endpoint (U8)
U8 | usb_init_device (void)
| usb_init_device.
U8 | host_config_pipe (U8, U8)
| --------------------------------------------------------- ------------------ HOST --------------------------------- ---------------------------------------------------------
U8 | host_determine_pipe_size (U16)
| host_determine_pipe_size.
void | host_disable_all_pipe (void)
| host_disable_all_pipe.
U8 | usb_get_nb_pipe_interrupt (void)

## Detailed Description

This file contains the USB low level driver definition - Compiler: IAR EWAVR and GNU GCC for AVR

- Supported devices: AT90USB1287, AT90USB1286, AT90USB647, AT90USB646
  Author:
    Atmel Corporation: http://www.atmel.com
    Support and FAQ: http://support.atmel.no/

Definition in file usb_drv.h.

## Typedef Documentation

typedef enum endpoint_parameter t_endpoint_parameter

## Enumeration Type Documentation

enum endpoint_parameter

Enumerator:

  ep_num |
  ep_type |
  ep_direction |
  ep_size |
  ep_bank |
  nyet_status |

Definition at line 48 of file usb_drv.h.

    00048 {ep_num, ep_type, ep_direction, ep_size, ep_bank, nyet_status} t_endpoint_parameter;

## Function Documentation

U8 usb_config_ep | ( | U8 | config0,
|  | U8 | config1 |
| ) |  |  |

usb_configure_endpoint.

This function configures an endpoint with the selected type.

Parameters:

  | config0 |
  | config1 |

Returns:
  Is_endpoint_configured.

Definition at line 67 of file usb_drv.c.

References Is_endpoint_configured, Usb_allocate_memory, and Usb_enable_endpoint.

    00068 {
    00069     Usb_enable_endpoint();
    00070     UECFG0X = config0;
    00071     UECFG1X = (UECFG1X & (1<<ALLOC)) | config1;
    00072     Usb_allocate_memory();
    00073     return (Is_endpoint_configured());
    00074 }

U8 usb_select_enpoint_interrupt | ( | void |  | ) |

usb_select_endpoint_interrupt.

This function select the endpoint where an event occurs and returns the number of this endpoint. If no event occurs on the endpoints, this function returns 0.

Parameters:

  | none |

Returns:
  endpoint number.

Definition at line 87 of file usb_drv.c.

References ep_num, MAX_EP_NB, and Usb_interrupt_flags.

    00088 {
    00089 U8 interrupt_flags;
    00090 U8 ep_num;
    00091
    00092    ep_num = 0;
    00093    interrupt_flags = Usb_interrupt_flags();
    00094
    00095    while(ep_num < MAX_EP_NB)
    00096    {
    00097       if (interrupt_flags & 1)
    00098       {
    00099          return (ep_num);
    00100       }
    00101       else
    00102       {
    00103          ep_num++;
    00104          interrupt_flags = interrupt_flags >> 1;
    00105       }
    00106    }
    00107    return 0;
    00108 }

U16 usb_get_nb_byte_epw | ( | void |  | ) |

U8 usb_send_packet | ( | U8 | ep_num,
|  | U8 * | tbuf,
|  | U8 | data_length |
| ) |  |  |

usb_send_packet.

This function moves the data pointed by tbuf to the selected endpoint fifo and sends it through the USB.

Parameters:

  | ep_num | number of the addressed endpoint
  | *tbuf | address of the first data to send
  | data_length | number of bytes to send

Returns:
  address of the next U8 to send.

Example: usb_send_packet(3,&first_data,0x20); // send packet on the endpoint #3 while(!(Usb_tx_complete)); // wait packet ACK'ed by the Host Usb_clear_tx_complete(); // acknowledge the transmit

Note: tbuf is incremented of 'data_length'.

Definition at line 130 of file usb_drv.c.

References Is_usb_write_enabled, Usb_select_endpoint, and Usb_write_byte.

    00131 {
    00132 U8 remaining_length;
    00133
    00134    remaining_length = data_length;
    00135    Usb_select_endpoint(ep_num);
    00136    while(Is_usb_write_enabled() && (0 != remaining_length))
    00137    {
    00138       Usb_write_byte(*tbuf);
    00139       remaining_length--;
    00140       tbuf++;
    00141    }
    00142    return remaining_length;
    00143 }

U8 usb_read_packet | ( | U8 | ep_num,
|  | U8 * | rbuf,
|  | U8 | data_length |
| ) |  |  |

usb_read_packet.

This function moves the data stored in the selected endpoint fifo to the address specified by *rbuf.

Parameters:

  | ep_num | number of the addressed endpoint
  | *rbuf | aaddress of the first data to write with the USB data
  | data_length | number of bytes to read

Returns:
  address of the next U8 to send.

Example: while(!(Usb_rx_complete)); // wait new packet received usb_read_packet(4,&first_data,usb_get_nb_byte); // read packet from ep 4 Usb_clear_rx(); // acknowledge the transmit

Note: rbuf is incremented of 'data_length'.

Definition at line 165 of file usb_drv.c.

References Is_usb_read_enabled, Usb_read_byte, and Usb_select_endpoint.

    00166 {
    00167 U8 remaining_length;
    00168
    00169    remaining_length = data_length;
    00170    Usb_select_endpoint(ep_num);
    00171
    00172    while(Is_usb_read_enabled() && (0 != remaining_length))
    00173    {
    00174       *rbuf = Usb_read_byte();
    00175       remaining_length--;
    00176       rbuf++;
    00177    }
    00178    return remaining_length;
    00179 }

void usb_halt_endpoint | ( | U8 | ep_num | ) |

usb_halt_endpoint.

This function sends a STALL handshake for the next Host request. A STALL handshake will be send for each next request untill a SETUP or a Clear Halt Feature occurs for this endpoint.

Parameters:

  | ep_num | number of the addressed endpoint

Returns:
  none

Definition at line 191 of file usb_drv.c.

References Usb_enable_stall_handshake, and Usb_select_endpoint.

    00192 {
    00193    Usb_select_endpoint(ep_num);
    00194    Usb_enable_stall_handshake();
    00195 }

void usb_reset_endpoint | ( | U8 |  | ) |

U8 usb_init_device | ( | void |  | ) |

usb_init_device.

This function initializes the USB device controller and configures the Default Control Endpoint.

Parameters:

  | none |

Returns:
  status

Definition at line 207 of file usb_drv.c.

References DIRECTION_OUT, EP_CONTROL, FALSE, Is_usb_endpoint_enabled, Is_usb_id_device, NYET_DISABLED, ONE_BANK, SIZE_64, SIZE_8, TYPE_CONTROL, usb_configure_endpoint, Usb_select_device, and Usb_select_endpoint.

    00208 {
    00209    Usb_select_device();
    00210    if(Is_usb_id_device())
    00211    {
    00212       Usb_select_endpoint(EP_CONTROL);
    00213       if(!Is_usb_endpoint_enabled())
    00214       {
    00215 #if (USB_LOW_SPEED_DEVICE==DISABLE)
    00216          return usb_configure_endpoint(EP_CONTROL,    \
    00217                                 TYPE_CONTROL,  \
    00218                                 DIRECTION_OUT, \
    00219                                 SIZE_64,       \
    00220                                 ONE_BANK,      \
    00221                                 NYET_DISABLED);
    00222 #else
    00223          return usb_configure_endpoint(EP_CONTROL,    \
    00224                                 TYPE_CONTROL,  \
    00225                                 DIRECTION_OUT, \
    00226                                 SIZE_8,       \
    00227                                 ONE_BANK,      \
    00228                                 NYET_DISABLED);
    00229 #endif
    00230       }
    00231    }
    00232    return FALSE;
    00233 }

U8 host_config_pipe | ( | U8 | config0,
|  | U8 | config1 |
| ) |  |  |

--------------------------------------------------------- ------------------ HOST --------------------------------- ---------------------------------------------------------

usb_configure_pipe.

This function configures a pipe with the selected type.

Parameters:

  | config0 |
  | config1 |

Returns:
  Is_endpoint_configured.

Definition at line 252 of file usb_drv.c.

References Host_allocate_memory, Host_enable_pipe, and Is_pipe_configured.

    00253 {
    00254     Host_enable_pipe();
    00255     UPCFG0X = config0;
    00256     UPCFG1X = config1;
    00257     Host_allocate_memory();
    00258     return (Is_pipe_configured());
    00259 }

U8 host_determine_pipe_size | ( | U16 | size | ) |

host_determine_pipe_size.

This function returns the size configuration register value according to the endpint size detected inthe device enumeration process.

Returns:
  pipe size register value.

Definition at line 268 of file usb_drv.c.

References SIZE_1024, SIZE_128, SIZE_16, SIZE_256, SIZE_32, SIZE_512, SIZE_64, and SIZE_8.

    00269 {
    00270         if(size <= 8  ) {return (SIZE_8   );}
    00271    else if(size <= 16 ) {return (SIZE_16  );}
    00272    else if(size <= 32 ) {return (SIZE_32  );}
    00273    else if(size <= 64 ) {return (SIZE_64  );}
    00274    else if(size <= 128) {return (SIZE_128 );}
    00275    else if(size <= 256) {return (SIZE_256 );}
    00276    else if(size <= 512) {return (SIZE_512 );}
    00277    else                 {return (SIZE_1024);}
    00278
    00279 }

void host_disable_all_pipe | ( | void |  | ) |

host_disable_all_pipe.

This function disable all pipes for the host controller Usefull to execute upon device disconnection.

Returns:
  none.

Definition at line 288 of file usb_drv.c.

References Host_disable_pipe, Host_reset_pipe, Host_select_pipe, Host_unallocate_memory, and i.

    00289 {
    00290 U8 i;
    00291    for (i=0;i<7;i++)
    00292    {
    00293       Host_reset_pipe(i);
    00294       Host_select_pipe(i);
    00295       Host_unallocate_memory();
    00296       Host_disable_pipe();
    00297    }
    00298 }

U8 usb_get_nb_pipe_interrupt | ( | void |  | ) |

Returns the pipe number that generates a USB communication interrupt This function sould be called only when an interrupt has been detected. Otherwize the return value is incorect

Parameters:

  | none |

Returns:
  pipe_number

Definition at line 309 of file usb_drv.c.

References Host_get_pipe_interrupt, i, and MAX_EP_NB.

    00310 {
    00311 U8 interrupt_flags;
    00312 U8 i;
    00313
    00314    interrupt_flags = Host_get_pipe_interrupt();
    00315    for(i=0;i< MAX_EP_NB;i++)
    00316    {
    00317       if (interrupt_flags & (1<<i))
    00318       {
    00319          return (i);
    00320       }
    00321    }
    00322    // This return should never occurs ....
    00323    return MAX_EP_NB+1;
    00324 }