# AVR32 UC3064 - Pioc power Test Documentation

## Introduction

This is the documentation for the data structures, functions, variables, defines, enums, and typedefs for the AT32UC3L-PICO POWER project.
It also gives an example of usage of the SCIF , PM , GPIO , FLASHCDW module on UC3 products. This example shows the power consumption of the UC3L064 part in the following mode:

- Active mode,
- Idle mode,
- Static mode with RTC,
- Static mode without RTC.

## Compilation Info

This software was written for the GNU GCC for AVR32 and IAR Systems compiler for AVR32. Other compilers may or may not work.

## Device Info

All AVR32 devices with a PM module and a SCIF module can be used. This example has been tested with the following setup:

- AT32UC3L-PICO POWER board

## Setup Information

CPU speed:
Active mode: 50 MHz
Idle mode: 50 MHz
Static mode with RTC: 115 kHz start
SStatic mode without RTC: 115 kHz start

## Contact Info

For more info about Atmel AVR32 visit Atmel AVR32
Support and FAQ: http://support.atmel.no/