# scif_osc_opt_t Struct Reference

OSC0/OSC1 startup options. More...

`#include <scif_uc3l.h>`

## Data Fields
unsigned long | freq_hz
| The input frequency (from the external clock or the crystal).
unsigned char | gain
| Gain for the oscillator.
scif_osc_mode_t | mode
| Set the oscillator mode.
unsigned char | startup
| Specify the oscillator startup time.

## Detailed Description

OSC0/OSC1 startup options.

Definition at line 155 of file scif_uc3l.h.

## Field Documentation

unsigned long scif_osc_opt_t::freq_hz

The input frequency (from the external clock or the crystal).

Definition at line 158 of file scif_uc3l.h.

Referenced by scif_start_osc().

unsigned char scif_osc_opt_t::gain

Gain for the oscillator.

Definition at line 164 of file scif_uc3l.h.

Referenced by scif_start_osc().

scif_osc_mode_t scif_osc_opt_t::mode

Set the oscillator mode.

Definition at line 160 of file scif_uc3l.h.

Referenced by scif_start_osc().

unsigned char scif_osc_opt_t::startup

Specify the oscillator startup time.

Definition at line 162 of file scif_uc3l.h.

Referenced by scif_start_osc().