# scif_osc32_opt_t Struct Reference

OSC32 startup options. More...

`#include <scif_uc3l.h>`

## Data Fields
bool | en1k
| 1kHz output enable/disable
bool | en32k
| 32kHz output enable/disable
scif_osc_mode_t | mode
| Set the oscillator mode.
bool | pinsel
| Select pins used for the 32kHz Crystal.
unsigned char | startup
| Specify the oscillator startup time.

## Detailed Description

OSC32 startup options.

Definition at line 168 of file scif_uc3l.h.

## Field Documentation

bool scif_osc32_opt_t::en1k

1kHz output enable/disable

Definition at line 177 of file scif_uc3l.h.

Referenced by scif_start_osc32().

bool scif_osc32_opt_t::en32k

32kHz output enable/disable

Definition at line 179 of file scif_uc3l.h.

Referenced by scif_start_osc32().

scif_osc_mode_t scif_osc32_opt_t::mode

Set the oscillator mode.

Definition at line 171 of file scif_uc3l.h.

Referenced by scif_start_osc32().

bool scif_osc32_opt_t::pinsel

Select pins used for the 32kHz Crystal.

Definition at line 175 of file scif_uc3l.h.

Referenced by scif_start_osc32().

unsigned char scif_osc32_opt_t::startup

Specify the oscillator startup time.

Definition at line 173 of file scif_uc3l.h.

Referenced by scif_start_osc32().