#-- Synopsys, Inc.
#-- Version D-2009.12A
#-- Project file \\idm\CAE\pavan m\USB\USBeee\Using_Fabric_Master\HW_USBee\synthesis\synthesis_1\run_options.txt
#-- Written on Sun Jul 18 21:43:58 2010


#project files
add_file -vhdl -lib work "//idm/CAE/pavan m/USB/USBeee/Using_Fabric_Master/HW_USBee/component/Actel/SmartFusionMSS/MSS/2.0.100/mss_comps.vhd"
add_file -vhdl -lib work "//idm/CAE/pavan m/USB/USBeee/Using_Fabric_Master/HW_USBee/component/work/usb_mss/MSS_CCC_0/usb_mss_tmp_MSS_CCC_0_MSS_CCC.vhd"
add_file -vhdl -lib work "//idm/CAE/pavan m/USB/USBeee/Using_Fabric_Master/HW_USBee/component/work/usb_mss/usb_mss.vhd"
add_file -vhdl -lib work "//idm/CAE/pavan m/USB/USBeee/Using_Fabric_Master/HW_USBee/smartgen/Fifo_1024/Fifo_1024.vhd"
add_file -vhdl -lib work "//idm/CAE/pavan m/USB/USBeee/Using_Fabric_Master/HW_USBee/hdl/usb_slave.vhd"
add_file -vhdl -lib work "//idm/CAE/pavan m/USB/USBeee/Using_Fabric_Master/HW_USBee/component/work/usbee_top_level/usbee_top_level.vhd"


#implementation: "synthesis_1"
impl -add synthesis_1 -type fpga

#par_1 attributes
set_option -job par_1 -add par
set_option -job par_1 -option run_backannotation 0

#device options
set_option -technology ProASIC3E
set_option -part A3PE600
set_option -package FBGA256
set_option -speed_grade Std
set_option -part_companion ""

#compilation/mapping options
set_option -use_fsm_explorer 0
set_option -top_module "work.usbee_top_level"

# mapper_options
set_option -frequency 1
set_option -write_verilog 0
set_option -write_vhdl 0
set_option -identify_debug_mode 1

# Actel 500K
set_option -run_prop_extract 1
set_option -maxfan 24
set_option -maxfan_hard3 0
set_option -disable_io_insertion 0
set_option -retiming 0
set_option -report_path 0
set_option -opcond COMWC
set_option -update_models_cp 0
set_option -preserve_registers 0

# Actel 500K
set_option -globalthreshold 50

# NFilter
set_option -popfeed 0
set_option -constprop 0
set_option -createhierarchy 0

# sequential_optimization_options
set_option -symbolic_fsm_compiler 1

# Compiler Options
set_option -compiler_compatible 0
set_option -resource_sharing 1

#automatic place and route (vendor) options
set_option -write_apr_constraint 1

#set result format/file last
project -result_file "//idm/CAE/pavan m/USB/USBeee/Using_Fabric_Master/HW_USBee/synthesis/synthesis_1/usbee_top_level.edn"
impl -active "synthesis_1"
