Resource Usage Report for MC_System_top 

Mapping to part: m2s010fbga484-1
Cell usage:
CCC             1 use
CLKINT          2 uses
MSS_010         1 use
RCOSC_25_50MHZ  1 use
CFG1           10 uses
CFG2           458 uses
CFG3           778 uses
CFG4           708 uses

Carry cells:
ARI1            1358 uses - used for arithmetic functions
ARI1            172 uses - used for Wide-Mux implementation
Total ARI1      1530 uses


Sequential Cells: 
SLE            2543 uses

DSP Blocks:    8 of 22 (36%)
 MACC:         3 Mults
 MACC:         5 MultAdds

I/O ports: 27
I/O primitives: 26
BIBUF          8 uses
INBUF          6 uses
OUTBUF         11 uses
TRIBUFF        1 use


Global Clock Buffers: 2 of 8 (25%)


Total LUTs:    3484

Extra resources required for RAM and MACC interface logic during P&R:

RAM64x18 Interface Logic : SLEs = 0; LUTs = 0;
RAM1K18  Interface Logic : SLEs = 0; LUTs = 0;
MACC     Interface Logic : SLEs = 288; LUTs = 288;

Total number of SLEs after P&R:  2543 + 0 + 0 + 288 = 2831;
Total number of LUTs after P&R:  3484 + 0 + 0 + 288 = 3772;

