`

    #Build: Synplify Pro I-2013.09M-SP1 , Build 034R, Jan 17 2014
    #install: C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1
    #OS: Windows 7 6.1
    #Hostname: W764-PINNINTIA

    #Implementation: synthesis

    $ Start of Compile
    #Thu Aug 07 15:16:55 2014

    Synopsys VHDL Compiler, version comp201309rcp1, Build 078R, built Jan 14 2014
    @N: :  | Running in 64-bit mode
    Copyright (C) 1994-2013 Synopsys, Inc. This software and the associated documentation are proprietary to Synopsys, Inc. This software may only be used in accordance with the terms and conditions of a written license agreement with Synopsys, Inc.  All other use or distribution of the software is strictly prohibited.

    @N:CD720 : std.vhd(146) | Setting time resolution to ns
    @N: : mas.vhd(35) | Top entity is set to mas.
    Options changed - recompiling
    VHDL syntax check successful!
    Options changed - recompiling
    @N:CD231 : std1164.vhd(913) | Using onehot encoding for type mvl9plus ('U'="1000000000")
    @N:CD630 : mas.vhd(35) | Synthesizing work.mas.mas
    @W:CG296 : mas.vhd(107) | Incomplete sensitivity list - assuming completeness
    @W:CG290 : mas.vhd(109) | Referenced variable s_reset_state is not in sensitivity list
    @W:CG296 : mas.vhd(152) | Incomplete sensitivity list - assuming completeness
    @W:CG290 : mas.vhd(154) | Referenced variable s_reset_state is not in sensitivity list
    @W:CD796 : mas.vhd(65) | Bit 1 of signal mas_done_sync is undriven. Possible simulation mismatch as initial value or default value is ignored. To avoid simulation mismatches, explicitly drive this bit.
    @W:CD796 : mas.vhd(65) | Bit 2 of signal mas_done_sync is undriven. Possible simulation mismatch as initial value or default value is ignored. To avoid simulation mismatches, explicitly drive this bit.
    Post processing for work.mas.mas
    @END

    At c_vhdl Exit (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 73MB peak: 73MB)

    Process took 0h:00m:01s realtime, 0h:00m:01s cputime
    # Thu Aug 07 15:16:55 2014

    ###########################################################]
    Pre-mapping Report

    Synopsys Generic Technology Pre-mapping, Version mapact, Build 1154R, Built Jan 20 2014 10:24:19
    Copyright (C) 1994-2013, Synopsys, Inc. This software and the associated documentation are proprietary to Synopsys, Inc. This software may only be used in accordance with the terms and conditions of a written license agreement with Synopsys, Inc.  All other use or distribution of the software is strictly prohibited.
    Product Version I-2013.09M-SP1

    Mapper Startup Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 99MB)

    Linked File: mas_scck.rpt
    Printing clock  summary report in "D:\MS_MC_single_axis\synthesis\mas_scck.rpt" file
    @N:MF248 :  | Running in 64-bit mode.
    @N:MF667 :  | Clock conversion disabled

    Design Input Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 102MB)

    Mapper Initialization Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 102MB)

    @N:BN133 :  | Ignoring syn_hier=hard property on top-level design.

    Start loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 100MB peak: 102MB)

    Finished loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 100MB peak: 102MB)

    syn_allowed_resources : blockrams=69,dsps=72  set on top level netlist mas

    Clock Summary
    **************

    Start             Requested     Requested     Clock        Clock
    Clock             Frequency     Period        Type         Group
    ------------------------------------------------------------------------------
    mas|sys_clk_i     100.0 MHz     10.000        inferred     Inferred_clkgroup_0
    ==============================================================================

    @W:MT530 : mas.vhd(154) | Found inferred clock mas|sys_clk_i which controls 46 sequential elements including product_o[43:0]. This clock has no specified timing constraint which may adversely impact design performance.

    Finished Pre Mapping Phase.
    @N:BN225 :  | Writing default property annotation file D:\MS_MC_single_axis\synthesis\mas.sap.
    Pre-mapping successful!

    At Mapper Exit (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 68MB peak: 132MB)

    Process took 0h:00m:01s realtime, 0h:00m:01s cputime
    # Thu Aug 07 15:16:57 2014

    ###########################################################]
    Map & Optimize Report

    Synopsys Generic Technology Mapper, Version mapact, Build 1154R, Built Jan 20 2014 10:24:19
    Copyright (C) 1994-2013, Synopsys, Inc. This software and the associated documentation are proprietary to Synopsys, Inc. This software may only be used in accordance with the terms and conditions of a written license agreement with Synopsys, Inc.  All other use or distribution of the software is strictly prohibited.
    Product Version I-2013.09M-SP1

    Mapper Startup Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 99MB)

    @N:MF248 :  | Running in 64-bit mode.
    @N:MF667 :  | Clock conversion disabled

    Design Input Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 100MB)

    Mapper Initialization Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 100MB)

    Start loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 100MB peak: 101MB)

    Finished loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 100MB peak: 103MB)

    Starting Optimization and Mapping (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 130MB peak: 132MB)

    Available hyper_sources - for debug and ip models
    	None Found

    Finished RTL optimizations (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 130MB peak: 132MB)

    Finished factoring (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 131MB peak: 132MB)

    Finished gated-clock and generated-clock conversion (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 131MB peak: 132MB)

    Finished generic timing optimizations - Pass 1 (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 132MB peak: 132MB)

    Starting Early Timing Optimization (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 132MB peak: 132MB)

    Finished Early Timing Optimization (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 132MB peak: 132MB)

    Finished generic timing optimizations - Pass 2 (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 132MB peak: 132MB)

    Finished preparing to map (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 132MB peak: 132MB)

    Finished technology mapping (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 131MB peak: 132MB)

    Pass		 CPU time		Worst Slack		Luts / Registers
    ------------------------------------------------------------
    Pass		 CPU time		Worst Slack		Luts / Registers
    ------------------------------------------------------------
    ------------------------------------------------------------

    Added 0 Buffers
    Added 0 Cells via replication
    	Added 0 Sequential Cells via replication
    	Added 0 Combinational Cells via replication

    Finished technology timing optimizations and critical path resynthesis (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 131MB peak: 132MB)

    Finished restoring hierarchy (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 131MB peak: 132MB)

    #### START OF CLOCK OPTIMIZATION REPORT #####[

    Clock optimization not enabled
    1 non-gated/non-generated clock tree(s) driving 4 clock pin(s) of sequential element(s)
    0 gated/generated clock tree(s) driving 0 clock pin(s) of sequential element(s)
    0 instances converted, 0 sequential instances remain driven by gated/generated clocks

    ====================================== Non-Gated/Non-Generated Clocks ======================================
    Clock Tree ID     Driving Element     Drive Element Type     Fanout     Sample Instance
    ------------------------------------------------------------------------------------------------------------
    ClockId0001        sys_clk_i           port                   4          op_mult.un3_product_o_muladd_0[35:0]
    ============================================================================================================

    ##### END OF CLOCK OPTIMIZATION REPORT ######]

    Writing Analyst data base D:\MS_MC_single_axis\synthesis\mas.srm

    Finished Writing Netlist Databases (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 130MB peak: 132MB)

    Writing EDIF Netlist and constraint files
    @N:BW103 :  | Synopsys Constraint File time units using default value of 1ns
    @N:BW107 :  | Synopsys Constraint File capacitance units using default value of 1pF
    I-2013.09M-SP1

    Finished Writing EDIF Netlist and constraint files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 131MB peak: 133MB)

    @W:MT246 : mas.vhd(158) | Blackbox MACC is missing a user supplied timing model. This may have a negative effect on timing analysis and optimizations (Quality of Results)
    @W:MT420 :  | Found inferred clock mas|sys_clk_i with period 10.00ns. Please declare a user-defined clock on object "p:sys_clk_i"

    ##### START OF TIMING REPORT #####[
    # Timing Report written on Thu Aug 07 15:16:58 2014
    #

    Top view:               mas
    Requested Frequency:    100.0 MHz
    Wire load mode:         top
    Paths requested:        5
    Constraint File(s):
    @N:MT320 :  | Timing report estimates place and route data. Please look at the place and route timing report for final timing.

    @N:MT322 :  | Clock constraints cover only FF-to-FF paths associated with the clock.

    Performance Summary
    *******************

    Worst slack in design: 8.972

                       Requested     Estimated     Requested     Estimated               Clock        Clock
    Starting Clock     Frequency     Frequency     Period        Period        Slack     Type         Group
    ---------------------------------------------------------------------------------------------------------------------
    mas|sys_clk_i      100.0 MHz     972.8 MHz     10.000        1.028         8.972     inferred     Inferred_clkgroup_0
    System             100.0 MHz     NA            10.000        NA            NA        system       system_clkgroup
    =====================================================================================================================

    Clock Relationships
    *******************

    Clocks                        |    rise  to  rise   |    fall  to  fall   |    rise  to  fall   |    fall  to  rise
    --------------------------------------------------------------------------------------------------------------------
    Starting       Ending         |  constraint  slack  |  constraint  slack  |  constraint  slack  |  constraint  slack
    --------------------------------------------------------------------------------------------------------------------
    mas|sys_clk_i  mas|sys_clk_i  |  10.000      8.972  |  No paths    -      |  No paths    -      |  No paths    -
    ====================================================================================================================
     Note: 'No paths' indicates there are no paths in the design for that pair of clock edges.
           'Diff grp' indicates that paths exist but the starting clock and ending clock are in different clock groups.

    Interface Information
    *********************

    No IO constraint found

    ====================================
    Detailed Report for Clock: mas|sys_clk_i
    ====================================

    Starting Points with Worst Slack
    ********************************

                         Starting                                                Arrival
    Instance             Reference         Type     Pin     Net                  Time        Slack
                         Clock
    ----------------------------------------------------------------------------------------------
    mas_done_sync[0]     mas|sys_clk_i     SLE      Q       mas_done_sync[0]     0.087       8.972
    ==============================================================================================

    Ending Points with Worst Slack
    ******************************

                   Starting                                                Required
    Instance       Reference         Type     Pin     Net                  Time         Slack
                   Clock
    -----------------------------------------------------------------------------------------
    mas_done_o     mas|sys_clk_i     SLE      D       mas_done_sync[0]     9.745        8.972
    =========================================================================================

    Worst Path Information
    View Worst Path in Analyst
    ***********************

    Path information for path number 1:
          Requested Period:                      10.000
        - Setup time:                            0.255
        + Clock delay at ending point:           0.000 (ideal)
        = Required time:                         9.745

        - Propagation time:                      0.773
        - Clock delay at starting point:         0.000 (ideal)
        = Slack (critical) :                     8.972

        Number of logic level(s):                0
        Starting point:                          mas_done_sync[0] / Q
        Ending point:                            mas_done_o / D
        The start point is clocked by            mas|sys_clk_i [rising] on pin CLK
        The end   point is clocked by            mas|sys_clk_i [rising] on pin CLK

    Instance / Net                Pin      Pin               Arrival     No. of
    Name                 Type     Name     Dir     Delay     Time        Fan Out(s)
    -------------------------------------------------------------------------------
    mas_done_sync[0]     SLE      Q        Out     0.087     0.087       -
    mas_done_sync[0]     Net      -        -       0.685     -           1
    mas_done_o           SLE      D        In      -         0.773       -
    ===============================================================================
    Total path delay (propagation time + setup) of 1.028 is 0.343(33.3%) logic and 0.685(66.7%) route.
    Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value

    ##### END OF TIMING REPORT #####]

    ---------------------------------------
    Resource Usage Report for mas

    Mapping to part: m2s050t_esfbga896std
    Cell usage:

    Sequential Cells:
    SLE            2 uses

    DSP Blocks:    1
     MACC:         1 MultAddSub

    Total LUTs:    0

    Mapper successful!

    At Mapper Exit (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:00s; Memory used current: 47MB peak: 133MB)

    Process took 0h:00m:01s realtime, 0h:00m:01s cputime
    # Thu Aug 07 15:16:59 2014

    ###########################################################]

`