*****************************************************************
Pin Report - Date: Wed Nov 29 16:02:45 2017 Pinchecksum: NOT-AVAILABLE
Product: Designer
Release: Libero SoC v11.8 SP2
Version: 11.8.2.4
Design Name: MC_System_top
Family: SmartFusion2
Die: M2S010
Package: 484 FBGA
*****************************************************************

Port             |Pin  |Fixed |Function                                     |Bank     |I/O Std   |Direction                      |I/O state in Flash*Freeze mode |Resistor Pull                      |I/O available in Flash*Freeze mode |Schmitt Trigger |Odt_Static    |Odt Imp (Ohm)  |Low Power Exit |Input Delay |Slew         |Pre-Emphasis      |Output Drive (mA) |Output Load (pF) |
-----------------|-----|------|---------------------------------------------|---------|----------|-------------------------------|-------------------------------|-----------------------------------|-----------------------------------|----------------|--------------|---------------|---------------|------------|-------------|------------------|------------------|-----------------|
A0_ADC_CS_O       F20   Yes    MSIO23NB1/MMUART_0_DTR/GPIO_18_B/USB_DATA6_C  Bank1     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
A0_ADC_SCK_O      F21   Yes    MSIO23PB1/MMUART_0_RTS/GPIO_17_B/USB_DATA5_C  Bank1     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
A0_ADC_SDI_I      K21   Yes    MSIO17PB2/SPI_1_SS6/GPIO_23_A                 Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
A0_ADC_SDO_O      K20   Yes    MSIO17NB2/SPI_1_SS7/GPIO_24_A                 Bank2     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
A0_PWM_UH_O       E4    Yes    MSIO70PB7                                     Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
A0_PWM_UL_O       F6    Yes    MSIO67NB7                                     Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
A0_PWM_VH_O       H7    Yes    MSIO75PB7                                     Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
A0_PWM_VL_O       K7    Yes    MSIO81NB7                                     Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
A0_PWM_WH_O       G7    Yes    MSIO75NB7                                     Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
A0_PWM_WL_O       J6    Yes    MSIO76NB7                                     Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
A0_RUNNING_LED    AB18  Yes    MSIO118PB4                                    Bank4     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
GPIO_0_M2F        L19   Yes    MSIO16PB2/SPI_1_SS4/GPIO_17_A                 Bank2     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
GPIO_41           K17   Yes    MSIO19PB2/SPI_0_SS3/GPIO_10_A/USB_DATA7_A     Bank2     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
GPIO_43           F18   Yes    MSIO24NB1/MMUART_0_DSR/GPIO_20_B              Bank1     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                12                 5                 
PPS               AA16  Yes    MSIO114PB4                                    Bank4     LVCMOS25   Input                           TRISTATE                        Up                                  No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
TD                AA17  Yes    MSIO114NB4                                    Bank4     LVCMOS25   Input                           TRISTATE                        Up                                  No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
USB_ULPI_DATA[0]  V22   Yes    MSIO3PB2/USB_DATA0_B                          Bank2     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
USB_ULPI_DATA[1]  V21   Yes    MSIO3NB2/USB_DATA1_B                          Bank2     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
USB_ULPI_DATA[2]  U22   Yes    MSIO4PB2/USB_DATA2_B                          Bank2     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
USB_ULPI_DATA[3]  U21   Yes    MSIO4NB2/USB_DATA3_B                          Bank2     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
USB_ULPI_DATA[4]  T20   Yes    MSIO5PB2/USB_DATA4_B                          Bank2     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
USB_ULPI_DATA[5]  T21   Yes    MSIO5NB2/USB_DATA5_B                          Bank2     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
USB_ULPI_DATA[6]  P17   Yes    MSIO6PB2/USB_DATA6_B                          Bank2     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
USB_ULPI_DATA[7]  V19   Yes    MSIO0NB2/USB_DATA7_B                          Bank2     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
USB_ULPI_DIR      R18   Yes    MSIO1NB2/USB_DIR_B                            Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
USB_ULPI_NXT      T19   Yes    MSIO2NB2/USB_NXT_B                            Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
USB_ULPI_STP      T18   Yes    MSIO2PB2/USB_STP_B                            Bank2     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
USB_ULPI_XCLK     R17   Yes    MSIO1PB2/USB_XCLK_B                           Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
