Resource Usage Report for MC_System_top 

Mapping to part: m2s010fbga484-1
Cell usage:
CCC             1 use
CLKINT          3 uses
MSS_010         1 use
RCOSC_25_50MHZ  1 use
CFG1           52 uses
CFG2           1084 uses
CFG3           1567 uses
CFG4           1564 uses

Carry cells:
ARI1            2424 uses - used for arithmetic functions
ARI1            144 uses - used for Wide-Mux implementation
Total ARI1      2568 uses


Sequential Cells: 
SLE            4578 uses

DSP Blocks:   12 of 22 (54%)
 MACC:         9 MultAdds
 MACC:         3 Mults

I/O ports: 36
I/O primitives: 35
BIBUF          8 uses
INBUF          5 uses
OUTBUF         21 uses
TRIBUFF        1 use


Global Clock Buffers: 3 of 8 (37%)


Total LUTs:    6835

Extra resources required for RAM and MACC interface logic during P&R:

RAM64x18 Interface Logic : SLEs = 0; LUTs = 0;
RAM1K18  Interface Logic : SLEs = 0; LUTs = 0;
MACC     Interface Logic : SLEs = 432; LUTs = 432;

Total number of SLEs after P&R:  4578 + 0 + 0 + 432 = 5010;
Total number of LUTs after P&R:  6835 + 0 + 0 + 432 = 7267;

