

##### START OF TIMING REPORT #####[
# Timing Report written on Mon Apr 23 19:46:48 2012
#


Top view:               Voltage_Monitor
Operating conditions:   smartfusion.COMWC-2
Requested Frequency:    100.0 MHz
Wire load mode:         top
Wire load model:        smartfusion
Paths requested:        5
Constraint File(s):    
@N: MT320 |This timing report estimates place and route data. Please look at the place and route timing report for final timing.

@N: MT322 |Clock constraints cover only FF-to-FF paths associated with the clock.



Performance Summary 
*******************


Worst slack in design: 4.357

                   Requested     Estimated     Requested     Estimated               Clock      Clock          
Starting Clock     Frequency     Frequency     Period        Period        Slack     Type       Group          
---------------------------------------------------------------------------------------------------------------
System             100.0 MHz     224.5 MHz     10.000        4.453         5.547     system     system_clkgroup
===============================================================================================================



Clock Relationships
*******************

Clocks            |    rise  to  rise   |    fall  to  fall   |    rise  to  fall   |    fall  to  rise 
--------------------------------------------------------------------------------------------------------
Starting  Ending  |  constraint  slack  |  constraint  slack  |  constraint  slack  |  constraint  slack
--------------------------------------------------------------------------------------------------------
System    System  |  0.000       4.357  |  No paths    -      |  No paths    -      |  No paths    -    
========================================================================================================
 Note: 'No paths' indicates there are no paths in the design for that pair of clock edges.
       'Diff grp' indicates that paths exist but the starting clock and ending clock are in different clock groups.



Interface Information 
*********************

No IO constraint found



====================================
Detailed Report for Clock: System
====================================



Starting Points with Worst Slack
********************************

                                         Starting                                                  Arrival          
Instance                                 Reference     Type        Pin         Net                 Time        Slack
                                         Clock                                                                      
--------------------------------------------------------------------------------------------------------------------
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     System        MSS_APB     GPO[28]     MSSINT_GPO_28_A     4.132       4.453
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     System        MSS_APB     GPO[29]     MSSINT_GPO_29_A     4.132       4.453
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     System        MSS_APB     GPO[30]     MSSINT_GPO_30_A     4.132       4.453
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     System        MSS_APB     GPO[31]     MSSINT_GPO_31_A     4.132       4.453
====================================================================================================================


Ending Points with Worst Slack
******************************

                                        Starting                                             Required          
Instance                                Reference     Type       Pin     Net                 Time         Slack
                                        Clock                                                                  
---------------------------------------------------------------------------------------------------------------
Voltage_Monitor_MSS_0.MSSINT_GPO_28     System        MSSINT     A       MSSINT_GPO_28_A     0.000        4.357
Voltage_Monitor_MSS_0.MSSINT_GPO_29     System        MSSINT     A       MSSINT_GPO_29_A     0.000        4.357
Voltage_Monitor_MSS_0.MSSINT_GPO_30     System        MSSINT     A       MSSINT_GPO_30_A     0.000        4.357
Voltage_Monitor_MSS_0.MSSINT_GPO_31     System        MSSINT     A       MSSINT_GPO_31_A     0.000        4.357
===============================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
    Propagation time:                        4.357
    + Clock delay at starting point:         0.000 (ideal)
-0.000
    - Requested Period:                      0.000
    - Hold time:                             0.000
    - Clock delay at ending point:           0.000 (ideal)
0.000
    = Slack (critical) :                     4.357

    Number of logic level(s):                0
    Starting point:                          Voltage_Monitor_MSS_0.MSS_ADLIB_INST / GPO[28]
    Ending point:                            Voltage_Monitor_MSS_0.MSSINT_GPO_28 / A
    The start point is clocked by            System [rising] on pin FCLK
    The end   point is clocked by            System [rising]

Instance / Net                                       Pin         Pin               Arrival     No. of    
Name                                     Type        Name        Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------------------------------
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     MSS_APB     GPO[28]     Out     4.132     4.132       -         
MSSINT_GPO_28_A                          Net         -           -       0.225     -           1         
Voltage_Monitor_MSS_0.MSSINT_GPO_28      MSSINT      A           In      -         4.357       -         
=========================================================================================================



##### END OF TIMING REPORT #####]

