@W: MO111 :"c:\sf_libero_keil_potlevel_tut_df\dev_kit\pot_led_libero_keil\voltage_monitor\component\work\voltage_monitor_mss\mss_ccc_0\voltage_monitor_mss_tmp_mss_ccc_0_mss_ccc.v":64:7:64:18|Tristate driver LPXIN_CLKOUT on net LPXIN_CLKOUT has its enable tied to GND (module Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC) 
@W: MO111 :"c:\sf_libero_keil_potlevel_tut_df\dev_kit\pot_led_libero_keil\voltage_monitor\component\work\voltage_monitor_mss\mss_ccc_0\voltage_monitor_mss_tmp_mss_ccc_0_mss_ccc.v":63:7:63:20|Tristate driver MAINXIN_CLKOUT on net MAINXIN_CLKOUT has its enable tied to GND (module Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC) 
@W: MO111 :"c:\sf_libero_keil_potlevel_tut_df\dev_kit\pot_led_libero_keil\voltage_monitor\component\work\voltage_monitor_mss\mss_ccc_0\voltage_monitor_mss_tmp_mss_ccc_0_mss_ccc.v":62:7:62:18|Tristate driver RCOSC_CLKOUT on net RCOSC_CLKOUT has its enable tied to GND (module Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC) 
@W: MT246 :"c:\sf_libero_keil_potlevel_tut_df\dev_kit\pot_led_libero_keil\voltage_monitor\component\work\voltage_monitor_mss\voltage_monitor_mss.v":453:7:453:19|Blackbox MSSINT is missing a user supplied timing model. This may have a negative effect on timing analysis and optimizations (Quality of Results) 
