

##### START OF TIMING REPORT #####[
# Timing Report written on Tue Nov 20 15:18:12 2012
#


Top view:               Voltage_Monitor
Operating conditions:   smartfusion.COMWC-2
Requested Frequency:    100.0 MHz
Wire load mode:         top
Wire load model:        smartfusion
Paths requested:        5
Constraint File(s):    
@N: MT320 |Timing report estimates place and route data. Please look at the place and route timing report for final timing.

@N: MT322 |Clock constraints cover only FF-to-FF paths associated with the clock.



Performance Summary 
*******************


Worst slack in design: 0.225

                   Requested     Estimated     Requested     Estimated               Clock      Clock          
Starting Clock     Frequency     Frequency     Period        Period        Slack     Type       Group          
---------------------------------------------------------------------------------------------------------------
System             100.0 MHz     171.5 MHz     10.000        5.831         4.169     system     system_clkgroup
===============================================================================================================



Clock Relationships
*******************

Clocks            |    rise  to  rise   |    fall  to  fall   |    rise  to  fall   |    fall  to  rise 
--------------------------------------------------------------------------------------------------------
Starting  Ending  |  constraint  slack  |  constraint  slack  |  constraint  slack  |  constraint  slack
--------------------------------------------------------------------------------------------------------
System    System  |  0.000       0.225  |  No paths    -      |  No paths    -      |  No paths    -    
========================================================================================================
 Note: 'No paths' indicates there are no paths in the design for that pair of clock edges.
       'Diff grp' indicates that paths exist but the starting clock and ending clock are in different clock groups.



Interface Information 
*********************

No IO constraint found



====================================
Detailed Report for Clock: System
====================================



Starting Points with Worst Slack
********************************

                                            Starting                                                        Arrival          
Instance                                    Reference     Type        Pin         Net                       Time        Slack
                                            Clock                                                                            
-----------------------------------------------------------------------------------------------------------------------------
Voltage_Monitor_MSS_0.MSS_ACE_0_TM0         System        INBUF_A     Y           MSS_ACE_0_TM0_Y           0.000       0.322
Voltage_Monitor_MSS_0.MSS_ACE_0_VAREF0      System        INBUF_A     Y           MSS_ACE_0_VAREF0_Y        0.000       0.322
Voltage_Monitor_MSS_0.MSS_ADLIB_INST        System        MSS_APB     EMCCLK      MSS_ADLIB_INST_EMCCLK     0.000       0.322
Voltage_Monitor_MSS_0.MSS_ADLIB_INST        System        MSS_APB     GPO[28]     MSSINT_GPO_28_A           0.000       0.322
Voltage_Monitor_MSS_0.MSS_ADLIB_INST        System        MSS_APB     GPO[29]     MSSINT_GPO_29_A           0.000       0.322
Voltage_Monitor_MSS_0.MSS_ADLIB_INST        System        MSS_APB     GPO[30]     MSSINT_GPO_30_A           0.000       0.322
Voltage_Monitor_MSS_0.MSS_ADLIB_INST        System        MSS_APB     GPO[31]     MSSINT_GPO_31_A           0.000       0.322
Voltage_Monitor_MSS_0.MSS_CCC_0.I_RCOSC     System        RCOSC       CLKOUT      N_CLKA_RCOSC              0.000       5.509
=============================================================================================================================


Ending Points with Worst Slack
******************************

                                         Starting                                                           Required          
Instance                                 Reference     Type        Pin           Net                        Time         Slack
                                         Clock                                                                                
------------------------------------------------------------------------------------------------------------------------------
Voltage_Monitor_MSS_0.MSSINT_GPO_28      System        MSSINT      A             MSSINT_GPO_28_A            0.000        0.225
Voltage_Monitor_MSS_0.MSSINT_GPO_29      System        MSSINT      A             MSSINT_GPO_29_A            0.000        0.225
Voltage_Monitor_MSS_0.MSSINT_GPO_30      System        MSSINT      A             MSSINT_GPO_30_A            0.000        0.225
Voltage_Monitor_MSS_0.MSSINT_GPO_31      System        MSSINT      A             MSSINT_GPO_31_A            0.000        0.225
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     System        MSS_APB     EMCCLKRTN     MSS_ADLIB_INST_EMCCLK      0.000        0.225
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     System        MSS_APB     TM0           MSS_ACE_0_TM0_Y            0.000        0.225
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     System        MSS_APB     VAREF0        MSS_ACE_0_VAREF0_Y         0.000        0.225
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     System        MSS_APB     FCLK          MSS_ADLIB_INST_FCLK        0.000        5.317
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     System        MSS_APB     PLLLOCK       MSS_ADLIB_INST_PLLLOCK     0.000        5.638
==============================================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
    Propagation time:                        0.225
    + Clock delay at starting point:         0.000 (ideal)
-0.000
    - Requested Period:                      0.000
    - Hold time:                             0.000
    - Clock delay at ending point:           0.000 (ideal)
0.000
    = Slack (critical) :                     0.225

    Number of logic level(s):                0
    Starting point:                          Voltage_Monitor_MSS_0.MSS_ACE_0_TM0 / Y
    Ending point:                            Voltage_Monitor_MSS_0.MSS_ADLIB_INST / TM0
    The start point is clocked by            System [rising]
    The end   point is clocked by            System [rising]

Instance / Net                                       Pin      Pin               Arrival     No. of    
Name                                     Type        Name     Dir     Delay     Time        Fan Out(s)
------------------------------------------------------------------------------------------------------
Voltage_Monitor_MSS_0.MSS_ACE_0_TM0      INBUF_A     Y        Out     0.000     0.000       -         
MSS_ACE_0_TM0_Y                          Net         -        -       0.225     -           1         
Voltage_Monitor_MSS_0.MSS_ADLIB_INST     MSS_APB     TM0      In      -         0.225       -         
======================================================================================================



##### END OF TIMING REPORT #####]

