# Actel Physical design constraints file
# Generated file

# Version: 10.0 10.0.9.37
# Family: SmartFusion , Die: A2F200M3F , Package: 484 FBGA
# Date generated: Mon Nov 21 17:22:06 2011 


# 
# IO banks setting
# 


# 
# I/O constraints
# 

set_io MSS_RESET_N    \
    -pinname R1       \
    -fixed yes        \
    -DIRECTION Input


set_io TM0_Voltage    \
    -pinname W8       \
    -fixed yes        \
    -DIRECTION Input


set_io UART_0_RXD     \
    -pinname U18      \
    -fixed yes        \
    -DIRECTION Input


set_io UART_0_TXD      \
    -pinname Y22       \
    -fixed yes         \
    -DIRECTION Output


set_io VAREF0         \
    -pinname U10      \
    -fixed yes        \
    -DIRECTION Input



#
# Non IO constraints
#


#
# Old IO constraints, commented out for reference
#

