Resource Usage Report for MDDR_TA_top 

Mapping to part: m2gl010tfbga484-1
Cell usage:
CCC             1 use
CLKINT          8 uses
MSS_010         1 use
RCOSC_25_50MHZ  1 use
RCOSC_25_50MHZ_FAB  1 use
SYSRESET        1 use
CFG1           27 uses
CFG2           367 uses
CFG3           271 uses
CFG4           642 uses

Carry primitives used for arithmetic functions:
ARI1           317 uses


Sequential Cells: 
SLE            956 uses

DSP Blocks:    0

I/O ports: 53
I/O primitives: 51
BIBUF          20 uses
INBUF          2 uses
OUTBUF         28 uses
OUTBUF_DIFF    1 use


Global Clock Buffers: 8


Total LUTs:    1624

