*****************************************************************
Pin Report - Date: Thu Mar 03 15:27:51 2016 Pinchecksum: NOT-AVAILABLE
Product: Designer
Release: v11.7
Version: 11.7.0.119
Design Name: ddc
Family: IGLOO2
Die: M2GL050T
Package: 896 FBGA
*****************************************************************

Port        |Pin  |Fixed |Function                                   |Bank     |I/O Std   |Direction                      |I/O state in Flash*Freeze mode |Resistor Pull                      |I/O available in Flash*Freeze mode |Schmitt Trigger |Odt_Static    |Odt Imp (Ohm)  |Low Power Exit |Input Delay |Slew         |Pre-Emphasis      |Output Drive (mA) |Output Load (pF) |
------------|-----|------|-------------------------------------------|---------|----------|-------------------------------|-------------------------------|-----------------------------------|-----------------------------------|----------------|--------------|---------------|---------------|------------|-------------|------------------|------------------|-----------------|
ADC[0]       AG12  No     DDRIO154PB5/FDDR_DQ2                        Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
ADC[1]       A11   No     DDRIO88PB0/MDDR_DQ_ECC3                     Bank0     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
ADC[2]       AJ10  No     DDRIO149NB5/FDDR_DQS_ECC_N                  Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
ADC[3]       AJ12  No     DDRIO153NB5/FDDR_DQ1                        Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
ADC[4]       AD12  No     DDRIO150PB5/FDDR_TMATCH_ECC_IN              Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
ADC[5]       AK10  No     DDRIO149PB5/FDDR_DQS_ECC                    Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
ADC[6]       AG10  No     DDRIO150NB5/FDDR_DM_RDQS_ECC                Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
ADC[7]       E11   No     DDRIO87PB0/CCC_NW1_CLKI3/MDDR_DQ_ECC1       Bank0     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
ADC[8]       AK12  No     DDRIO153PB5/FDDR_DQ0                        Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
ADC[9]       AF12  No     DDRIO154NB5/FDDR_DQ3                        Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
clk          AG11  No     DDRIO152NB5/GB7/CCC_SW1_CLKI2/FDDR_DQ_ECC0  Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
clkDiv64     P3    No     MSIO114PB8/GB6/CCC_NW1_CLKI1                Bank8     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
clkDiv128    A9    No     DDRIO91PB0/GB0/CCC_NW0_CLKI3                Bank0     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[0]      AF18  No     DDRIO166NB5/FDDR_DQ19                       Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[1]      P30   No     MSIO25PB2                                   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[2]      AJ16  No     DDRIO161NB5/FDDR_DQS1_N                     Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[3]      L29   No     MSIO33NB2                                   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[4]      AF20  No     DDRIO169NB5/FDDR_DQ22                       Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[5]      AK14  No     DDRIO156NB5/FDDR_DQ4                        Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[6]      T27   No     MSIO21NB3                                   Bank3     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[7]      AG14  No     DDRIO157PB5/FDDR_DQ5                        Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[8]      R29   No     MSIO23NB3                                   Bank3     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[9]      U25   No     MSIO19PB3                                   Bank3     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[10]     AK15  No     DDRIO159PB5/CCC_SW1_CLKI3/FDDR_DQ8          Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[11]     P25   No     MSIO28PB2                                   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[12]     AF15  No     DDRIO160NB5/FDDR_DQ11                       Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[13]     N24   No     MSIO36PB2                                   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[14]     N25   No     MSIO35PB2                                   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[15]     AJ21  No     DDRIO171NB5/FDDR_DQ25                       Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[16]     AJ13  No     DDRIO155NB5/FDDR_DQS0_N                     Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[17]     AK22  No     DDRIO173NB5/FDDR_DQS3_N                     Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[18]     N28   No     MSIO29PB2                                   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[19]     AF14  No     DDRIO157NB5/FDDR_DQ6                        Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[20]     P29   No     MSIO25NB2                                   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[21]     P24   No     MSIO31PB2                                   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[22]     M30   No     MSIO29NB2                                   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[23]     AK17  No     DDRIO163PB5/GB15/VCCC_SE1_CLKI/FDDR_DQ12    Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[24]     D9    No     DDRIO92NB0/CCC_NW0_CLKI2                    Bank0     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[25]     P23   No     MSIO32PB2                                   Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[26]     AJ19  No     DDRIO167NB5/FDDR_DQS2_N                     Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[27]     AK16  No     DDRIO161PB5/GB11/VCCC_SE0_CLKI/FDDR_DQS1    Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[28]     AJ17  No     DDRIO163NB5/FDDR_DQ13                       Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[29]     AJ14  No     DDRIO158PB5/FDDR_DQ7                        Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[30]     AJ23  No     DDRIO175NB5/FDDR_DQ29                       Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
Freq[31]     AF11  No     DDRIO152PB5/GB3/CCC_SW0_CLKI3/FDDR_DQ_ECC1  Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
GlobalReset  AF17  No     DDRIO164PB5/VCCC_SE1_CLKI/FDDR_DQ14         Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
I_out[0]     AA3   No     MSIOD129NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[1]     V4    No     MSIOD126PB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[2]     T6    No     MSIOD128PB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[3]     V2    No     MSIOD127NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[4]     U8    No     MSIOD125PB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[5]     W4    No     MSIOD132NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[6]     T5    No     MSIOD125NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[7]     V5    No     MSIOD130PB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[8]     V6    No     MSIOD129PB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[9]     W5    No     MSIOD130NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[10]    V1    No     MSIOD127PB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[11]    U9    No     MSIOD132PB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[12]    W1    No     MSIOD128NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
I_out[13]    V3    No     MSIOD126NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[0]     T1    No     MSIOD120NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[1]     R2    No     MSIOD119NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[2]     U3    No     MSIOD123NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[3]     R8    No     MSIO113PB8                                  Bank8     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[4]     T7    No     MSIOD120PB7/CCC_SW1_CLKI0                   Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[5]     R5    No     MSIO116NB8                                  Bank8     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[6]     U1    No     MSIOD122NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[7]     T8    No     MSIOD124PB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[8]     R9    No     MSIO117PB8/CCC_NW0_CLKI0                    Bank8     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[9]     T4    No     MSIOD121NB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[10]    U4    No     MSIOD123PB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[11]    R1    No     MSIOD119PB7/GB1/CCC_SW0_CLKI1               Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[12]    U7    No     MSIOD121PB7/CCC_SW0_CLKI0                   Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
Q_out[13]    U2    No     MSIOD122PB7                                 Bank7     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
