# Power Report for design top with the following settings:

Vendor: | Microsemi Corporation
Program: | Microsemi Libero Software, Release v2021.1 (Version 2021.1.0.17)
| Copyright (C) 1989-
Date: | Thu Jun 3 13:18:51 2021
Version: | 3.0

Design: | top
Family: | SmartFusion2
Die: | M2S090TS
Package: | 484 FBGA
Temperature Range: | COM
Voltage Range: | COM
Operating Conditions: | Typical
Operating Mode: | Active
Process: | Typical
Data Source: | Production

## Power Summary

| Power (mW) | Percentage
--- | --- | ---
Total Power | 116.654 | 100.0%
Static Power | 19.970 | 17.1%
Dynamic Power | 96.684 | 82.9%

## Breakdown by Rail

| Power (mW) | Voltage (V) | Current (mA)
--- | --- | --- | ---
Rail VDD | 88.166 | 1.200 | 73.472
Rail CCC_NW1_PLL_VDDA | 9.000 | 3.300 | 2.727
Rail VDDI 2.5 | 1.163 | 2.500 | 0.465
Rail MDDR_PLL_VDDA | 5.000 | 3.300 | 1.515
Rail VPP | 13.325 | 3.300 | 4.038

## Breakdown by Clock

| Power (mW) | Percentage
--- | --- | ---
ENVM_INIT_M3_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (clocks) | 65.949 | 99.1%
ENVM_INIT_M3_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (register outputs) | 0.000 | 0.0%
ENVM_INIT_M3_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (primary inputs) | 0.000 | 0.0%
ENVM_INIT_M3_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (combinational outputs) | 0.559 | 0.8%
ENVM_INIT_M3_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (set/reset nets) | 0.000 | 0.0%
ENVM_INIT_M3_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (clocks) | 0.000 | 0.0%
ENVM_INIT_M3_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (register outputs) | 0.011 | 0.0%
ENVM_INIT_M3_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (primary inputs) | 0.000 | 0.0%
ENVM_INIT_M3_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (combinational outputs) | 0.000 | 0.0%
ENVM_INIT_M3_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (set/reset nets) | 0.000 | 0.0%
Input to Output | 0.000 | 0.0%

## Breakdown by Type

| Power (mW) | Percentage
--- | --- | ---
Type Net | 0.214 | 0.2%
Type Gate | 9.215 | 7.9%
Type I/O | 0.559 | 0.5%
Type Core Static | 18.535 | 15.9%
Type Banks Static | 0.611 | 0.5%
Type VPP Static | 0.825 | 0.7%
Type Built-in Blocks | 86.697 | 74.3%