*****************************************************************
Pin Report - Date: Mon Feb 22 14:59:52 2016 Pinchecksum: NOT-AVAILABLE
Product: Designer
Release: v11.7
Version: 11.7.0.119
Design Name: Disp
Family: SmartFusion2
Die: M2S090T
Package: 484 FBGA
*****************************************************************

Port                  |Pin  |Fixed |Function                                               |Bank     |I/O Std   |Direction                      |I/O state in Flash*Freeze mode |Resistor Pull                      |I/O available in Flash*Freeze mode |Schmitt Trigger |Odt_Static    |Odt Imp (Ohm)  |Low Power Exit |Input Delay |Slew         |Pre-Emphasis      |Output Drive (mA) |Output Load (pF) |
----------------------|-----|------|-------------------------------------------------------|---------|----------|-------------------------------|-------------------------------|-----------------------------------|-----------------------------------|----------------|--------------|---------------|---------------|------------|-------------|------------------|------------------|-----------------|
DEVRST_N               R15   Fixed  DEVRST_N                                                ---       
I2C_0_SCL              G16   Yes    MSIO61NB2/I2C_0_SCL/GPIO_31_B/USB_DATA1_C               Bank2     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
I2C_0_SDA              G17   Yes    MSIO61PB2/I2C_0_SDA/GPIO_30_B/USB_DATA0_C               Bank2     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
I2C_1_SCL              R22   Yes    MSIO11NB3/CCC_NE1_CLKI0/I2C_1_SCL/GPIO_1_A/USB_DATA4_A  Bank3     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
I2C_1_SDA              P22   Yes    MSIO11PB3/CCC_NE0_CLKI0/I2C_1_SDA/GPIO_0_A/USB_DATA3_A  Bank3     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
MDDR_ADDR[0]           B17   Yes    DDRIO70NB1/MDDR_ADDR0                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[1]           D16   Yes    DDRIO69PB1/MDDR_ADDR1                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[2]           E16   Yes    DDRIO69NB1/MDDR_ADDR2                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[3]           C17   Yes    DDRIO68PB1/MDDR_ADDR3                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[4]           C18   Yes    DDRIO68NB1/MDDR_ADDR4                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[5]           B19   Yes    DDRIO67PB1/MDDR_ADDR5                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[6]           A20   Yes    DDRIO67NB1/MDDR_ADDR6                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[7]           C19   Yes    DDRIO66NB1/MDDR_ADDR7                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[8]           E17   Yes    DDRIO65PB1/MDDR_ADDR8                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[9]           F17   Yes    DDRIO65NB1/MDDR_ADDR9                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[10]          A21   Yes    DDRIO64PB1/MDDR_ADDR10                                  Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[11]          B21   Yes    DDRIO64NB1/MDDR_ADDR11                                  Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[12]          E19   Yes    DDRIO63PB1/MDDR_ADDR12                                  Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[13]          D20   Yes    DDRIO63NB1/MDDR_ADDR13                                  Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[14]          D18   Yes    DDRIO62PB1/MDDR_ADDR14                                  Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ADDR[15]          E18   Yes    DDRIO62NB1/MDDR_ADDR15                                  Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_BA[0]             A18   Yes    DDRIO71PB1/MDDR_BA0                                     Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_BA[1]             A19   Yes    DDRIO71NB1/MDDR_BA1                                     Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_BA[2]             C16   Yes    DDRIO70PB1/MDDR_BA2                                     Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_CAS_N             F15   Yes    DDRIO73NB1/MDDR_CAS_N                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_CKE               B15   Yes    DDRIO74PB1/MDDR_CKE                                     Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_CLK               A16   Yes    DDRIO72PB1/MDDR_CLK                                     Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_CLK_N             A17   Yes    DDRIO72NB1/MDDR_CLK_N                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_CS_N              C15   Yes    DDRIO74NB1/MDDR_CS_N                                    Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_DM_RDQS[0]        A10   Yes    DDRIO84PB1/MDDR_DM_RDQS0                                Bank1     LPDDRI     Inout                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                5                 
MDDR_DQ[0]             B9    Yes    DDRIO87PB1/MDDR_DQ0                                     Bank1     LPDDRI     Inout                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                5                 
MDDR_DQ[1]             A9    Yes    DDRIO87NB1/MDDR_DQ1                                     Bank1     LPDDRI     Inout                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                5                 
MDDR_DQ[2]             F10   Yes    DDRIO86PB1/MDDR_DQ2                                     Bank1     LPDDRI     Inout                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                5                 
MDDR_DQ[3]             E10   Yes    DDRIO86NB1/MDDR_DQ3                                     Bank1     LPDDRI     Inout                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                5                 
MDDR_DQ[4]             A11   Yes    DDRIO84NB1/MDDR_DQ4                                     Bank1     LPDDRI     Inout                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                5                 
MDDR_DQ[5]             D10   Yes    DDRIO83PB1/MDDR_DQ5                                     Bank1     LPDDRI     Inout                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                5                 
MDDR_DQ[6]             D11   Yes    DDRIO83NB1/MDDR_DQ6                                     Bank1     LPDDRI     Inout                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                5                 
MDDR_DQ[7]             E12   Yes    DDRIO82PB1/MDDR_DQ7                                     Bank1     LPDDRI     Inout                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                5                 
MDDR_DQS[0]            B11   Yes    DDRIO85PB1/MDDR_DQS0                                    Bank1     LPDDRI     Inout                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                5                 
MDDR_DQS_TMATCH_0_IN   G12   Yes    DDRIO78PB1/MDDR_TMATCH_0_IN                             Bank1     LPDDRI     Input                           TRISTATE                        None                                ---                                 ---              Off            50              Off             Off          ---           ---                ---                ---               
MDDR_DQS_TMATCH_0_OUT  F12   Yes    DDRIO82NB1/MDDR_TMATCH_0_OUT                            Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_ODT               C20   Yes    DDRIO66PB1/MDDR_ODT                                     Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_RAS_N             F14   Yes    DDRIO75PB1/MDDR_RAS_N                                   Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_RESET_N           E15   Yes    DDRIO73PB1/MDDR_RESET_N                                 Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MDDR_WE_N              G14   Yes    DDRIO75NB1/MDDR_WE_N                                    Bank1     LPDDRI     Output                          TRISTATE                        None                                ---                                 ---              ---            ---             ---             ---          ---           ---                ---                5                 
MMUART_1_RXD           G18   Yes    MSIO55NB2/MMUART_1_RXD/GPIO_26_B/USB_DATA3_C            Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
MMUART_1_TXD           H19   Yes    MSIO54NB2/MMUART_1_TXD/GPIO_24_B/USB_DATA2_C            Bank2     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
SPI_0_CLK              N19   Yes    MSIO12PB3/SPI_0_CLK/USB_XCLK_A                          Bank3     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
SPI_0_DI               N20   Yes    MSIO12NB3/SPI_0_SDI/GPIO_5_A/USB_DIR_A                  Bank3     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
SPI_0_DO               N21   Yes    MSIO13PB3/SPI_0_SDO/GPIO_6_A/USB_STP_A                  Bank3     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
SPI_0_SS0              N22   Yes    MSIO13NB3/SPI_0_SS0/GPIO_7_A/USB_NXT_A                  Bank3     LVCMOS25   Inout                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          SLOW          ---                4                  5                 
SPI_1_CLK_F2M          D21   No     MSI59NB2/MMUART_0_TXD/GPIO_27_B/USB_DIR_C               Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
SPI_1_CLK_M2F          AB15  Yes    MSIO213PB5/VCCC_SE1_CLKI                                Bank5     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
SPI_1_DI_F2M           AA15  Yes    MSIO213NB5                                              Bank5     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
SPI_1_DO_M2F           AA16  Yes    MSIO222PB5                                              Bank5     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
SPI_1_SS0_F2M          C22   No     MSIO60PB2/MMUART_0_RXD/GPIO_28_B/USB_STP_C              Bank2     LVCMOS25   Input                           TRISTATE                        None                                No                                  Off              ---            ---             Off             Off          ---           ---                ---                ---               
SPI_1_SS0_M2F          AB18  Yes    MSIO230PB5                                              Bank5     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
SPI_1_SS0_M2F_OE       B22   No     MSIO60NB2/MMUART_0_CLK/GPIO_29_B/USB_NXT_C              Bank2     LVCMOS25   Output                          TRISTATE                        None                                No                                  ---              ---            ---             ---             ---          SLOW          ---                4                  5                 
