# Power Report for design top with the following settings:

Vendor: | Microsemi Corporation
Program: | Microsemi Libero Software, Release v12.6 (Version 12.900.20.24)
| Copyright (C) 1989-
Date: | Tue Mar 30 11:09:48 2021
Version: | 3.0

Design: | top
Family: | SmartFusion2
Die: | M2S150TS
Package: | 1152 FC
Temperature Range: | COM
Voltage Range: | COM
Operating Conditions: | Typical
Operating Mode: | Active
Process: | Typical
Data Source: | Production

## Power Summary

| Power (mW) | Percentage
--- | --- | ---
Total Power | 161.804 | 100.0%
Static Power | 34.950 | 21.6%
Dynamic Power | 126.854 | 78.4%

## Breakdown by Rail

| Power (mW) | Voltage (V) | Current (mA)
--- | --- | --- | ---
Rail VDD | 127.812 | 1.200 | 106.510
Rail VDDI 2.5 | 6.667 | 2.500 | 2.667
Rail CCC_NW1_PLL_VDDA | 9.000 | 3.300 | 2.727
Rail MDDR_PLL_VDDA | 5.000 | 3.300 | 1.515
Rail VPP | 13.325 | 3.300 | 4.038

## Breakdown by Clock

| Power (mW) | Percentage
--- | --- | ---
SmartFusion2_FIC_Tutorial_sb_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (clocks) | 88.489 | 91.5%
SmartFusion2_FIC_Tutorial_sb_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (register outputs) | 1.014 | 1.0%
SmartFusion2_FIC_Tutorial_sb_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (primary inputs) | 0.000 | 0.0%
SmartFusion2_FIC_Tutorial_sb_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (combinational outputs) | 7.170 | 7.4%
SmartFusion2_FIC_Tutorial_sb_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (set/reset nets) | 0.000 | 0.0%
SmartFusion2_FIC_Tutorial_sb_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (clocks) | 0.000 | 0.0%
SmartFusion2_FIC_Tutorial_sb_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (register outputs) | 0.015 | 0.0%
SmartFusion2_FIC_Tutorial_sb_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (primary inputs) | 0.000 | 0.0%
SmartFusion2_FIC_Tutorial_sb_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (combinational outputs) | 0.000 | 0.0%
SmartFusion2_FIC_Tutorial_sb_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (set/reset nets) | 0.000 | 0.0%
Input to Output | 0.000 | 0.0%

## Breakdown by Type

| Power (mW) | Percentage
--- | --- | ---
Type Net | 2.661 | 1.6%
Type Gate | 14.642 | 9.0%
Type I/O | 5.514 | 3.4%
Type Memory | 17.341 | 10.7%
Type Core Static | 32.949 | 20.4%
Type Banks Static | 1.176 | 0.7%
Type VPP Static | 0.825 | 0.5%
Type Built-in Blocks | 86.697 | 53.6%