| BLDC control on ATAVRMC303 with ATxMega128A1

Modules
Here is a list of all modules:
[detail level 1 2 3 4]

▼ADC Module | ADC Module
▼ADC Macros | Low level macros that permit the use of the ADC of the product
Turn on the ADC | Turn on the ADC
ADC Alignement Configuration | Configure the Result alignement
ADC High Speed Mode Configuration | Set the high spped mode in case ADC frequency is higher than 200KHz
ADC Vref Configuration | Configure the Vref
ADC IT Configuration | Configure the ADC IT
ADC Prescaler Configuration | Configure the ADC prescaler
ADC Channel Selection | Select the ADC channel to be converted
▼ADC Start Conversion | Start the Analog to Digital Conversion
ADC Start Normal Conversion | Start the conversion in normal mode
ADC Start Idle Conversion | Start the Analog to Digital Conversion in noise reduction mode
ADC Get x Bits Result | ADC Get x Bits Result
Turn Off the ADC | Turn Off the ADC
conversion is finished or not | Check conversion status
ADC Low Level Fucntions | ADC Low Level Functions
▼ADC Defines Configuration Values | Defines allowing to init the ADC with the wanted configuration
▼DAC Defines Configuration Values | Defines allowing to init the DAC with the wanted configuration
COMPARATORs Defines Configuration Values | Defines allowing to init the COMPARATORs with the wanted configuration