| Xmega IEC60730 Class B Library 1.0 |

All Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
classb_wdt_test.h File Reference

## Detailed Description

Settings for the watchdog timer test.

Application note:
  AVR1610: Guide to IEC60730 Class B compliance with XMEGA

Documentation
  For comprehensive code documentation, supported compilers, compiler settings and supported devices see readme.html

Author:
  Atmel Corporation: http://www.atmel.com
  Support email: avr@a.nosp@m.tmel.nosp@m..com

Copyright (C) 2012 Atmel Corporation. All rights reserved.

Definition in file classb_wdt_test.h.

`#include "avr_compiler.h"`
`#include "classb_rtc_common.h"`
`#include "error_handler.h"`
Include dependency graph for classb_wdt_test.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
Configuration settings
#define | CLASSB_WDT_WPER WDT_WPER_500CLK_gc
| This is the closed period, where WDT cannot be reset.
#define | CLASSB_WDT_PER WDT_PER_250CLK_gc
| This is the open period, where WDT has to be reset.

## Functions
Class B Test
void | classb_wdt_test (void)
| This is the watchdog timer (WDT) self-diagnostic test.