- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

# conf_usb.h

Go to the documentation of this file.

    00001 /*This file is prepared for Doxygen automatic documentation generation.*/
    00013
    00014 /* Copyright (c) 2009 Atmel Corporation. All rights reserved.
    00015  *
    00016  * Redistribution and use in source and binary forms, with or without
    00017  * modification, are permitted provided that the following conditions are met:
    00018  *
    00019  * 1. Redistributions of source code must retain the above copyright notice,
    00020  * this list of conditions and the following disclaimer.
    00021  *
    00022  * 2. Redistributions in binary form must reproduce the above copyright notice,
    00023  * this list of conditions and the following disclaimer in the documentation
    00024  * and/or other materials provided with the distribution.
    00025  *
    00026  * 3. The name of Atmel may not be used to endorse or promote products derived
    00027  * from this software without specific prior written permission.
    00028  *
    00029  * 4. This software may only be redistributed and used in connection with an Atmel
    00030  * AVR product.
    00031  *
    00032  * THIS SOFTWARE IS PROVIDED BY ATMEL "AS IS" AND ANY EXPRESS OR IMPLIED
    00033  * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
    00034  * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NON-INFRINGEMENT ARE EXPRESSLY AND
    00035  * SPECIFICALLY DISCLAIMED. IN NO EVENT SHALL ATMEL BE LIABLE FOR ANY DIRECT,
    00036  * INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
    00037  * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
    00038  * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
    00039  * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
    00040  * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
    00041  * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
    00042  */
    00043 #ifndef _CONF_USB_H_
    00044 #define _CONF_USB_H_
    00045
    00046 #include "modules/usb/usb_commun.h"
    00047 #include "modules/usb/usb_commun_hid.h"
    00048
    00049
    00053
    00054
    00055    // _________________ USB MODE CONFIGURATION ____________________________
    00056    //
    00061
    00065       #define USB_DEVICE_FEATURE          ENABLED
    00066
    00068
    00069    // _________________ USB REGULATOR CONFIGURATION _______________________
    00070    //
    00073
    00078 #ifndef USE_USB_PADS_REGULATOR
    00079    #define USE_USB_PADS_REGULATOR   ENABLE      // Possible values ENABLE or DISABLE
    00080 #endif
    00081
    00082
    00083
    00084 // _________________ DEVICE MODE CONFIGURATION __________________________
    00085
    00089
    00090 #define USB_DEVICE_SN_USE          DISABLE            // DISABLE
    00091 #define USE_DEVICE_SN_UNIQUE       DISABLE            // ignore if USB_DEVICE_SN_USE = DISABLE
    00092
    00093 #define EP_MOUSE_IN           1  //! Number of the mouse interrupt IN endpoint
    00094
    00095 #define USB_REMOTE_WAKEUP_FEATURE    ENABLE   //! don't allow remote wake up
    00096
    00097 #define USB_LOW_SPEED_DEVICE         ENABLE
    00098
    00099 #define USB_RESET_CPU         DISABLED   //! an USB reset does not reset the CPU
    00100
    00101 #define Usb_unicode(a)         ((U16)(a))
    00102
    00106    // write here the action to associate to each USB event
    00107    // be carefull not to waste time in order not disturbing the functions
    00108 #define Usb_sof_action()         sof_action();
    00109 #define Usb_resume_action()
    00110 #define Usb_suspend_action()     suspend_action();
    00111 #define Usb_wake_up_action()
    00112 #define Usb_reset_action()
    00113 #define Usb_vbus_on_action()
    00114 #define Usb_vbus_off_action()
    00115 #define Usb_set_configuration_action()
    00116
    00117
    00118 extern void sof_action(void);
    00119 extern void suspend_action(void);
    00121
    00122
    00124
    00125 #endif // _CONF_USB_H_