Data Fields

# S_UsbRequest Struct Reference

Usb Request. More...

`#include <usb_descriptors.h>`

## Data Fields
U8 | bmRequestType
| Characteristics of the request.
U8 | bRequest
| Specific request.
U16 | wValue
| field that varies according to request
U16 | wIndex
| field that varies according to request
U16 | wLength
| Number of bytes to transfer if Data.

## Detailed Description

Usb Request.

Definition at line 164 of file usb_descriptors.h.

## Field Documentation

U8 S_UsbRequest::bmRequestType

Characteristics of the request.

Definition at line 166 of file usb_descriptors.h.

U8 S_UsbRequest::bRequest

Specific request.

Definition at line 167 of file usb_descriptors.h.

U16 S_UsbRequest::wValue

field that varies according to request

Definition at line 168 of file usb_descriptors.h.

U16 S_UsbRequest::wIndex

field that varies according to request

Definition at line 169 of file usb_descriptors.h.

U16 S_UsbRequest::wLength

Number of bytes to transfer if Data.

Definition at line 170 of file usb_descriptors.h.

The documentation for this struct was generated from the following file:

- usb_descriptors.h