Defines

# conversion is finished or not
[ADC Macros]

Check conversion status. More...

## Defines
#define | Is_adc_conv_finished() ((ADCSRA & (1<<ADIF)) ? TRUE : FALSE)
#define | Is_adc_conv_not_finished() ((ADCSRA | ~(1<<ADIF)) ? TRUE : FALSE)

## Detailed Description

Check conversion status.

## Define Documentation

#define Is_adc_conv_finished | ( | ) | ((ADCSRA & (1<<ADIF)) ? TRUE : FALSE)

Definition at line 162 of file adc_drv.h.

Referenced by get_temp_sensor_val().

#define Is_adc_conv_not_finished | ( | ) | ((ADCSRA | ~(1<<ADIF)) ? TRUE : FALSE)

Definition at line 163 of file adc_drv.h.