Functions

# timer16_drv.c File Reference

This file contains the low level functions (drivers) of 16-bit Timer(s) More...

`#include "config.h"`
`#include "timer16_drv.h"`
Include dependency graph for timer16_drv.c:

Go to the source code of this file.

## Functions
U16 | timer16_get_counter (void)
| This function READ the 16-bit TIMER counter.
U16 | timer16_get_capture (void)
| This function READ the 16-bit TIMER capture register.

## Detailed Description

This file contains the low level functions (drivers) of 16-bit Timer(s)

- Compiler: IAR EWAVR and GNU GCC for AVR
- Supported devices: ATmega32U4

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file timer16_drv.c.

## Function Documentation

U16 timer16_get_counter | ( | void | ) |

This function READ the 16-bit TIMER counter.

Warning:

Parameters:

Returns:
  16-bit counter value

Definition at line 66 of file timer16_drv.c.

    {
        U16 u16_temp;

        u16_temp  =  Timer16_get_counter_low();
        u16_temp |= (Timer16_get_counter_high() << 8 );

        return u16_temp;
    }

U16 timer16_get_capture | ( | void | ) |

This function READ the 16-bit TIMER capture register.

Warning:

Parameters:

Returns:
  16-bit capture value

Definition at line 87 of file timer16_drv.c.

    {
        U16 u16_temp;

        u16_temp  =  Timer16_get_capture_low();
        u16_temp |= (Timer16_get_capture_high() << 8 );

        return u16_temp;
    }