# chip/at32uc3a3/include/chip/spi.h File Reference

AT32UC3A3 chip-specific SPI definitions. More...

`#include <chip/memory-map.h>`
`#include <stddef.h>`

Include dependency graph for spi.h:

Go to the source code of this file.

## Functions
static void * | get_spi_regs (unsigned int id)
| Get a pointer to the SPI registers.

## Detailed Description

AT32UC3A3 chip-specific SPI definitions.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: AT32UC3A3
- AppNote:

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file spi.h.

## Function Documentation

static void* get_spi_regs | ( | unsigned int | id | ) | `[inline, static]`

Get a pointer to the SPI registers.

Parameters:

  | id | The ID of the SPI.

Returns:
  A pointer to a virtual address corresponding to the base address of the SPIid registers.

Definition at line 55 of file spi.h.