# board/atevk1104/include/board/clk.h File Reference

ATEVK1104 clock configuration. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Defines
#define | BOARD_OSC32_HZ 32768
| OSC32 rate in Hz.
#define | BOARD_OSC32_STARTUP_US 71000
| OSC32 startup time in microseconds.
#define | BOARD_OSC32_XTAL 1
| OSC32 is a crystal, not an external clock.
#define | BOARD_OSC0_HZ 12000000
| OSC0 rate in Hz.
#define | BOARD_OSC0_STARTUP_US 18000
| OSC0 startup time in microseconds.
#define | BOARD_OSC0_XTAL 1
| OSC0 is a crystal, not an external clock.
#define | BOARD_OSC1_HZ 11289600
| OSC1 rate in Hz.
#define | BOARD_OSC1_STARTUP_US 18000
| OSC1 startup time in microseconds.
#define | BOARD_OSC1_XTAL 1
| OSC1 is a crystal, not an external clock.

## Detailed Description

ATEVK1104 clock configuration.

- Compiler: IAR EWAVR32 and GNU GCC for AVR32
- Supported devices: ATEVK1104
- AppNote:

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file clk.h.

## Define Documentation

#define BOARD_OSC0_HZ 12000000

OSC0 rate in Hz.

Definition at line 52 of file clk.h.

#define BOARD_OSC0_STARTUP_US 18000

OSC0 startup time in microseconds.

Definition at line 54 of file clk.h.

Referenced by pm_init_osc().

#define BOARD_OSC0_XTAL 1

OSC0 is a crystal, not an external clock.

Definition at line 56 of file clk.h.

Referenced by pm_init_osc().

#define BOARD_OSC1_HZ 11289600

OSC1 rate in Hz.

Definition at line 59 of file clk.h.

#define BOARD_OSC1_STARTUP_US 18000

OSC1 startup time in microseconds.

Definition at line 61 of file clk.h.

Referenced by pm_init_osc().

#define BOARD_OSC1_XTAL 1

OSC1 is a crystal, not an external clock.

Definition at line 63 of file clk.h.

Referenced by pm_init_osc().

#define BOARD_OSC32_HZ 32768

OSC32 rate in Hz.

Definition at line 45 of file clk.h.

#define BOARD_OSC32_STARTUP_US 71000

OSC32 startup time in microseconds.

Definition at line 47 of file clk.h.

#define BOARD_OSC32_XTAL 1

OSC32 is a crystal, not an external clock.

Definition at line 49 of file clk.h.