# scsi_mode_param_header6 Struct Reference

SCSI Mode Parameter Header used by MODE SELECT(6) and MODE SENSE(6). More...

`#include <spc_protocol.h>`

## Data Fields
uint8_t | mode_data_length
| Number of bytes after this.
uint8_t | medium_type
| Medium Type.
uint8_t | device_specific_parameter
| Defined by command set.
uint8_t | block_descriptor_length
| Length of block descriptors.

## Detailed Description

SCSI Mode Parameter Header used by MODE SELECT(6) and MODE SENSE(6).

Definition at line 211 of file spc_protocol.h.

## Field Documentation

uint8_t scsi_mode_param_header6::block_descriptor_length

Length of block descriptors.

Definition at line 215 of file spc_protocol.h.

uint8_t scsi_mode_param_header6::device_specific_parameter

Defined by command set.

Definition at line 214 of file spc_protocol.h.

uint8_t scsi_mode_param_header6::medium_type

Medium Type.

Definition at line 213 of file spc_protocol.h.

uint8_t scsi_mode_param_header6::mode_data_length

Number of bytes after this.

Definition at line 212 of file spc_protocol.h.

The documentation for this struct was generated from the following file:

- include/scsi/spc_protocol.h