- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# Host controller states
[USB host task]

Defines for device state coding. More...

## Defines
#define | DEVICE_UNATTACHED 0
#define | DEVICE_ATTACHED 1
#define | DEVICE_POWERED 2
#define | DEVICE_DEFAULT 3
#define | DEVICE_ADDRESSED 4
#define | DEVICE_CONFIGURED 5
#define | DEVICE_READY 6
#define | DEVICE_ERROR 7
#define | DEVICE_SUSPENDED 8
#define | DEVICE_WAIT_RESUME 9
#define | DEVICE_DISCONNECTED 10
#define | DEVICE_DISCONNECTED_ACK 11
#define | Host_set_device_supported() (device_status |= 0x01)
#define | Host_clear_device_supported() (device_status &= ~0x01)
#define | Is_host_device_supported() (device_status & 0x01)
#define | Host_set_device_ready() (device_status |= 0x02)
#define | Host_clear_device_ready() (device_status &= ~0x02)
#define | Is_host_device_ready() (device_status & 0x02)
#define | Host_set_configured() (device_status |= 0x04)
#define | Host_clear_configured() (device_status &= ~0x04)
#define | Is_host_configured() (device_status & 0x04)
#define | Host_clear_device_status() (device_status = 0x00)

## Detailed Description

Defines for device state coding.

## Define Documentation

#define DEVICE_UNATTACHED 0

Definition at line 140 of file usb_host_task.h.

Referenced by usb_device_task(), usb_host_task(), and usb_host_task_init().

#define DEVICE_ATTACHED 1

Definition at line 141 of file usb_host_task.h.

Referenced by usb_host_task().

#define DEVICE_POWERED 2

Definition at line 142 of file usb_host_task.h.

Referenced by usb_host_task().

#define DEVICE_DEFAULT 3

Definition at line 143 of file usb_host_task.h.

Referenced by usb_host_task().

#define DEVICE_ADDRESSED 4

Definition at line 144 of file usb_host_task.h.

Referenced by usb_host_task().

#define DEVICE_CONFIGURED 5

Definition at line 145 of file usb_host_task.h.

Referenced by usb_host_task().

#define DEVICE_READY 6

Definition at line 146 of file usb_host_task.h.

Referenced by usb_host_task().

#define DEVICE_ERROR 7

Definition at line 148 of file usb_host_task.h.

Referenced by usb_host_task().

#define DEVICE_SUSPENDED 8

Definition at line 150 of file usb_host_task.h.

Referenced by usb_host_task().

#define DEVICE_WAIT_RESUME 9

Definition at line 151 of file usb_host_task.h.

Referenced by usb_host_task().

#define DEVICE_DISCONNECTED 10

Definition at line 153 of file usb_host_task.h.

Referenced by usb_general_interrupt(), and usb_host_task().

#define DEVICE_DISCONNECTED_ACK 11

Definition at line 154 of file usb_host_task.h.

Referenced by usb_host_task().

#define Host_set_device_supported | ( |  | ) | (device_status |= 0x01)

Definition at line 156 of file usb_host_task.h.

Referenced by enumerate_hub_port_device(), and usb_host_task().

#define Host_clear_device_supported | ( |  | ) | (device_status &= ~0x01)

Definition at line 157 of file usb_host_task.h.

Referenced by usb_host_task().

#define Is_host_device_supported | ( |  | ) | (device_status & 0x01)

Definition at line 158 of file usb_host_task.h.

#define Host_set_device_ready | ( |  | ) | (device_status |= 0x02)

Definition at line 160 of file usb_host_task.h.

Referenced by usb_host_task().

#define Host_clear_device_ready | ( |  | ) | (device_status &= ~0x02)

Definition at line 161 of file usb_host_task.h.

Referenced by usb_host_task().

#define Is_host_device_ready | ( |  | ) | (device_status & 0x02)

Definition at line 162 of file usb_host_task.h.

#define Host_set_configured | ( |  | ) | (device_status |= 0x04)

Definition at line 164 of file usb_host_task.h.

Referenced by host_auto_configure_endpoint(), and usb_host_task().

#define Host_clear_configured | ( |  | ) | (device_status &= ~0x04)

Definition at line 165 of file usb_host_task.h.

Referenced by usb_host_task().

#define Is_host_configured | ( |  | ) | (device_status & 0x04)

Definition at line 166 of file usb_host_task.h.

#define Host_clear_device_status | ( |  | ) | (device_status = 0x00)

Definition at line 168 of file usb_host_task.h.