- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# config.h

Go to the documentation of this file.

    00001 /*This file has been prepared for Doxygen automatic documentation generation.*/
    00013
    00014 /* Copyright (c) 2007, Atmel Corporation All rights reserved.
    00015  *
    00016  * Redistribution and use in source and binary forms, with or without
    00017  * modification, are permitted provided that the following conditions are met:
    00018  *
    00019  * 1. Redistributions of source code must retain the above copyright notice,
    00020  * this list of conditions and the following disclaimer.
    00021  *
    00022  * 2. Redistributions in binary form must reproduce the above copyright notice,
    00023  * this list of conditions and the following disclaimer in the documentation
    00024  * and/or other materials provided with the distribution.
    00025  *
    00026  * 3. The name of ATMEL may not be used to endorse or promote products derived
    00027  * from this software without specific prior written permission.
    00028  *
    00029  * THIS SOFTWARE IS PROVIDED BY ATMEL ``AS IS'' AND ANY EXPRESS OR IMPLIED
    00030  * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
    00031  * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NON-INFRINGEMENT ARE EXPRESSLY AND
    00032  * SPECIFICALLY DISCLAIMED. IN NO EVENT SHALL ATMEL BE LIABLE FOR ANY DIRECT,
    00033  * INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
    00034  * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
    00035  * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
    00036  * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
    00037  * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
    00038  * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
    00039  */
    00040
    00041 #ifndef _CONFIG_H_
    00042 #define _CONFIG_H_
    00043
    00044 // Compiler switch (do not change these settings)
    00045 #include "lib_mcu/compiler.h"             // Compiler definitions
    00046 #ifdef __GNUC__
    00047    #include <avr/io.h>                    // Use AVR-GCC library
    00048 #elif __ICCAVR__
    00049    #define ENABLE_BIT_DEFINITIONS
    00050    #include <ioavr.h>                     // Use IAR-AVR library
    00051 #else
    00052    #error Current COMPILER not supported
    00053 #endif
    00054
    00055
    00058
    00059 #include "conf/conf_scheduler.h"          // Scheduler tasks declaration
    00060
    00062 #define  STK525   1                       // do not change these settings
    00063 #define  TARGET_BOARD STK525
    00064 #include "lib_board\stk_525\stk_525.h"
    00065
    00067 #undef USE_ADC
    00068
    00070 #define FOSC 8000
    00071
    00072 #define USE_TIMER16 TIMER16_1
    00073
    00074 // -------- END Generic Configuration -------------------------------------
    00075
    00076 #define HOST_SYNC_MODE     ENABLE
    00077 #ifdef __ICCAVR__
    00078 #  define HOST_UPGRADE_MODE  ENABLE
    00079 #else
    00080 #  define HOST_UPGRADE_MODE  DISABLE
    00081 #endif
    00082
    00083 // UART Sample configuration, if we have one ... __________________________
    00084 #define BAUDRATE        57600
    00085 #define USE_UART2
    00086 #define UART_U2
    00087
    00088 #ifndef __GNUC__
    00089 #define uart_putchar putchar
    00090 #endif
    00091
    00092 #define r_uart_ptchar int
    00093 #define p_uart_ptchar int
    00094
    00095
    00096 #define SBC_VENDOR_ID         {'A','T','M','E','L',' ',' ',' '}      // 8 Bytes only
    00097 #define SBC_PRODUCT_ID        {'A','T','9','0','U','S','B','1','2','8',' ','M',' ','S',' ',' '}  // 16 Bytes only
    00098 #define SBC_REVISION_ID       {'0','.','0','0'}  // 4 Bytes only
    00099
    00100
    00101 // Nav_util.c configuration
    00102 #define MAX_FILE_LENGHT       30
    00103
    00104 // USHELL configuration, if we have one ... ___________________________
    00105
    00106 #define USHELL_DFU            DISABLE
    00107 #define USHELL_USB            ENABLE
    00108 #define USHELL_HID            DISABLE
    00109 #define USHELL_HISTORY        1
    00110
    00111 #define USHELL_NB_LINE        20
    00112 #define USHELL_NB_COL         80
    00113
    00114 #define TRACE                 DISABLE
    00115
    00116 #if (TRACE==ENABLE)
    00117 extern void ushell_trace_msg(U8 code *str);
    00118 #define LOG_STR_CODE(s)    ushell_trace_msg(s)
    00119 #endif
    00120
    00122
    00123 #endif // _CONFIG_H_
    00124