- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# usb_descriptors.h File Reference

`#include "config.h"`
`#include "modules/usb/device_chap9/usb_standard_request.h"`
`#include "conf_usb.h"`

Include dependency graph for usb_descriptors.h:

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | S_UsbRequest
| Usb Request. More...
struct | S_usb_device_descriptor
| Usb Device Descriptor. More...
struct | S_usb_configuration_descriptor
| Usb Configuration Descriptor. More...
struct | S_usb_interface_descriptor
| Usb Interface Descriptor. More...
struct | S_usb_endpoint_descriptor
| Usb Endpoint Descriptor. More...
struct | S_usb_language_id
| Usb Language Descriptor. More...
struct | S_usb_manufacturer_string_descriptor
struct | S_usb_product_string_descriptor
struct | S_usb_serial_number
struct | S_usb_user_configuration_descriptor
## Defines
#define | Usb_get_dev_desc_pointer() (&(usb_dev_desc.bLength))
#define | Usb_get_dev_desc_length() (sizeof (usb_dev_desc))
#define | Usb_get_conf_desc_pointer() (&(usb_conf_desc.cfg_mouse.bLength))
#define | Usb_get_conf_desc_length() (sizeof (usb_conf_desc))
#define | USB_SPECIFICATION 0x0200
#define | DEVICE_CLASS 0
#define | DEVICE_SUB_CLASS 0
#define | DEVICE_PROTOCOL 0
#define | EP_CONTROL_LENGTH 64
#define | VENDOR_ID VID_ATMEL
#define | PRODUCT_ID PID_AT90USB128_64_MS
#define | RELEASE_NUMBER 0x1000
#define | MAN_INDEX 0x01
#define | PROD_INDEX 0x02
#define | SN_INDEX 0x03
#define | NB_CONFIGURATION 1
#define | NB_INTERFACE 1
#define | CONF_NB 1
#define | CONF_INDEX 0
#define | CONF_ATTRIBUTES USB_CONFIG_BUSPOWERED
#define | MAX_POWER 50
#define | INTERFACE_NB 0
#define | ALTERNATE 0
#define | NB_ENDPOINT 2
#define | INTERFACE_CLASS MS_CLASS
#define | INTERFACE_SUB_CLASS MS_SUB_CLASS6
#define | INTERFACE_PROTOCOL MS_PROTOCOL
#define | INTERFACE_INDEX 0
#define | ENDPOINT_NB_2 (EP_MS_IN | USB_ENDPOINT_IN)
#define | EP_ATTRIBUTES_2 0x02
#define | EP_IN_LENGTH 64
#define | EP_SIZE_2 EP_IN_LENGTH
#define | EP_INTERVAL_2 0x00
#define | ENDPOINT_NB_3 EP_MS_OUT
#define | EP_ATTRIBUTES_3 0x02
#define | EP_IN_LENGTH 64
#define | EP_SIZE_3 EP_IN_LENGTH
#define | EP_INTERVAL_3 0x00
#define | DEVICE_STATUS USB_DEVICE_STATUS_BUS_POWERED
#define | LANG_ID 0x00
#define | USB_MN_LENGTH 5
#define | USB_MANUFACTURER_NAME
#define | USB_PN_LENGTH 22
#define | USB_PRODUCT_NAME
#define | USB_SN_LENGTH 0x0D
#define | USB_SERIAL_NUMBER
#define | LANGUAGE_ID 0x0409

## Detailed Description

USB Identifers.

This file contains the usb parameters that uniquely identify the application through descriptor tables.

- Compiler: IAR EWAVR and GNU GCC for AVR
- Supported devices: AT90USB1287, AT90USB1286, AT90USB647, AT90USB646

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file usb_descriptors.h.

## Define Documentation

#define Usb_get_dev_desc_pointer | ( |  | ) | (&(usb_dev_desc.bLength))

Definition at line 55 of file usb_descriptors.h.

Referenced by usb_get_descriptor().

#define Usb_get_dev_desc_length | ( |  | ) | (sizeof (usb_dev_desc))

Definition at line 56 of file usb_descriptors.h.

Referenced by usb_get_descriptor().

#define Usb_get_conf_desc_pointer | ( |  | ) | (&(usb_conf_desc.cfg_mouse.bLength))

Definition at line 57 of file usb_descriptors.h.

Referenced by usb_get_descriptor().

#define Usb_get_conf_desc_length | ( |  | ) | (sizeof (usb_conf_desc))

Definition at line 58 of file usb_descriptors.h.

Referenced by usb_get_descriptor().

#define USB_SPECIFICATION 0x0200

Definition at line 63 of file usb_descriptors.h.

#define DEVICE_CLASS 0

Definition at line 64 of file usb_descriptors.h.

#define DEVICE_SUB_CLASS 0

Definition at line 65 of file usb_descriptors.h.

#define DEVICE_PROTOCOL 0

Definition at line 66 of file usb_descriptors.h.

#define EP_CONTROL_LENGTH 64

Definition at line 67 of file usb_descriptors.h.

Referenced by usb_get_descriptor().

#define VENDOR_ID VID_ATMEL

Definition at line 68 of file usb_descriptors.h.

#define PRODUCT_ID PID_AT90USB128_64_MS

Definition at line 69 of file usb_descriptors.h.

#define RELEASE_NUMBER 0x1000

Definition at line 70 of file usb_descriptors.h.

#define MAN_INDEX 0x01

Definition at line 71 of file usb_descriptors.h.

Referenced by usb_user_get_descriptor().

#define PROD_INDEX 0x02

Definition at line 72 of file usb_descriptors.h.

Referenced by usb_user_get_descriptor().

#define SN_INDEX 0x03

Definition at line 74 of file usb_descriptors.h.

Referenced by usb_user_get_descriptor().

#define NB_CONFIGURATION 1

Definition at line 78 of file usb_descriptors.h.

Referenced by usb_set_configuration().

#define NB_INTERFACE 1

Definition at line 81 of file usb_descriptors.h.

#define CONF_NB 1

Definition at line 82 of file usb_descriptors.h.

#define CONF_INDEX 0

Definition at line 83 of file usb_descriptors.h.

#define CONF_ATTRIBUTES USB_CONFIG_BUSPOWERED

Definition at line 84 of file usb_descriptors.h.

#define MAX_POWER 50

Definition at line 85 of file usb_descriptors.h.

#define INTERFACE_NB 0

Definition at line 88 of file usb_descriptors.h.

Referenced by usb_user_interface_reset(), and usb_user_read_request().

#define ALTERNATE 0

Definition at line 89 of file usb_descriptors.h.

#define NB_ENDPOINT 2

Definition at line 90 of file usb_descriptors.h.

#define INTERFACE_CLASS MS_CLASS

Definition at line 91 of file usb_descriptors.h.

#define INTERFACE_SUB_CLASS MS_SUB_CLASS6

Definition at line 92 of file usb_descriptors.h.

#define INTERFACE_PROTOCOL MS_PROTOCOL

Definition at line 93 of file usb_descriptors.h.

#define INTERFACE_INDEX 0

Definition at line 94 of file usb_descriptors.h.

#define ENDPOINT_NB_2 (EP_MS_IN | USB_ENDPOINT_IN)

Definition at line 97 of file usb_descriptors.h.

#define EP_ATTRIBUTES_2 0x02

Definition at line 98 of file usb_descriptors.h.

#define EP_IN_LENGTH 64

Definition at line 107 of file usb_descriptors.h.

#define EP_SIZE_2 EP_IN_LENGTH

Definition at line 100 of file usb_descriptors.h.

#define EP_INTERVAL_2 0x00

Definition at line 101 of file usb_descriptors.h.

#define ENDPOINT_NB_3 EP_MS_OUT

Definition at line 105 of file usb_descriptors.h.

#define EP_ATTRIBUTES_3 0x02

Definition at line 106 of file usb_descriptors.h.

#define EP_IN_LENGTH 64

Definition at line 107 of file usb_descriptors.h.

#define EP_SIZE_3 EP_IN_LENGTH

Definition at line 108 of file usb_descriptors.h.

#define EP_INTERVAL_3 0x00

Definition at line 109 of file usb_descriptors.h.

#define DEVICE_STATUS USB_DEVICE_STATUS_BUS_POWERED

Definition at line 111 of file usb_descriptors.h.

#define LANG_ID 0x00

Definition at line 113 of file usb_descriptors.h.

Referenced by usb_user_get_descriptor().

#define USB_MN_LENGTH 5

Definition at line 119 of file usb_descriptors.h.

#define USB_MANUFACTURER_NAME

Value:

    { Usb_unicode('A') \
    , Usb_unicode('T') \
    , Usb_unicode('M') \
    , Usb_unicode('E') \
    , Usb_unicode('L') \
    }

Definition at line 120 of file usb_descriptors.h.

#define USB_PN_LENGTH 22

Definition at line 128 of file usb_descriptors.h.

#define USB_PRODUCT_NAME

Value:

    { Usb_unicode('A') \
     ,Usb_unicode('V') \
     ,Usb_unicode('R') \
     ,Usb_unicode(' ') \
     ,Usb_unicode('U') \
     ,Usb_unicode('S') \
     ,Usb_unicode('B') \
     ,Usb_unicode(' ') \
     ,Usb_unicode('M') \
     ,Usb_unicode('S') \
     ,Usb_unicode(' ') \
     ,Usb_unicode('F') \
     ,Usb_unicode('I') \
     ,Usb_unicode('L') \
     ,Usb_unicode('E') \
     ,Usb_unicode(' ') \
     ,Usb_unicode('S') \
     ,Usb_unicode('Y') \
     ,Usb_unicode('S') \
     ,Usb_unicode('T') \
     ,Usb_unicode('E') \
     ,Usb_unicode('M') \
    }

Definition at line 129 of file usb_descriptors.h.

#define USB_SN_LENGTH 0x0D

Definition at line 154 of file usb_descriptors.h.

#define USB_SERIAL_NUMBER

Value:

    { Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
     ,Usb_unicode('0') \
    }

Definition at line 156 of file usb_descriptors.h.

#define LANGUAGE_ID 0x0409

Definition at line 172 of file usb_descriptors.h.